<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.56" y2="0" width="0" layer="20"/>
<wire x1="35.56" y1="0" x2="35.56" y2="26.67" width="0" layer="20"/>
<wire x1="35.56" y1="26.67" x2="23.622" y2="26.67" width="0" layer="20"/>
<wire x1="23.622" y1="26.67" x2="23.622" y2="20.955" width="0" layer="20"/>
<wire x1="23.622" y1="20.955" x2="11.43" y2="20.955" width="0" layer="20"/>
<wire x1="11.43" y1="20.955" x2="11.43" y2="26.67" width="0" layer="20"/>
<wire x1="11.43" y1="26.67" x2="0" y2="26.67" width="0" layer="20"/>
<wire x1="0" y1="26.67" x2="0" y2="0" width="0" layer="20"/>
<text>Antenna trace 12mils (50Ohms impedance)</text>
<text>1 oz copper</text>
<text>6.7 mil prepreg</text>
<text>0.5 oz copper</text>
<text>47 mil core</text>
<text>0.5 oz copper</text>
<text>6.7 mil prepreg</text>
<text>1 oz copper</text>
<text>er is 3.66</text>
<text>Stackup:</text>
<text>OpenMV</text>
<text>AMS00X</text>
<text>DAC</text>
<text>TXD</text>
<text>RXD</text>
<text>SEL</text>
<text>SCK</text>
<text>MISO</text>
<text>SWD</text>
<text>SWC</text>
<text>BOOT</text>
<text>RST</text>
<text>GND</text>
<text>3v3</text>
<text>VCC</text>
<text>PWM2</text>
<text>MOSI</text>
<text>PWM1</text>
<text>OSHW</text>
</plain>
<libraries>
<library name="sfe">
<packages>
<package name="0603-CAP">
</package>
<package name="LED-0603">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="openmv">
<packages>
<package name="OPENMV3">
</package>
<package name="OPENMV-LOGO">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP12R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
<library name="iofault">
<packages>
<package name="OSHW_6X150_NOTEXT">
</package>
</packages>
</library>
<library name="AMS">
<packages>
<package name="AMS00X">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="TP1" library="testpad" package="TP12R" value="TPTP12R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="openmv" package="OPENMV3" value="OPENMV3"/>
<element name="U$1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="C2" library="sfe" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="TP12R" value="TPTP12R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="openmv" package="OPENMV-LOGO" value="OPENMV-LOGO"/>
<element name="LOGO1" library="iofault" package="OSHW_6X150_NOTEXT" value="OSHW_LOGO_6MILX0150-NT"/>
<element name="U$3" library="AMS" package="AMS00X" value="AMS00X"/>
<element name="R1" library="sfe" package="0603-RES" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="TP12R" value="TPTP12R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="TP12R" value="TPTP12R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="TP12R" value="TPTP12R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="TP12R" value="TPTP12R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="testpad" package="TP12R" value="TPTP12R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="TP12R" value="TPTP12R">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="sfe" package="LED-0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="sfe" package="0603-RES" value="220R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="sfe" package="0603-CAP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="28"/>
<contactref element="U$3" pad="P$27"/>
<contactref element="U$3" pad="P$26"/>
<contactref element="U$3" pad="P$25"/>
<contactref element="U$3" pad="P$24"/>
<contactref element="U$3" pad="P$23"/>
<contactref element="U$3" pad="P$22"/>
<contactref element="U$3" pad="P$19"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$3" pad="P$28"/>
<contactref element="U$3" pad="P$29"/>
<contactref element="U$3" pad="P$30"/>
<contactref element="U$3" pad="P$31"/>
<contactref element="U$3" pad="P$32"/>
<contactref element="U$3" pad="P$33"/>
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$69">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="VIN">
<contactref element="U2" pad="27"/>
</signal>
<signal name="RESET">
<contactref element="U2" pad="26"/>
<contactref element="U$3" pad="P$8"/>
</signal>
<signal name="SSEL">
<contactref element="U2" pad="14"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="11"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="17"/>
</signal>
<signal name="IRQ">
<contactref element="U2" pad="25"/>
</signal>
<signal name="3V3">
<contactref element="U2" pad="18"/>
<contactref element="U$3" pad="P$21"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="USER_TX">
<contactref element="U$3" pad="P$6"/>
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="16"/>
</signal>
<signal name="USER_RX">
<contactref element="U$3" pad="P$10"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="N$1">
<contactref element="U$3" pad="P$11"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="N$2">
<contactref element="U$3" pad="P$4"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="N$4">
<contactref element="U$3" pad="P$5"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$5">
<contactref element="U$3" pad="P$3"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$6">
<contactref element="U$3" pad="P$2"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="USER_RTS">
<contactref element="U$3" pad="P$7"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="USER_CTS">
<contactref element="U$3" pad="P$9"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="N$7">
<contactref element="U$3" pad="P$13"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="N$10">
<contactref element="U$3" pad="P$14"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="N$11">
<contactref element="U$3" pad="P$17"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="N$13">
<contactref element="U$3" pad="P$16"/>
</signal>
<signal name="N$14">
<contactref element="D1" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R2" pad="2"/>
<contactref element="U$3" pad="P$15"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
