<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="53.01" y2="0" width="0" layer="20"/>
<wire x1="53.01" y1="0" x2="53.01" y2="50.79" width="0" layer="20"/>
<wire x1="53.01" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<text>SD     Tiva
1        PD_1
2        PD_3
4        +3.3V
5        PD_0
6        GND
8        PD_2</text>
<text>RTC/GPS   Tiva
CLK/RX     PC_4
DAT/TX      PC_5
RST           PC_6</text>
</plain>
<libraries>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TE-CON-SD-CARD">
<description>TE Connectivity SD Card connector 2041021</description>
</package>
</packages>
</library>
<library name="con-samtec">
<description>&lt;b&gt;Samtec Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSW-110-02-S-D">
<description>&lt;b&gt;THROUGH-HOLE .025" SQ POST HEADER&lt;/b&gt;&lt;p&gt;
Source: Samtec TSW.pdf</description>
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LSP10">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.0 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="SparkFun-Boards" package="TE-CON-SD-CARD" value="TE-CON-SD-CARDSMD2041021"/>
<element name="X1" library="con-samtec" package="TSW-110-02-S-D" value="TSW-110-02-S-D">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-samtec" package="TSW-110-02-S-D" value="TSW-110-02-S-D">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="VCC" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CLK/RX" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DAT/TX" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RST" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="X1" pad="7"/>
<contactref element="U$1" pad="P1"/>
</signal>
<signal name="N$5">
<contactref element="X1" pad="5"/>
<contactref element="U$1" pad="P5"/>
</signal>
<signal name="N$4">
<contactref element="X1" pad="9"/>
<contactref element="U$1" pad="P7"/>
</signal>
<signal name="N$2">
<contactref element="X1" pad="11"/>
<contactref element="U$1" pad="P2"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P4"/>
<contactref element="X1" pad="2"/>
<contactref element="VCC" pad="MP"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P6"/>
<contactref element="X1" pad="3"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND3"/>
<contactref element="U$1" pad="P3"/>
</signal>
<signal name="N$9">
<contactref element="CLK/RX" pad="MP"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="DAT/TX" pad="MP"/>
<contactref element="X2" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="RST" pad="MP"/>
<contactref element="X2" pad="12"/>
</signal>
<signal name="N$11">
<contactref element="GND" pad="MP"/>
<contactref element="X2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
