<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.6425" y2="0" width="0" layer="20"/>
<wire x1="33.6425" y1="0" x2="33.6425" y2="37.7725" width="0" layer="20"/>
<wire x1="33.6425" y1="37.7725" x2="0" y2="37.7725" width="0" layer="20"/>
<wire x1="0" y1="37.7725" x2="0" y2="0" width="0" layer="20"/>
<text>SW1</text>
<text>SW2</text>
<text>SW3</text>
<text>PWR</text>
<text>PRNT</text>
<text>LCD</text>
<text>3V3</text>
<text>5V</text>
<text>GPIO4</text>
<text>GPIO27</text>
<text>GPIO8</text>
<text>GPIO7</text>
<text>GND</text>
<text>MOSI</text>
<text>MISO</text>
<text>CLK</text>
<text>Guest Kiosk 201503.3</text>
<text>TDYKES.COM</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X13">
</package>
<package name="MOLEX-1X4">
</package>
<package name="MOLEX-1X2">
</package>
<package name="MOLEX-1X3">
</package>
<package name="1X10_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="2X13" value="M13X22X13"/>
<element name="LCD" library="SparkFun-Connectors" package="MOLEX-1X4" value="LCD"/>
<element name="POWER" library="SparkFun-Connectors" package="MOLEX-1X2" value="POWER"/>
<element name="SER" library="SparkFun-Connectors" package="MOLEX-1X3" value="SER"/>
<element name="SW1" library="SparkFun-Connectors" package="MOLEX-1X3" value="SW1"/>
<element name="SW2" library="SparkFun-Connectors" package="MOLEX-1X3" value="SW2"/>
<element name="SW3" library="SparkFun-Connectors" package="MOLEX-1X3" value="SW3"/>
<element name="JP4" library="SparkFun-Connectors" package="1X10_NO_SILK" value="M10NO_SILK_PTH_FEMALE">
<attribute name="PROD_ID" value="CONN-11563"/>
</element>
</elements>
<signals>
<signal name="5V">
<contactref element="JP1" pad="2"/>
<contactref element="LCD" pad="2"/>
<contactref element="POWER" pad="2"/>
<contactref element="JP4" pad="8"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="6"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW2" pad="1"/>
<contactref element="SW3" pad="1"/>
<contactref element="SER" pad="1"/>
<contactref element="LCD" pad="1"/>
<contactref element="POWER" pad="1"/>
<contactref element="JP4" pad="10"/>
</signal>
<signal name="TXD">
<contactref element="JP1" pad="8"/>
<contactref element="SER" pad="2"/>
</signal>
<signal name="RXD">
<contactref element="JP1" pad="10"/>
<contactref element="SER" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="JP1" pad="3"/>
<contactref element="LCD" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="JP1" pad="5"/>
<contactref element="LCD" pad="4"/>
</signal>
<signal name="GPIO17">
<contactref element="JP1" pad="11"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="GPIO18">
<contactref element="JP1" pad="12"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="GPIO22">
<contactref element="JP1" pad="15"/>
<contactref element="SW2" pad="2"/>
</signal>
<signal name="GPIO23">
<contactref element="JP1" pad="16"/>
<contactref element="SW2" pad="3"/>
</signal>
<signal name="GPIO24">
<contactref element="JP1" pad="18"/>
<contactref element="SW3" pad="2"/>
</signal>
<signal name="GPIO25">
<contactref element="JP1" pad="22"/>
<contactref element="SW3" pad="3"/>
</signal>
<signal name="3V3">
<contactref element="JP1" pad="1"/>
<contactref element="JP4" pad="9"/>
</signal>
<signal name="GPIO8">
<contactref element="JP1" pad="24"/>
<contactref element="JP4" pad="5"/>
</signal>
<signal name="GPIO4">
<contactref element="JP1" pad="7"/>
<contactref element="JP4" pad="7"/>
</signal>
<signal name="GPIO10">
<contactref element="JP1" pad="19"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="GPIO27">
<contactref element="JP1" pad="13"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="GPIO7">
<contactref element="JP1" pad="26"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="GPIO9">
<contactref element="JP1" pad="21"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="GPIO11">
<contactref element="JP1" pad="23"/>
<contactref element="JP4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
