<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<text>Infinite Noise</text>
<text>INFNOISE TRNG</text>
<wire x1="0" y1="0" x2="0" y2="12.192" width="0" layer="20"/>
<wire x1="0" y1="12.192" x2="34.8488" y2="12.192" width="0" layer="20"/>
<wire x1="34.8488" y1="12.192" x2="34.8488" y2="0" width="0" layer="20"/>
<wire x1="34.8488" y1="0" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="infnoise">
<description>Parts for the Infinite Noise Generator</description>
<packages>
<package name="0603-IND">
</package>
<package name="DFN8-2X3">
<description>&lt;b&gt;DCB Package 8-Lead Plastic DFN (2mm × 2mm)&lt;/b&gt;&lt;p&gt;
Source: http://www.linear.com/pc/downloadDocument.do?navId=H0,C1,C1003,C1042,C1032,C1063,P26952,D16357</description>
</package>
<package name="SSOP8-P-0.50A">
</package>
<package name="QFN24-4X4">
<description>&lt;b&gt;UF Package 24-Lead (4mm × 4mm) Plastic QFN&lt;/b&gt;&lt;p&gt;
Source: http://cds.linear.com/docs/Datasheet/5598f.pdf</description>
</package>
<package name="SC70-5L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="USB-A-PCB">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MICRO-FIDUCIAL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="AMP1" library="infnoise" package="DFN8-2X3" value="TSV912IQ2T"/>
<element name="C8" library="infnoise" package="0603-CAP" value="220pF"/>
<element name="C9" library="infnoise" package="0603-CAP" value="220pF">
<attribute name="NAME"/>
</element>
<element name="C4" library="infnoise" package="0603-CAP" value="47pF">
<attribute name="NAME"/>
</element>
<element name="C5" library="infnoise" package="0603-CAP" value="47pF">
<attribute name="NAME"/>
</element>
<element name="C6" library="infnoise" package="0603-CAP" value="100nF"/>
<element name="C2" library="infnoise" package="0603-CAP" value="4.7uF"/>
<element name="C3" library="infnoise" package="0603-CAP" value="100nF"/>
<element name="C1" library="infnoise" package="0603-CAP" value="10nF"/>
<element name="COMP1" library="infnoise" package="SSOP8-P-0.50A" value="TC75W57FK"/>
<element name="USB1" library="infnoise" package="QFN24-4X4" value="FT240XQ">
<attribute name="NAME"/>
</element>
<element name="L1" library="infnoise" package="0603-IND" value="FERRITE-BEAD0603-IND"/>
<element name="R1" library="infnoise" package="0603-RES" value="27">
<attribute name="NAME"/>
</element>
<element name="R2" library="infnoise" package="0603-RES" value="27">
<attribute name="NAME"/>
</element>
<element name="R6" library="infnoise" package="0603-RES" value="8.2K"/>
<element name="R5" library="infnoise" package="0603-RES" value="10K"/>
<element name="R7" library="infnoise" package="0603-RES" value="8.2K"/>
<element name="R8" library="infnoise" package="0603-RES" value="10K"/>
<element name="R3" library="infnoise" package="0603-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="R4" library="infnoise" package="0603-RES" value="10K">
<attribute name="NAME"/>
</element>
<element name="R9" library="infnoise" package="0603-RES" value="10K"/>
<element name="SW1" library="infnoise" package="SC70-5L" value="MC74VHC1G66DFT1G">
<attribute name="NAME"/>
</element>
<element name="SW2" library="infnoise" package="SC70-5L" value="MC74VHC1G66DFT1G"/>
<element name="C7" library="infnoise" package="0603-CAP" value="10nF">
<attribute name="NAME"/>
</element>
<element name="FID1" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="FID2" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="FID3" library="SparkFun-Aesthetics" package="MICRO-FIDUCIAL" value="FIDUCIALUFIDUCIAL"/>
<element name="X1" library="infnoise" package="USB-A-PCB" value="USB"/>
</elements>
<signals>
<signal name="USB_P">
<contactref element="C4" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="X1" pad="USB_P"/>
</signal>
<signal name="USB_M">
<contactref element="R2" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="X1" pad="USB_M"/>
</signal>
<signal name="VCCIN">
<contactref element="C1" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="X1" pad="5V"/>
</signal>
<signal name="VCC">
<contactref element="USB1" pad="15"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="USB1" pad="3"/>
<contactref element="USB1" pad="16"/>
<contactref element="USB1" pad="EXP"/>
<contactref element="C8" pad="1"/>
<contactref element="AMP1" pad="4"/>
<contactref element="AMP1" pad="EXP"/>
<contactref element="COMP1" pad="4"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW2" pad="3"/>
<contactref element="USB1" pad="9"/>
<contactref element="USB1" pad="8"/>
<contactref element="USB1" pad="7"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="X1" pad="GND"/>
</signal>
<signal name="VCC33">
<contactref element="USB1" pad="24"/>
<contactref element="COMP1" pad="8"/>
<contactref element="AMP1" pad="8"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW2" pad="5"/>
<contactref element="USB1" pad="12"/>
<contactref element="USB1" pad="13"/>
<contactref element="C6" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="A">
<contactref element="AMP1" pad="3"/>
<contactref element="C8" pad="2"/>
<contactref element="COMP1" pad="3"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="AMP1OUT">
<contactref element="SW2" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="AMP1" pad="1"/>
</signal>
<signal name="FB1">
<contactref element="AMP1" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="AMP2OUT">
<contactref element="SW1" pad="1"/>
<contactref element="AMP1" pad="7"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="FB2">
<contactref element="R7" pad="2"/>
<contactref element="AMP1" pad="6"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="B">
<contactref element="AMP1" pad="5"/>
<contactref element="COMP1" pad="5"/>
<contactref element="SW2" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="COMP1">
<contactref element="COMP1" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="USB1" pad="1"/>
</signal>
<signal name="COMP2">
<contactref element="COMP1" pad="7"/>
<contactref element="R8" pad="2"/>
<contactref element="USB1" pad="22"/>
</signal>
<signal name="VREF">
<contactref element="COMP1" pad="2"/>
<contactref element="COMP1" pad="6"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="SW1EN">
<contactref element="SW1" pad="4"/>
<contactref element="USB1" pad="23"/>
</signal>
<signal name="USBDM">
<contactref element="R2" pad="2"/>
<contactref element="USB1" pad="11"/>
</signal>
<signal name="SW2EN">
<contactref element="SW2" pad="4"/>
<contactref element="USB1" pad="21"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="2"/>
<contactref element="USB1" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
