<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.3" y2="0" width="0" layer="20"/>
<wire x1="20.3" y1="0" x2="20.32" y2="17.78" width="0" layer="20"/>
<wire x1="20.32" y1="17.78" x2="0" y2="17.78" width="0" layer="20"/>
<wire x1="0" y1="17.78" x2="0" y2="0" width="0" layer="20"/>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LONGPADS">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RED" library="adafruit" package="CHIPLED_1206" value="APT3216SURCK">
<attribute name="NAME"/>
</element>
<element name="GRN" library="adafruit" package="CHIPLED_1206" value="APT3216QBC">
<attribute name="NAME"/>
</element>
<element name="BLU" library="adafruit" package="CHIPLED_1206" value="APT3216QBC">
<attribute name="NAME"/>
</element>
<element name="WHT" library="adafruit" package="CHIPLED_1206" value="XZCWD55F-1">
<attribute name="NAME"/>
</element>
<element name="YEL" library="adafruit" package="CHIPLED_1206" value="APT3216YC">
<attribute name="NAME"/>
</element>
<element name="AMB" library="adafruit" package="CHIPLED_1206" value="150120AS75000">
<attribute name="NAME"/>
</element>
<element name="ANODE" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="CATHODE" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="ANODE" pad="6"/>
<contactref element="RED" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="ANODE" pad="5"/>
<contactref element="GRN" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="ANODE" pad="4"/>
<contactref element="BLU" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="ANODE" pad="3"/>
<contactref element="WHT" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="ANODE" pad="2"/>
<contactref element="YEL" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="ANODE" pad="1"/>
<contactref element="AMB" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="AMB" pad="C"/>
<contactref element="CATHODE" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="YEL" pad="C"/>
<contactref element="CATHODE" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="WHT" pad="C"/>
<contactref element="CATHODE" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="CATHODE" pad="4"/>
<contactref element="BLU" pad="C"/>
</signal>
<signal name="N$11">
<contactref element="GRN" pad="C"/>
<contactref element="CATHODE" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="CATHODE" pad="6"/>
<contactref element="RED" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
