<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="38.1" width="0.254" layer="20"/>
<wire x1="0" y1="38.1" x2="25.4" y2="38.1" width="0.254" layer="20"/>
<wire x1="25.4" y1="38.1" x2="25.4" y2="0" width="0.254" layer="20"/>
<wire x1="25.4" y1="0" x2="0" y2="0" width="0.254" layer="20"/>
<text>5V</text>
<text>GND</text>
<text>M1</text>
<text>GND</text>
<text>M2</text>
<text>GND</text>
<text>M3</text>
<text>GND</text>
<text>M4</text>
<text>GND</text>
<text>SP+</text>
<text>SP-</text>
<text>PLAY</text>
<text>RECORD</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="SO-28W">
<description>&lt;B&gt;Small Outline Wide Plastic Gull Wing&lt;/B&gt;&lt;p&gt;
300-mil body, package type SO</description>
</package>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
<package name="0603-RES">
</package>
<package name="LED-0603">
</package>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
<package name="1X02">
</package>
<package name="1X08">
</package>
<package name="MIC-9.7MM">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="PS603">
</package>
</packages>
</library>
<library name="_DENNIS">
<description>Dennis Personal collection of parts.
http://www.atmel.com/images/doc2549.pdf</description>
<packages>
<package name="DCLOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun" package="SO-28W" value="ISD1900ISD1932">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="0603-RES" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="SparkFun" package="LED-0603" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun" package="AYZ0202" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun" package="0603-RES" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="0603-RES" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun" package="0603-RES" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun" package="0603-CAP" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun" package="0603-RES" value="54K"/>
<element name="U$10" library="SparkFun" package="MIC-9.7MM" value="MIC9.7MM"/>
<element name="U$14" library="adafruit" package="PS603" value="PS603SPK"/>
<element name="U$15" library="_DENNIS" package="DCLOGO" value="DCLOGO"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C7" pad="C"/>
<contactref element="C5" pad="C"/>
<contactref element="C2" pad="2"/>
<contactref element="C6" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="C"/>
<contactref element="C3" pad="2"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="16"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="JP4" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="U1" pad="27"/>
<contactref element="U1" pad="25"/>
<contactref element="JP7" pad="2"/>
<contactref element="JP7" pad="4"/>
<contactref element="JP7" pad="6"/>
<contactref element="JP7" pad="8"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="5V">
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="A"/>
<contactref element="C1" pad="1"/>
<contactref element="C6" pad="A"/>
<contactref element="C2" pad="1"/>
<contactref element="C5" pad="A"/>
<contactref element="U1" pad="28"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="14"/>
<contactref element="S1" pad="3"/>
<contactref element="JP4" pad="2"/>
<contactref element="LED1" pad="A"/>
<contactref element="R2" pad="2"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="23"/>
</signal>
<signal name="REC">
<contactref element="U1" pad="24"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="MIC+">
<contactref element="U1" pad="18"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="MIC-">
<contactref element="U1" pad="19"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="AGC">
<contactref element="U1" pad="17"/>
<contactref element="C7" pad="A"/>
</signal>
<signal name="FT">
<contactref element="U1" pad="26"/>
</signal>
<signal name="SP+">
<contactref element="U1" pad="15"/>
<contactref element="JP5" pad="1"/>
<contactref element="U$14" pad="1"/>
</signal>
<signal name="SP-">
<contactref element="U1" pad="13"/>
<contactref element="JP5" pad="2"/>
<contactref element="U$14" pad="2"/>
</signal>
<signal name="LED">
<contactref element="U1" pad="22"/>
<contactref element="R1" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="U$10" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="U$10" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="M1">
<contactref element="U1" pad="2"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="M2">
<contactref element="JP7" pad="3"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="M3">
<contactref element="U1" pad="4"/>
<contactref element="JP7" pad="5"/>
</signal>
<signal name="M4">
<contactref element="JP7" pad="7"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="R5" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
