<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="33.25" x2="0" y2="2.75" width="0.05" layer="20"/>
<wire x1="0" y1="2.75" x2="2.75" y2="0" width="0.05" layer="20" curve="90"/>
<wire x1="33.25" y1="0" x2="36" y2="2.75" width="0.05" layer="20" curve="90"/>
<wire x1="36" y1="2.75" x2="36" y2="33.25" width="0.05" layer="20"/>
<wire x1="36" y1="33.25" x2="33.25" y2="36" width="0.05" layer="20" curve="90"/>
<wire x1="2.75" y1="36" x2="0" y2="33.25" width="0.05" layer="20" curve="90"/>
<wire x1="2.75" y1="0" x2="33.25" y2="0" width="0.05" layer="20"/>
<text>PDB36 v1.0
2014-DEC-26
TIM KOSTKA</text>
<wire x1="2.75" y1="36" x2="33.25" y2="36" width="0.05" layer="20"/>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="kcl_pdb360">
<packages>
<package name="HOLE3MM">
</package>
<package name="SLOT18AWG">
</package>
<package name="12AWG">
<description>Hole for soldering 12 AWG wire.</description>
</package>
<package name="ZIPTIE3MM">
<description>Plated via for a small zip tie.</description>
</package>
</packages>
</library>
<library name="kcl_passives">
<packages>
<package name="HDR1X03">
</package>
<package name="WSL3921">
<description>Vishay Power Metal Strip resistor.</description>
</package>
<package name="HDR1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="kcl_passives" package="WSL3921" value="0.001">
<attribute name="VALUE"/>
</element>
<element name="J1" library="kcl_pdb360" package="HOLE3MM" value="TPMOUNT3MM"/>
<element name="J2" library="kcl_pdb360" package="HOLE3MM" value="TPMOUNT3MM"/>
<element name="J3" library="kcl_pdb360" package="HOLE3MM" value="TPMOUNT3MM"/>
<element name="J4" library="kcl_pdb360" package="HOLE3MM" value="TPMOUNT3MM"/>
<element name="J5" library="kcl_pdb360" package="SLOT18AWG" value="+"/>
<element name="J6" library="kcl_pdb360" package="SLOT18AWG" value="+"/>
<element name="J7" library="kcl_passives" package="HDR1X03" value="HDR1X3">
<attribute name="VALUE"/>
</element>
<element name="J8" library="kcl_pdb360" package="SLOT18AWG" value="+"/>
<element name="J9" library="kcl_pdb360" package="SLOT18AWG" value="+"/>
<element name="J10" library="kcl_pdb360" package="SLOT18AWG" value="-"/>
<element name="J11" library="kcl_pdb360" package="SLOT18AWG" value="-"/>
<element name="J12" library="kcl_pdb360" package="SLOT18AWG" value="-"/>
<element name="J13" library="kcl_pdb360" package="SLOT18AWG" value="-"/>
<element name="J15" library="kcl_passives" package="HDR1X02" value="HDR1X2">
<attribute name="VALUE"/>
</element>
<element name="J14" library="kcl_passives" package="HDR1X02" value="HDR1X2">
<attribute name="VALUE"/>
</element>
<element name="J16" library="kcl_pdb360" package="12AWG" value="TP12AWG"/>
<element name="J17" library="kcl_pdb360" package="12AWG" value="TP12AWG"/>
<element name="J18" library="kcl_pdb360" package="ZIPTIE3MM" value="TPZIPTIE3MM"/>
<element name="J19" library="kcl_pdb360" package="ZIPTIE3MM" value="TPZIPTIE3MM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="J7" pad="1"/>
<contactref element="J10" pad="1@3"/>
<contactref element="J10" pad="1@4"/>
<contactref element="J10" pad="1@2"/>
<contactref element="J10" pad="1@1"/>
<contactref element="J11" pad="1@3"/>
<contactref element="J11" pad="1@4"/>
<contactref element="J11" pad="1@2"/>
<contactref element="J11" pad="1@1"/>
<contactref element="J12" pad="1@3"/>
<contactref element="J12" pad="1@4"/>
<contactref element="J12" pad="1@2"/>
<contactref element="J12" pad="1@1"/>
<contactref element="J13" pad="1@3"/>
<contactref element="J13" pad="1@4"/>
<contactref element="J13" pad="1@2"/>
<contactref element="J13" pad="1@1"/>
<contactref element="J15" pad="1"/>
<contactref element="J14" pad="1"/>
<contactref element="J17" pad="1@5"/>
<contactref element="J17" pad="1@3"/>
<contactref element="J17" pad="1@10"/>
<contactref element="J17" pad="1@8"/>
<contactref element="J17" pad="1@12"/>
<contactref element="J17" pad="1@1"/>
<contactref element="J17" pad="1@13"/>
<contactref element="J17" pad="1@4"/>
<contactref element="J17" pad="1@7"/>
<contactref element="J17" pad="1@9"/>
<contactref element="J17" pad="1@11"/>
<contactref element="J17" pad="1@6"/>
<contactref element="J17" pad="1@2"/>
<contactref element="J18" pad="P$1"/>
<contactref element="J10" pad="1@5"/>
<contactref element="J10" pad="1@6"/>
<contactref element="J10" pad="1@7"/>
<contactref element="J10" pad="1@8"/>
<contactref element="J10" pad="1@9"/>
<contactref element="J10" pad="1@10"/>
<contactref element="J10" pad="1@11"/>
<contactref element="J10" pad="1@12"/>
<contactref element="J10" pad="1@13"/>
<contactref element="J11" pad="1@5"/>
<contactref element="J11" pad="1@6"/>
<contactref element="J11" pad="1@7"/>
<contactref element="J11" pad="1@8"/>
<contactref element="J11" pad="1@9"/>
<contactref element="J11" pad="1@10"/>
<contactref element="J11" pad="1@11"/>
<contactref element="J11" pad="1@12"/>
<contactref element="J11" pad="1@13"/>
<contactref element="J12" pad="1@5"/>
<contactref element="J12" pad="1@6"/>
<contactref element="J12" pad="1@7"/>
<contactref element="J12" pad="1@8"/>
<contactref element="J12" pad="1@9"/>
<contactref element="J12" pad="1@10"/>
<contactref element="J12" pad="1@11"/>
<contactref element="J12" pad="1@12"/>
<contactref element="J12" pad="1@13"/>
<contactref element="J13" pad="1@5"/>
<contactref element="J13" pad="1@6"/>
<contactref element="J13" pad="1@7"/>
<contactref element="J13" pad="1@8"/>
<contactref element="J13" pad="1@9"/>
<contactref element="J13" pad="1@10"/>
<contactref element="J13" pad="1@11"/>
<contactref element="J13" pad="1@12"/>
<contactref element="J13" pad="1@13"/>
</signal>
<signal name="VIN">
<contactref element="R1" pad="1"/>
<contactref element="J7" pad="2"/>
<contactref element="J16" pad="1@5"/>
<contactref element="J16" pad="1@3"/>
<contactref element="J16" pad="1@10"/>
<contactref element="J16" pad="1@8"/>
<contactref element="J16" pad="1@12"/>
<contactref element="J16" pad="1@1"/>
<contactref element="J16" pad="1@13"/>
<contactref element="J16" pad="1@4"/>
<contactref element="J16" pad="1@7"/>
<contactref element="J16" pad="1@9"/>
<contactref element="J16" pad="1@11"/>
<contactref element="J16" pad="1@6"/>
<contactref element="J16" pad="1@2"/>
<contactref element="J19" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="J7" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="J9" pad="1@3"/>
<contactref element="J9" pad="1@4"/>
<contactref element="J9" pad="1@2"/>
<contactref element="J9" pad="1@1"/>
<contactref element="J8" pad="1@3"/>
<contactref element="J8" pad="1@4"/>
<contactref element="J8" pad="1@2"/>
<contactref element="J8" pad="1@1"/>
<contactref element="J6" pad="1@3"/>
<contactref element="J6" pad="1@4"/>
<contactref element="J6" pad="1@2"/>
<contactref element="J6" pad="1@1"/>
<contactref element="J5" pad="1@3"/>
<contactref element="J5" pad="1@4"/>
<contactref element="J5" pad="1@2"/>
<contactref element="J5" pad="1@1"/>
<contactref element="J15" pad="2"/>
<contactref element="J14" pad="2"/>
<contactref element="J5" pad="1@5"/>
<contactref element="J5" pad="1@6"/>
<contactref element="J5" pad="1@7"/>
<contactref element="J5" pad="1@8"/>
<contactref element="J5" pad="1@9"/>
<contactref element="J5" pad="1@10"/>
<contactref element="J5" pad="1@11"/>
<contactref element="J5" pad="1@12"/>
<contactref element="J5" pad="1@13"/>
<contactref element="J6" pad="1@5"/>
<contactref element="J6" pad="1@6"/>
<contactref element="J6" pad="1@7"/>
<contactref element="J6" pad="1@8"/>
<contactref element="J6" pad="1@9"/>
<contactref element="J6" pad="1@10"/>
<contactref element="J6" pad="1@11"/>
<contactref element="J6" pad="1@12"/>
<contactref element="J6" pad="1@13"/>
<contactref element="J8" pad="1@5"/>
<contactref element="J8" pad="1@6"/>
<contactref element="J8" pad="1@7"/>
<contactref element="J8" pad="1@8"/>
<contactref element="J8" pad="1@9"/>
<contactref element="J8" pad="1@10"/>
<contactref element="J8" pad="1@11"/>
<contactref element="J8" pad="1@12"/>
<contactref element="J8" pad="1@13"/>
<contactref element="J9" pad="1@5"/>
<contactref element="J9" pad="1@6"/>
<contactref element="J9" pad="1@7"/>
<contactref element="J9" pad="1@8"/>
<contactref element="J9" pad="1@9"/>
<contactref element="J9" pad="1@10"/>
<contactref element="J9" pad="1@11"/>
<contactref element="J9" pad="1@12"/>
<contactref element="J9" pad="1@13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
