<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<hole x="29.28209375" y="12.597984375" drill="2.05231875"/>
<hole x="22.18225625" y="12.64470625" drill="2.05231875"/>
<hole x="14.937175" y="12.46259375" drill="2.05231875"/>
<text>5V</text>
<text>Button</text>
<text>LED</text>
<text>Mindbender Mansion</text>
<text>Floor Switch  OMSI 2014</text>
<text>Mindbender Mansion</text>
<text>Avago ASMT-QRBD-AEF0E (red)</text>
<text>Avago ASMT-QGBE-NFH0E (green)</text>
<text>thomas h. 10/2014</text>
<text>10 ohm resistors for green</text>
<text>18 ohm resistors for red</text>
<wire x1="-3.81" y1="37.1475" x2="-3.4925" y2="3.81" width="0.1524" layer="20" curve="-91.67683"/>
<wire x1="-3.4925" y1="3.81" x2="3.81" y2="-3.4925" width="0.1524" layer="20" curve="180"/>
<wire x1="3.81" y1="-3.4925" x2="37.30625" y2="-3.96875" width="0.1524" layer="20" curve="-93.369045"/>
<wire x1="37.30625" y1="-3.96875" x2="44.1325" y2="3.65125" width="0.1524" layer="20" curve="180"/>
<wire x1="44.1325" y1="3.65125" x2="44.29125" y2="36.98875" width="0.1524" layer="20" curve="-91.1124"/>
<wire x1="44.29125" y1="36.98875" x2="36.98875" y2="44.29125" width="0.1524" layer="20" curve="180"/>
<wire x1="36.98875" y1="44.29125" x2="3.65125" y2="44.1325" width="0.1524" layer="20" curve="-95.178482"/>
<wire x1="3.65125" y1="44.1325" x2="-3.81" y2="37.1475" width="0.1524" layer="20" curve="180"/>
<text>Spelling Floor Switch</text>
</plain>
<libraries>
<library name="Black_Star2">
<packages>
<package name="KSA_SEALED_TAC_SWITCH">
</package>
</packages>
</library>
<library name="OMSI - ADN">
<packages>
<package name="1X01-16GAUGE">
</package>
<package name="1X01-BOLT_HOLE">
</package>
<package name="LED_AVAGO_MOD2">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S3" library="Black_Star2" package="KSA_SEALED_TAC_SWITCH" value=""/>
<element name="5V" library="OMSI - ADN" package="1X01-16GAUGE" value="M01ADN">
<attribute name="NAME"/>
</element>
<element name="BUTTON" library="OMSI - ADN" package="1X01-16GAUGE" value="M01ADN">
<attribute name="NAME"/>
</element>
<element name="LED" library="OMSI - ADN" package="1X01-16GAUGE" value="M01ADN">
<attribute name="NAME"/>
</element>
<element name="JP1" library="OMSI - ADN" package="1X01-BOLT_HOLE" value="M01ADN2"/>
<element name="JP2" library="OMSI - ADN" package="1X01-BOLT_HOLE" value="M01ADN2"/>
<element name="JP3" library="OMSI - ADN" package="1X01-BOLT_HOLE" value="M01ADN2"/>
<element name="JP4" library="OMSI - ADN" package="1X01-BOLT_HOLE" value="M01ADN2"/>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="OMSI - ADN" package="LED_AVAGO_MOD2" value="LEDW/SINK"/>
<element name="U$2" library="OMSI - ADN" package="LED_AVAGO_MOD2" value="LEDW/SINK"/>
<element name="U$3" library="OMSI - ADN" package="LED_AVAGO_MOD2" value="LEDW/SINK"/>
<element name="U$4" library="OMSI - ADN" package="LED_AVAGO_MOD2" value="LEDW/SINK"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="5V" pad="1"/>
<contactref element="S3" pad="P$3"/>
<contactref element="R1" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$8">
<contactref element="BUTTON" pad="1"/>
<contactref element="S3" pad="P$1"/>
</signal>
<signal name="LGND">
<contactref element="LED" pad="1"/>
<contactref element="U$1" pad="C"/>
<contactref element="U$2" pad="C"/>
<contactref element="U$3" pad="C"/>
<contactref element="U$4" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="P$1"/>
<contactref element="U$1" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="A"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$5">
<contactref element="R3" pad="P$1"/>
<contactref element="U$3" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="U$4" pad="A"/>
<contactref element="R4" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
