<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.3">
<drawing>
<board>
<plain>
<circle x="23" y="23" radius="23" width="0.254" layer="20"/>
<text>GND</text>
<text>GND</text>
<text>Vcc</text>
<text>Vcc</text>
<text>RST</text>
<text>RST</text>
<text>TST</text>
<text>TST</text>
<text>LS</text>
<text>SW</text>
<text>_</text>
<text>_</text>
<text>+</text>
<text>+</text>
</plain>
<libraries>
<library name="TI_MSP430_v16">
<packages>
<package name="RSA16">
<description>*** TI: RSA *** JEDEC: S-PQFP-N16 *** 16 PINS ***
---&gt; PIN TP (exposed thermal die pad) should be connected with GND</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT89">
</package>
<package name="1206">
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B2,54">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="TI_MSP430_v16" package="RSA16" value="G2X[2/3]1---RSA16"/>
<element name="LED1_1" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED1_2" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED1_3" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED1_4" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED1_5" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED1_6" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED2_1" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED2_2" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED2_3" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED2_4" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED2_5" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED2_6" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED3_1" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED3_2" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED3_3" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED3_4" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED3_5" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="LED3_6" library="SparkFun" package="SOT89" value="AMC7135SOT89"/>
<element name="D1" library="SparkFun" package="1206" value=""/>
<element name="L3-" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="L2-" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="L1-" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="S+" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="S-" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun" package="1206" value=""/>
<element name="R2" library="SparkFun" package="1206" value=""/>
<element name="L1+" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="L2+" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="L3+" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="LS+" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LS-" library="testpad" package="B2,54" value="TPB2,54">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="JP1" library="SparkFun" package="1X04_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun" package="1206" value=""/>
</elements>
<signals>
<signal name="L2">
<contactref element="LED2_1" pad="3"/>
<contactref element="LED2_6" pad="3"/>
<contactref element="LED2_5" pad="3"/>
<contactref element="LED2_4" pad="3"/>
<contactref element="LED2_3" pad="3"/>
<contactref element="LED2_2" pad="3"/>
<contactref element="L2-" pad="TP"/>
</signal>
<signal name="GND">
<contactref element="LED1_6" pad="2"/>
<contactref element="LED1_6" pad="4"/>
<contactref element="LED3_6" pad="2"/>
<contactref element="LED3_6" pad="4"/>
<contactref element="LED2_6" pad="2"/>
<contactref element="LED2_6" pad="4"/>
<contactref element="LED2_1" pad="2"/>
<contactref element="LED2_1" pad="4"/>
<contactref element="LED2_2" pad="2"/>
<contactref element="LED2_2" pad="4"/>
<contactref element="LED2_3" pad="2"/>
<contactref element="LED2_3" pad="4"/>
<contactref element="LED2_4" pad="2"/>
<contactref element="LED2_4" pad="4"/>
<contactref element="LED2_5" pad="2"/>
<contactref element="LED2_5" pad="4"/>
<contactref element="LED3_5" pad="2"/>
<contactref element="LED3_5" pad="4"/>
<contactref element="LED3_4" pad="2"/>
<contactref element="LED3_4" pad="4"/>
<contactref element="LED3_3" pad="2"/>
<contactref element="LED3_3" pad="4"/>
<contactref element="LED3_2" pad="2"/>
<contactref element="LED3_2" pad="4"/>
<contactref element="LED3_1" pad="2"/>
<contactref element="LED3_1" pad="4"/>
<contactref element="S-" pad="TP"/>
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="13"/>
<contactref element="R2" pad="1"/>
<contactref element="LED1_5" pad="4"/>
<contactref element="LED1_5" pad="2"/>
<contactref element="LED1_4" pad="4"/>
<contactref element="LED1_4" pad="2"/>
<contactref element="LED1_3" pad="4"/>
<contactref element="LED1_3" pad="2"/>
<contactref element="LED1_2" pad="4"/>
<contactref element="LED1_2" pad="2"/>
<contactref element="LED1_1" pad="4"/>
<contactref element="LED1_1" pad="2"/>
<contactref element="LS-" pad="TP"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="D1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="L1+" pad="TP"/>
<contactref element="L2+" pad="TP"/>
<contactref element="L3+" pad="TP"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="4"/>
<contactref element="S+" pad="TP"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="16"/>
<contactref element="U$1" pad="15"/>
<contactref element="D1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="PWM">
<contactref element="LED1_2" pad="1"/>
<contactref element="LED1_3" pad="1"/>
<contactref element="LED1_4" pad="1"/>
<contactref element="LED1_5" pad="1"/>
<contactref element="LED1_6" pad="1"/>
<contactref element="LED1_1" pad="1"/>
<contactref element="LED2_6" pad="1"/>
<contactref element="LED2_5" pad="1"/>
<contactref element="LED2_4" pad="1"/>
<contactref element="LED2_3" pad="1"/>
<contactref element="LED2_2" pad="1"/>
<contactref element="LED2_1" pad="1"/>
<contactref element="LED3_6" pad="1"/>
<contactref element="LED3_5" pad="1"/>
<contactref element="LED3_4" pad="1"/>
<contactref element="LED3_3" pad="1"/>
<contactref element="LED3_2" pad="1"/>
<contactref element="LED3_1" pad="1"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="L1">
<contactref element="LED1_1" pad="3"/>
<contactref element="LED1_6" pad="3"/>
<contactref element="LED1_5" pad="3"/>
<contactref element="LED1_4" pad="3"/>
<contactref element="LED1_3" pad="3"/>
<contactref element="LED1_2" pad="3"/>
<contactref element="L1-" pad="TP"/>
</signal>
<signal name="L3">
<contactref element="LED3_1" pad="3"/>
<contactref element="LED3_6" pad="3"/>
<contactref element="LED3_5" pad="3"/>
<contactref element="LED3_4" pad="3"/>
<contactref element="LED3_3" pad="3"/>
<contactref element="LED3_2" pad="3"/>
<contactref element="L3-" pad="TP"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
<contactref element="U$1" pad="1"/>
<contactref element="LS+" pad="TP"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="9"/>
<contactref element="JP1" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
