<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="45.77" y2="0" width="0" layer="20"/>
<wire x1="45.77" y1="0" x2="45.77" y2="20" width="0" layer="20"/>
<wire x1="45.77" y1="20" x2="0" y2="20" width="0" layer="20"/>
<wire x1="0" y1="20" x2="0" y2="0" width="0" layer="20"/>
<text>V.6.2</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>PWM</text>
<text>1</text>
<text>2</text>
<text>John loves Anya
and our baby boy</text>
<text>blower</text>
<text>servo</text>
<text>5VTC</text>
<text>REFG</text>
<text>100k</text>
</plain>
<libraries>
<library name="rcl_smd">
<description>&lt;p&gt;&lt;b&gt;Resistors, Capacitors, Inductors in chip/molded packages&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;Land patterns as per IPC-SM-782&lt;/p&gt;
&lt;p&gt;Silk screen outlines as per &lt;a href="http://www.pcblibraries.com/forum/smt-library-silkscreen-outlines_topic26.html"&gt;http://www.pcblibraries.com/forum/smt-library-silkscreen-outlines_topic26.html&lt;/a&gt; with 0.3 mm between the body/pad and line center.&lt;/p&gt;</description>
<packages>
<package name="C0805">
<description>Metric: 2012</description>
</package>
<package name="R0805">
<description>Metric: 2012</description>
</package>
</packages>
</library>
<library name="v-reg">
<description>&lt;b&gt;Voltage Regulators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="HeaterMeterPI">
<description>Generated from &lt;b&gt;HeaterMeterPI.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="MSOP8">
</package>
<package name="RJ45-8-1H">
<description>Amphenol RJHSE-5080 no LED
Mouser 523-RJHSE-5080</description>
</package>
</packages>
</library>
<library name="2.5mm inline screw mono jack">
<description>Generated from &lt;b&gt;HeaterMeterPI.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="CUI-MJ-2508">
<description>CUI Inc MJ-2508 and MJ-2508N (non-threaded)

DigiKey Part CP-2508-ND and CP-2508N-ND</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="opamps">
<packages>
<package name="SOIC-8">
<description>SOIC-8</description>
</package>
</packages>
</library>
<library name="3361P-Trimmer">
<description>3314G-1-254E</description>
<packages>
<package name="3314G-1-254E">
<description>http://www.mouser.com/Search/ProductDetail.aspx?qs=fHAReS3gvjLSMYSnFcSX8Q%3d%3d</description>
</package>
</packages>
</library>
<library name="AMP_MTATC">
<packages>
<package name="1X06MTA">
</package>
</packages>
</library>
<library name="HeaterMeterPI inline jack2.5mm">
<description>Generated from &lt;b&gt;HeaterMeterPI.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="PCC-SMP">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rcl_smd" package="C0805" value=".1u">
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl_smd" package="C0805" value="1n">
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl_smd" package="C0805" value=".1u">
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl_smd" package="C0805" value=".1">
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl_smd" package="C0805" value="1n">
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl_smd" package="C0805" value="10n">
<attribute name="VALUE"/>
</element>
<element name="MCP1700" library="v-reg" package="SOT23" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="HeaterMeterPI" package="MSOP8" value="AD849X"/>
<element name="JP1" library="2.5mm inline screw mono jack" package="CUI-MJ-2508" value="AUDIO-MONO"/>
<element name="JP3" library="2.5mm inline screw mono jack" package="CUI-MJ-2508" value="AUDIO-MONO"/>
<element name="R24" library="rcl_smd" package="R0805" value="1k">
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl_smd" package="R0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl_smd" package="R0805" value="10k">
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl_smd" package="R0805" value="1m">
<attribute name="VALUE"/>
</element>
<element name="5VTOTC" library="jumper" package="SJ" value="5VTC">
<attribute name="VALUE"/>
</element>
<element name="REFTOGND" library="jumper" package="SJ" value="REFG">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="HeaterMeterPI" package="RJ45-8-1H" value="RJ45-8"/>
<element name="U2" library="opamps" package="SOIC-8" value="">
<attribute name="VALUE"/>
</element>
<element name="100K" library="3361P-Trimmer" package="3314G-1-254E" value="100k"/>
<element name="TC1" library="HeaterMeterPI inline jack2.5mm" package="PCC-SMP" value="THERMOCOUPLE"/>
<element name="J1" library="AMP_MTATC" package="1X06MTA" value=""/>
</elements>
<signals>
<signal name="N$1">
<contactref element="C9" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="R25" pad="1"/>
<contactref element="TC1" pad="TC+"/>
</signal>
<signal name="GND">
<contactref element="C8" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="R24" pad="1"/>
<contactref element="REFTOGND" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="MCP1700" pad="1"/>
<contactref element="U2" pad="4"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="100K" pad="1"/>
</signal>
<signal name="TCAMPOUT">
<contactref element="U$1" pad="7"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="GROUND">
<contactref element="U$1" pad="4"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SERVO">
<contactref element="U$1" pad="6"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="BLOWER+">
<contactref element="U$1" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="PROBE1">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PROBE2">
<contactref element="U$1" pad="2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="REF1">
<contactref element="U2" pad="2"/>
<contactref element="U2" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="REFTOGND" pad="1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U2" pad="3"/>
<contactref element="100K" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="5VTOTC" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="U2" pad="7"/>
<contactref element="MCP1700" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="MCP1700" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="5VTOTC" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R26" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="TC1" pad="TC-"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="100K" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
