<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="19.7231" x2="21.59" y2="19.7231" width="0" layer="20"/>
<wire x1="21.59" y1="19.7231" x2="21.59" y2="0.2225" width="0" layer="20"/>
<wire x1="21.59" y1="0.2225" x2="73.66" y2="0.2225" width="0" layer="20"/>
<wire x1="73.66" y1="0.2225" x2="73.66" y2="11.1125" width="0" layer="20"/>
<wire x1="73.66" y1="11.1125" x2="91.5924" y2="11.1125" width="0" layer="20"/>
<wire x1="91.5924" y1="11.1125" x2="91.5924" y2="56.1213" width="0" layer="20"/>
<wire x1="91.5924" y1="56.1213" x2="0" y2="56.1213" width="0" layer="20"/>
<wire x1="0" y1="56.1213" x2="0" y2="19.7231" width="0" layer="20"/>
<text>1</text>
<text>ATMEGA644A</text>
<text>D5</text>
<text>CONTRAST</text>
<text>GND</text>
<text>DC#1</text>
<text>80M</text>
<text>17/20M</text>
<text>6M</text>
<text>+13.8V</text>
<text>GND</text>
<text>10-15M</text>
<text>30/40M</text>
<text>PTT-&gt;</text>
<text>DC#2</text>
<text>COR</text>
<text>TEMP</text>
<text>VOLT</text>
<text>FWD</text>
<text>RFL</text>
<text>D5</text>
<text>HARDROCK50 AMPLIFIER</text>
<text>SANGUINO CONTROL BOARD</text>
<text>REV. E  10/2013</text>
<text>BAND UP</text>
<text>BAND DOWN</text>
<text>KEY MODE</text>
<text>KEY</text>
<text>MODE</text>
<text>BAND</text>
<text>UP</text>
<text>DOWN</text>
<text>BAND</text>
<text>PWR/TX</text>
<text>POWER/TX</text>
<text>HARDROCK-50 SANGUINO CTRL BRD</text>
<text></text>
<text>GND</text>
<text>+5V</text>
<text>TX1</text>
<text>SDA</text>
<text>DTR</text>
<text>PTT_IN</text>
<text>RX1</text>
<text>PGC</text>
<text>RB3</text>
<text>SCL</text>
<text>TRIM THESE PINS VERY CLOSE</text>
<text>AND SEE BUILD INSTRUCTIONS</text>
<text>FOR HOW TO CHECK CLEARANCE</text>
<text>REV. B 10/2012</text>
<text>R</text>
<text>G</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="LCD-16X2">
</package>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="M1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.25 W</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SMC_C">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="crystal">
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Curtis5">
<packages>
<package name="2X10/ROWSWAP">
</package>
<package name="BI-LED">
</package>
<package name="CA6V">
<description>&lt;b&gt;POTENTIOMETER&lt;/b&gt;&lt;p&gt;
distributor Schukat</description>
</package>
<package name="TO92">
<description>TO-92</description>
</package>
</packages>
</library>
<library name="diode">
<packages>
<package name="DO34-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 1.8 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="pinhead">
<packages>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2031">
<description>.100" (2.54mm) Center Header - 3 Pin</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL40">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C6" library="rcl" package="C1206" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="06R4202"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="X1" library="crystal" package="HC49/S" value="16mhz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="56P2867"/>
<attribute name="VENDOR" value="NEWARK"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="C1" library="rcl" package="C1206" value="22pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="22T0021"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="C2" library="rcl" package="C1206" value="22pf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="22T0021 "/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="C8" library="rcl" package="C1206" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="06R4202"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="C4" library="rcl" package="C1206" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="06R4202"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="D1" library="diode" package="DO34-7" value="1N914">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="1N914BCT-ND"/>
<attribute name="VENDOR" value="DIGIKEY"/>
</element>
<element name="D2" library="diode" package="DO34-7" value="1N914">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="1N914BCT-ND"/>
<attribute name="VENDOR" value="DIGIKEY"/>
</element>
<element name="C3" library="rcl" package="C1206" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="06R4202"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="R2" library="rcl" package="M1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="39K0872"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="R1" library="rcl" package="M1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="39K0871"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="R3" library="rcl" package="M1206" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="39K0871"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="JP5" library="Curtis5" package="2X10/ROWSWAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun" package="TACTILE-PTH" value="KEYMODE">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="15N4471"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="S2" library="SparkFun" package="TACTILE-PTH" value="BAND-DOWN">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="15N4471"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="S3" library="SparkFun" package="TACTILE-PTH" value="BAND-UP">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="15N4471"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="R7" library="rcl" package="M1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="39K0872"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="R6" library="rcl" package="M1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="39K0872"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="D3" library="Curtis5" package="BI-LED" value="LED-BICOLOR"/>
<element name="R10" library="Curtis5" package="CA6V" value="10K">
<attribute name="NAME"/>
<attribute name="PARTNUM" value="TPS-10K"/>
<attribute name="VENDOR" value="ALLELECTRONICS"/>
</element>
<element name="R4" library="rcl" package="M1206" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="53K2429"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="R5" library="rcl" package="M1206" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="53K2429"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="JP6" library="pinhead" package="2X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Curtis5" package="TO92" value="2N7000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PARTNUM" value="89K1814"/>
<attribute name="VENDOR" value="NEWARK"/>
</element>
<element name="C5" library="rcl" package="SMC_C" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="M1206" value="10K">
<attribute name="PARTNUM" value="53K2429"/>
<attribute name="VENDOR" value="NEWARK"/>
<attribute name="NAME"/>
</element>
<element name="C7" library="rcl" package="C1206" value=".1uF">
<attribute name="PARTNUM" value="06R4202"/>
<attribute name="VENDOR" value="NEWARK"/>
<attribute name="NAME"/>
</element>
<element name="JP4" library="con-molex" package="22-23-2031" value="RF SENSE">
<attribute name="OC_NEWARK" value="30C0862"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCD1" library="SparkFun" package="LCD-16X2" value="LCD-16X2SILK"/>
<element name="IC1" library="atmel" package="DIL40" value="ATMEGA644-10PU">
<attribute name="OC_NEWARK" value="23M5062"/>
<attribute name="MPN" value="ATMEGA644V-10PU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1288342"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="adafruit" package="TO252" value="7805DT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT"/>
<element name="JP2" library="SparkFun" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT"/>
<element name="JP3" library="SparkFun" package="STAND-OFF-TIGHT" value="STAND-OFFTIGHT"/>
<element name="R11" library="rcl" package="M1206" value="10K">
<attribute name="PARTNUM" value="39K0872"/>
<attribute name="VENDOR" value="NEWARK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="M1206" value="10K">
<attribute name="PARTNUM" value="39K0872"/>
<attribute name="VENDOR" value="NEWARK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="M1206" value="10K">
<attribute name="PARTNUM" value="39K0872"/>
<attribute name="VENDOR" value="NEWARK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="M1206" value="10K">
<attribute name="PARTNUM" value="53K2429"/>
<attribute name="VENDOR" value="NEWARK"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="S2" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="D3" pad="CATH"/>
<contactref element="JP6" pad="10"/>
<contactref element="Q1" pad="3"/>
<contactref element="C5" pad="-"/>
<contactref element="C4" pad="2"/>
<contactref element="JP4" pad="3"/>
<contactref element="LCD1" pad="16"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="31"/>
<contactref element="IC1" pad="31"/>
<contactref element="IC2" pad="3"/>
<contactref element="R10" pad="A"/>
<contactref element="LCD1" pad="1"/>
<contactref element="LCD1" pad="5"/>
<contactref element="JP5" pad="11"/>
<contactref element="JP5" pad="13"/>
<contactref element="JP5" pad="15"/>
<contactref element="JP5" pad="17"/>
<contactref element="JP5" pad="19"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="C6" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R10" pad="E"/>
<contactref element="JP6" pad="9"/>
<contactref element="C4" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="LCD1" pad="2"/>
<contactref element="LCD1" pad="15"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC1" pad="30"/>
<contactref element="IC2" pad="2"/>
<contactref element="JP4" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="V0">
<contactref element="R10" pad="S"/>
<contactref element="LCD1" pad="3"/>
</signal>
<signal name="PGC">
<contactref element="JP6" pad="6"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="+13.8V">
<contactref element="JP5" pad="1"/>
<contactref element="C5" pad="+"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="6M">
<contactref element="JP5" pad="3"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="DTC#1">
<contactref element="JP5" pad="9"/>
<contactref element="IC1" pad="33"/>
</signal>
<signal name="DTC#2">
<contactref element="JP5" pad="10"/>
<contactref element="IC1" pad="39"/>
</signal>
<signal name="PTTOUT">
<contactref element="JP5" pad="8"/>
<contactref element="IC1" pad="40"/>
</signal>
<signal name="COR">
<contactref element="JP5" pad="12"/>
<contactref element="IC1" pad="38"/>
</signal>
<signal name="RFLPOWER">
<contactref element="JP5" pad="14"/>
<contactref element="IC1" pad="37"/>
</signal>
<signal name="FWDPOWER">
<contactref element="JP5" pad="16"/>
<contactref element="IC1" pad="36"/>
</signal>
<signal name="TEMP">
<contactref element="JP5" pad="18"/>
<contactref element="IC1" pad="35"/>
</signal>
<signal name="VOLT">
<contactref element="JP5" pad="20"/>
<contactref element="IC1" pad="34"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="C"/>
<contactref element="C3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="PTT_PIC">
<contactref element="R1" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="IC1" pad="29"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="RS">
<contactref element="LCD1" pad="4"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="ENABLE">
<contactref element="LCD1" pad="6"/>
<contactref element="IC1" pad="24"/>
</signal>
<signal name="DB4">
<contactref element="LCD1" pad="11"/>
<contactref element="IC1" pad="25"/>
</signal>
<signal name="DB5">
<contactref element="LCD1" pad="12"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="DB7">
<contactref element="LCD1" pad="14"/>
<contactref element="IC1" pad="28"/>
</signal>
<signal name="UP">
<contactref element="S3" pad="3"/>
<contactref element="IC1" pad="19"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="DOWN">
<contactref element="S2" pad="3"/>
<contactref element="IC1" pad="20"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="MENU">
<contactref element="S1" pad="3"/>
<contactref element="IC1" pad="18"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="R7" pad="2"/>
<contactref element="JP6" pad="4"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="17/20M">
<contactref element="JP5" pad="5"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="80M">
<contactref element="JP5" pad="7"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="R">
<contactref element="D3" pad="R"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="G">
<contactref element="D3" pad="G"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="LED_GREEN">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="LED_RED">
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="PTT_IN">
<contactref element="R3" pad="1"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="RB3">
<contactref element="JP6" pad="2"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="RF_SAMPLE">
<contactref element="JP4" pad="2"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="10/12/15M">
<contactref element="JP5" pad="4"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="30/40M">
<contactref element="JP5" pad="6"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="9"/>
<contactref element="R8" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="IC1" pad="12"/>
<contactref element="X1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="XTAL1">
<contactref element="IC1" pad="13"/>
<contactref element="C2" pad="1"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="DB6">
<contactref element="LCD1" pad="13"/>
<contactref element="IC1" pad="27"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="23"/>
<contactref element="R6" pad="2"/>
<contactref element="JP6" pad="5"/>
</signal>
<signal name="TXO">
<contactref element="IC1" pad="15"/>
<contactref element="JP6" pad="7"/>
</signal>
<signal name="RXI">
<contactref element="IC1" pad="14"/>
<contactref element="JP6" pad="8"/>
</signal>
<signal name="PGM">
<contactref element="JP6" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$16">
</signal>
</signals>
</board>
</drawing>
</eagle>
