<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20"/>
<wire x1="1.27" y1="0" x2="40.64" y2="0" width="0" layer="20"/>
<wire x1="40.64" y1="0" x2="44.45" y2="3.81" width="0" layer="20"/>
<wire x1="44.45" y1="3.81" x2="44.45" y2="21.59" width="0" layer="20"/>
<wire x1="44.45" y1="21.59" x2="40.64" y2="25.4" width="0" layer="20"/>
<wire x1="40.64" y1="25.4" x2="1.27" y2="25.4" width="0" layer="20"/>
<wire x1="1.27" y1="25.4" x2="0" y2="24.13" width="0" layer="20"/>
<wire x1="0" y1="24.13" x2="0" y2="1.27" width="0" layer="20"/>
<text>VCC</text>
<text>FLOW_B</text>
<text>FLOW_A</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>Kegboard Coaster</text>
<text>7/2/2013</text>
<text>KEGBOT.ORG</text>
<text>VCC</text>
<text>GPIO_B</text>
<text>GPIO_A</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>OW_B</text>
<text>OW_A</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>FLOW_A</text>
<text>FLOW_B</text>
<text>2.1</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="RJ45-8">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="AXIAL-0.3">
</package>
<package name="SCREWTERMINAL-3.5MM-6">
</package>
</packages>
</library>
<library name="SparkFun-20100412">
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
<package name="CAP-PTH-SMALL2">
</package>
</packages>
</library>
<library name="geoffculp">
<packages>
<package name="TO-92">
<description>&lt;b&gt;TO 92&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mikey-molex">
<packages>
<package name="53324-0360">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="HEADER-RJ1" library="SparkFun" package="RJ45-8" value="RJ45-8PTH"/>
<element name="LED1" library="SparkFun" package="LED3MM" value=""/>
<element name="R1" library="SparkFun" package="AXIAL-0.3" value="1k"/>
<element name="JP2" library="SparkFun-20100412" package="STAND-OFF" value="STAND-OFF"/>
<element name="C1" library="SparkFun-20100412" package="CAP-PTH-SMALL2" value=""/>
<element name="U$1" library="geoffculp" package="TO-92" value="TEMPERATURE-SENSOR"/>
<element name="JP1-FLOW" library="SparkFun" package="SCREWTERMINAL-3.5MM-6" value=""/>
<element name="JP2-ONEWIRE" library="SparkFun" package="SCREWTERMINAL-3.5MM-6" value=""/>
<element name="JP3-GPIO" library="SparkFun" package="SCREWTERMINAL-3.5MM-6" value=""/>
<element name="JP4" library="mikey-molex" package="53324-0360" value="M03"/>
<element name="JP5" library="mikey-molex" package="53324-0360" value="M03"/>
</elements>
<signals>
<signal name="ONEWIRE_A">
<contactref element="HEADER-RJ1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="JP2-ONEWIRE" pad="2"/>
</signal>
<signal name="FLOW_B">
<contactref element="HEADER-RJ1" pad="8"/>
<contactref element="JP1-FLOW" pad="5"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="5V">
<contactref element="R1" pad="P$1"/>
<contactref element="HEADER-RJ1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="JP1-FLOW" pad="1"/>
<contactref element="JP1-FLOW" pad="4"/>
<contactref element="JP2-ONEWIRE" pad="1"/>
<contactref element="JP2-ONEWIRE" pad="4"/>
<contactref element="JP3-GPIO" pad="1"/>
<contactref element="JP3-GPIO" pad="4"/>
<contactref element="JP4" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="K"/>
<contactref element="HEADER-RJ1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="JP1-FLOW" pad="3"/>
<contactref element="JP1-FLOW" pad="6"/>
<contactref element="JP2-ONEWIRE" pad="3"/>
<contactref element="JP2-ONEWIRE" pad="6"/>
<contactref element="JP3-GPIO" pad="3"/>
<contactref element="JP3-GPIO" pad="6"/>
<contactref element="JP4" pad="3"/>
<contactref element="JP5" pad="3"/>
</signal>
<signal name="ONEWIRE_B">
<contactref element="HEADER-RJ1" pad="4"/>
<contactref element="JP2-ONEWIRE" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="P$2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="GPIO_A">
<contactref element="HEADER-RJ1" pad="3"/>
<contactref element="JP3-GPIO" pad="2"/>
</signal>
<signal name="FLOW_A">
<contactref element="HEADER-RJ1" pad="6"/>
<contactref element="JP1-FLOW" pad="2"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="GPIO_B">
<contactref element="HEADER-RJ1" pad="7"/>
<contactref element="JP3-GPIO" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
