<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.84" y2="0" width="0" layer="20"/>
<wire x1="22.84" y1="0" x2="22.84" y2="32.055" width="0" layer="20"/>
<wire x1="22.84" y1="32.055" x2="0" y2="32.055" width="0" layer="20"/>
<wire x1="0" y1="32.055" x2="0" y2="0" width="0" layer="20"/>
<text>IN-19 Socket Board - marc2912.com</text>
<hole x="11.43" y="16.51" drill="5.08"/>
<text>LEG</text>
<text>FRONT</text>
</plain>
<libraries>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2071">
<description>.100" (2.54mm) Center Header - 7 Pin</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="RTH025W">
</package>
</packages>
</library>
<library name="russian-nixies">
<description>&lt;b&gt;Russian IN series nixie tubes&lt;/b&gt;&lt;br&gt;&lt;br&gt;

Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Measurements taken from nixies in my collection
&lt;li&gt;http://www.tube-tester.com
&lt;/ul&gt;&lt;br&gt;
&lt;author&gt;Created by p.s.troost@student.tue.nl&lt;/author&gt;</description>
<packages>
<package name="IN-19">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CON1" library="con-molex" package="22-23-2071" value="HOT">
<attribute name="OC_NEWARK" value="56H0445"/>
<attribute name="MPN" value="22-23-2071"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1654534"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON2" library="con-molex" package="22-23-2071" value="">
<attribute name="OC_NEWARK" value="56H0445"/>
<attribute name="MPN" value="22-23-2071"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="1654534"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="dp_devices" package="RTH025W" value="10K">
<attribute name="VALUE"/>
</element>
<element name="IN-19" library="russian-nixies" package="IN-19" value="IN-19A">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="180V">
<contactref element="R1" pad="1"/>
<contactref element="IN-19" pad="8"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="CON1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="CON1" pad="3"/>
<contactref element="IN-19" pad="11"/>
</signal>
<signal name="N$8">
<contactref element="IN-19" pad="5"/>
<contactref element="CON2" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="IN-19" pad="4"/>
<contactref element="CON2" pad="4"/>
</signal>
<signal name="N$10">
<contactref element="IN-19" pad="2"/>
<contactref element="CON2" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="IN-19" pad="14"/>
<contactref element="CON2" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="IN-19" pad="12"/>
<contactref element="CON2" pad="7"/>
</signal>
<signal name="N$1">
<contactref element="IN-19" pad="6"/>
<contactref element="CON2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IN-19" pad="10"/>
<contactref element="CON1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
