<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="15.24" y1="11.43" x2="27.94" y2="11.43" width="0" layer="20"/>
<wire x1="27.94" y1="11.43" x2="27.94" y2="13.335" width="0" layer="20"/>
<wire x1="27.94" y1="13.335" x2="33.02" y2="15.24" width="0" layer="20"/>
<wire x1="33.02" y1="15.24" x2="33.02" y2="69.205" width="0" layer="20"/>
<wire x1="33.02" y1="69.205" x2="10.16" y2="69.205" width="0" layer="20"/>
<wire x1="10.16" y1="69.205" x2="10.16" y2="15.24" width="0" layer="20"/>
<wire x1="10.16" y1="15.24" x2="15.24" y2="13.335" width="0" layer="20"/>
<wire x1="15.24" y1="13.335" x2="15.24" y2="11.43" width="0" layer="20"/>
<text>CrashSync</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="capacitors-film">
<description>&lt;b&gt;Capacitors, Ceramic&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;very small capacitances: 1 - 1000pF
&lt;/ul&gt;</description>
<packages>
<package name="BOX_SMALL">
</package>
</packages>
</library>
<library name="capacitors-elec">
<description>&lt;b&gt;Capacitors, Polar Electrolytic, Radial &lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;large value capacitors: .22 - 470uF (uF = µF = mF)
&lt;li&gt;often used in power supply filters
&lt;/ul&gt;</description>
<packages>
<package name="063_025">
<description>&lt;b&gt;6.3mm diameter, 2.5 mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
<package name="050_020_1">
<description>&lt;b&gt;5mm diameter, 2mm lead spacing, 0.1" pad spacing&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="integrated circuits">
<description>&lt;b&gt;Integrated Circuits&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;mostly op amps (e.g., 4558, TL072)&lt;/li&gt;
&lt;li&gt;also CD4049 (for Anderton's Tube Sound Fuzz, the Red Llama, ...)
&lt;li&gt;generally gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="potentiometers">
<packages>
<package name="PADS_SMALL">
<description>&lt;b&gt;Potentiometer&lt;/b&gt;
&lt;p&gt;3 terminals for circuit board for wires connecting to 3 lugs of pot off-board</description>
</package>
</packages>
</library>
<library name="resistors">
<description>&lt;b&gt;Resistors&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;6mm long -- the size of 1/4 watt resistors
&lt;li&gt; all resistor values have the same size package; you choose the value of resistance 
&lt;/ul&gt;</description>
<packages>
<package name="R0207/3">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
length: 6mm&lt;br&gt;
format: 0.1" (perfboard)&lt;br&gt;
spacing: 3 holes

&lt;p&gt;This length resistor applies to 1/4 watt metal film.</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL08">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diodes">
<description>&lt;b&gt;Diodes&lt;/b&gt;
&lt;ul&gt;
&lt;li&gt;Zener 1N47xx (as in protection for the MOSFET in the AMZ MOSFET Booster)
&lt;li&gt;rectifier 1N4001-1N4008 (for polarity reversal protection in power supply sections)
&lt;li&gt;clipping 1N914 (as in a TS808)
&lt;li&gt;LED (light emitting diode, 3mm and 5mm)
&lt;li&gt;mostly gathered from Eagle libraries
&lt;/ul&gt;</description>
<packages>
<package name="DO41-3">
<description>&lt;b&gt;DO-41 0.3" pad spacing&lt;/b&gt;</description>
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="FilthMunster">
<packages>
<package name="FM_LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+9V" library="wirepad" package="2,15/1,0" value=""/>
<element name="C1" library="capacitors-film" package="BOX_SMALL" value="10n"/>
<element name="C2" library="capacitors-elec" package="063_025" value="47u"/>
<element name="C4" library="capacitors-film" package="BOX_SMALL" value="1n"/>
<element name="G" library="wirepad" package="2,15/1,0" value=""/>
<element name="GN" library="wirepad" package="2,15/1,0" value=""/>
<element name="I" library="wirepad" package="2,15/1,0" value=""/>
<element name="IC1" library="integrated circuits" package="DIL08" value=""/>
<element name="LEVEL" library="potentiometers" package="PADS_SMALL" value="100kA"/>
<element name="O" library="wirepad" package="2,15/1,0" value=""/>
<element name="R1" library="resistors" package="R0207/3" value="150K"/>
<element name="R2" library="resistors" package="R0207/3" value="10M"/>
<element name="R3" library="resistors" package="R0207/3" value="56K"/>
<element name="R4" library="resistors" package="R0207/3" value="56K"/>
<element name="R5" library="resistors" package="R0207/3" value="1M"/>
<element name="R6" library="resistors" package="R0207/3" value="470K"/>
<element name="C5" library="capacitors-film" package="BOX_SMALL" value="330p"/>
<element name="R7" library="resistors" package="R0207/3" value="1K"/>
<element name="C7" library="capacitors-film" package="BOX_SMALL" value="47n"/>
<element name="R8" library="resistors" package="R0207/3" value="1M"/>
<element name="R9" library="resistors" package="R0207/3" value="56K"/>
<element name="R10" library="resistors" package="R0207/3" value="1M"/>
<element name="R11" library="resistors" package="R0207/3" value="10K"/>
<element name="R12" library="resistors" package="R0207/3" value="10K"/>
<element name="IC2" library="linear" package="DIL08" value="LM555N">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="resistors" package="R0207/3" value="2K2"/>
<element name="C8" library="capacitors-film" package="BOX_SMALL" value="47n"/>
<element name="DEPTH" library="potentiometers" package="PADS_SMALL" value="100kB"/>
<element name="R14" library="resistors" package="R0207/3" value="4K7"/>
<element name="R15" library="resistors" package="R0207/3" value="10K"/>
<element name="C10" library="capacitors-film" package="BOX_SMALL" value="10n"/>
<element name="R16" library="resistors" package="R0207/3" value="2K2"/>
<element name="C3" library="capacitors-elec" package="050_020_1" value="1u"/>
<element name="C6" library="capacitors-elec" package="050_020_1" value="10u"/>
<element name="C9" library="capacitors-elec" package="050_020_1" value="10u"/>
<element name="D1" library="diodes" package="DO41-3" value="1N5817"/>
<element name="LED" library="diodes" package="LED3MM" value="LED3MM"/>
<element name="L" library="wirepad" package="2,15/1,0" value=""/>
<element name="FM_LOGO1" library="FilthMunster" package="FM_LOGO" value="FM_LOGO"/>
</elements>
<signals>
<signal name="GND">
<contactref element="GN" pad="1"/>
<contactref element="G" pad="1"/>
<contactref element="C2" pad="-"/>
<contactref element="LEVEL" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="R13" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="-"/>
</signal>
<signal name="+9V">
<contactref element="C2" pad="+"/>
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="R8" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="R16" pad="2"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="LEVEL" pad="3"/>
<contactref element="C10" pad="2"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="C6" pad="+"/>
<contactref element="C9" pad="+"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="2"/>
<contactref element="C6" pad="-"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="6"/>
<contactref element="C7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="5"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="R10" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="IC2" pad="4"/>
<contactref element="R12" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="DEPTH" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="DEPTH" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="DEPTH" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="IC2" pad="3"/>
<contactref element="C3" pad="+"/>
</signal>
<signal name="N$14">
<contactref element="R15" pad="2"/>
<contactref element="C3" pad="-"/>
</signal>
<signal name="N$15">
<contactref element="+9V" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="R16" pad="1"/>
<contactref element="LED" pad="A"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="I" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="LEVEL" pad="2"/>
<contactref element="O" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="LED" pad="K"/>
<contactref element="L" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
