<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<wire x1="23.495" y1="49.403" x2="43.866" y2="49.403" width="0" layer="20"/>
<wire x1="43.866" y1="49.403" x2="43.866" y2="64.887" width="0" layer="20"/>
<wire x1="43.866" y1="64.887" x2="23.495" y2="64.887" width="0" layer="20"/>
<wire x1="23.495" y1="64.887" x2="23.495" y2="49.403" width="0" layer="20"/>
<text>GND</text>
<text>+</text>
<text>RXD</text>
<text>TXD</text>
<text>PPM</text>
<text>P/N</text>
<text>MOSI</text>
<text>MISO</text>
<text>SCK</text>
<text>RST</text>
<text>GND</text>
<text>VCC</text>
<text>C1</text>
<text>C2</text>
<text>Q1</text>
<text>R</text>
<text>D1</text>
<text>LED1</text>
<text>C3</text>
<text>+</text>
<text>yfetre@gmail.com</text>
<text>yfetre@gmail.com</text>
<text>Convertisseur MLINK-&gt;PPM</text>
<text>V1.0</text>
</plain>
<libraries>
<library name="crystal">
<packages>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<packages>
<package name="MLF32">
<description>&lt;b&gt;32M1-A&lt;/b&gt; Micro Lead Frame package (MLF)</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="PLCC2">
<description>&lt;b&gt;LC TOPLED®, Low Current LED,&lt;/b&gt;&lt;p&gt;
LS T679, LY T679, LG T679&lt;br&gt;
Source: http://catalog.osram-os.com .. LG_LS_LY_T679_OBS.pdf</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOD-323">
<description>&lt;b&gt;SOD323&lt;/b&gt; (2.5x1.2mm)</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP07R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
</packages>
</library>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q1" library="crystal" package="CTS406" value="7.3728M"/>
<element name="LED" library="led" package="PLCC2" value="">
<attribute name="COLOR" value="green"/>
</element>
<element name="R" library="rcl" package="M0805" value="470"/>
<element name="D1" library="adafruit" package="SOD-323" value=""/>
<element name="IC2" library="atmel" package="MLF32" value="MEGA8-MI">
<attribute name="OC_NEWARK" value="15R0272"/>
<attribute name="MPN" value="ATMEGA88PA-MU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1715491"/>
</element>
<element name="C1" library="rcl" package="C0805" value="22p"/>
<element name="C2" library="rcl" package="C0805" value="22p"/>
<element name="C3" library="rcl" package="C0805" value="100n"/>
<element name="TP1" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP2" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP3" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP4" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP5" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TP6" library="testpad" package="TP07R" value="TPSQTP07R">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="SJ1" library="SparkFun" package="SJ_2S" value="SOLDERJUMPERNC"/>
<element name="GND" library="wirepad" package="SMD1,27-2,54" value=""/>
<element name="+" library="wirepad" package="SMD1,27-2,54" value=""/>
<element name="BD" library="wirepad" package="SMD1,27-2,54" value=""/>
<element name="TX" library="wirepad" package="SMD1,27-2,54" value=""/>
<element name="PPM" library="wirepad" package="SMD1,27-2,54" value=""/>
<element name="PPM1" library="wirepad" package="SMD1,27-2,54" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="LED" pad="C"/>
<contactref element="IC2" pad="21"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="TP3" pad="TP"/>
<contactref element="SJ1" pad="2"/>
<contactref element="GND" pad="1"/>
</signal>
<signal name="+UB">
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="TP4" pad="TP"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="PPM">
<contactref element="IC2" pad="13"/>
<contactref element="PPM" pad="1"/>
</signal>
<signal name="XTAL1">
<contactref element="Q1" pad="3"/>
<contactref element="IC2" pad="7"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="Q1" pad="1"/>
<contactref element="IC2" pad="8"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="AVCC">
<contactref element="IC2" pad="18"/>
</signal>
<signal name="TXD">
<contactref element="IC2" pad="31"/>
<contactref element="TX" pad="1"/>
</signal>
<signal name="PC5">
<contactref element="IC2" pad="28"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="LED" pad="A"/>
<contactref element="R" pad="2"/>
</signal>
<signal name="PB0">
<contactref element="R" pad="1"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="MISO">
<contactref element="IC2" pad="16"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="MOSI">
<contactref element="IC2" pad="15"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="RST">
<contactref element="IC2" pad="29"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="SCK">
<contactref element="IC2" pad="17"/>
<contactref element="TP6" pad="TP"/>
</signal>
<signal name="RXD">
<contactref element="IC2" pad="30"/>
<contactref element="BD" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="+" pad="1"/>
<contactref element="PPM1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
