<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="80" x2="0" y2="71.12" width="0" layer="20"/>
<wire x1="0" y1="80.01" x2="15.875" y2="80.01" width="0.254" layer="20"/>
<wire x1="15.875" y1="80.01" x2="15.875" y2="71.12" width="0.254" layer="20"/>
<wire x1="15.875" y1="71.12" x2="0" y2="71.12" width="0.254" layer="20"/>
<wire x1="0" y1="71.12" x2="0" y2="80.01" width="0.254" layer="20"/>
<text>MOSI</text>
<text>RST</text>
<text>SCK</text>
<text>MISO</text>
<text>GND</text>
<text>5V</text>
<text>IMP</text>
<text>Ch1</text>
<text>Ch2</text>
<text>GND</text>
<text>//Moe
fpv-team.de</text>
<text>2CH RC
Switch </text>
<text>V0.1</text>
</plain>
<libraries>
<library name="wirepad">
<description>&lt;b&gt;Single Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMD1,27-2,54">
<description>&lt;b&gt;SMD PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="8S2">
<description>&lt;b&gt;8S2&lt;/b&gt; 8-lead, 0.208 Body&lt;p&gt;
Plastic Small Outline Package (EIAJ)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="transistor-fet">
<description>&lt;b&gt;Field Effect Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
Symbols changed according to IEC617&lt;p&gt; 
All types, packages and assignment to symbols and pins checked&lt;p&gt;
Package outlines partly checked&lt;p&gt;
&lt;p&gt;
JFET = junction FET&lt;p&gt;
IGBT-x = insulated gate bipolar transistor&lt;p&gt;
x=N: NPN; x=P: PNP&lt;p&gt;
IGFET-mc-nnn; (IGFET=insulated gate field effect transistor)&lt;P&gt;
m=D: depletion mode (Verdr&amp;auml;ngungstyp)&lt;p&gt;
m=E: enhancement mode (Anreicherungstyp)&lt;p&gt;
c: N=N-channel; P=P-Channel&lt;p&gt;
GDSB: gate, drain, source, bulk&lt;p&gt;
&lt;p&gt;
by R. Vogg  15.March.2002</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="+5V" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="GND0" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="atmel" package="8S2" value="TINY13-20SU">
<attribute name="OC_NEWARK" value="96K6522"/>
<attribute name="MPN" value="ATTINY13-20SU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9171568"/>
</element>
<element name="IMP" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="IN1" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="IN2" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="MISO" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="MOSI" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-fet" package="SOT23" value="SST5486"/>
<element name="Q2" library="transistor-fet" package="SOT23" value="SST5486"/>
<element name="RST" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
<element name="SCK" library="wirepad" package="SMD1,27-2,54" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="4"/>
<contactref element="GND" pad="1"/>
<contactref element="GND0" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="5"/>
<contactref element="IMP" pad="1"/>
<contactref element="MOSI" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="IC1" pad="8"/>
<contactref element="+5V" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="3"/>
<contactref element="IN1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="Q2" pad="3"/>
<contactref element="IN2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="3"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="RST" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="MISO" pad="1"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="SCK" pad="1"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$11">
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
