<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="82.22" y2="0" width="0" layer="20"/>
<wire x1="82.22" y1="0" x2="82.22" y2="63.49" width="0" layer="20"/>
<wire x1="82.22" y1="63.49" x2="0" y2="63.49" width="0" layer="20"/>
<wire x1="0" y1="63.49" x2="0" y2="0" width="0" layer="20"/>
<text>+</text>
<text>-</text>
<text>VCC</text>
<text>GND</text>
<text>BASS AMPLIFIER</text>
<text>CALEB ENGINEERING, LLC</text>
<text>Rev A</text>
<text>7-12-2014</text>
<text>12V</text>
<text>VOLUME</text>
<text>GAIN</text>
<text>SPEAKER</text>
</plain>
<libraries>
<library name="caleb-con-OST-termblock">
<packages>
<package name="EDZ350-2POS">
</package>
</packages>
</library>
<library name="caleb-passive">
<packages>
<package name="R0400TH">
</package>
<package name="C5X2">
</package>
<package name="CT6EP">
</package>
<package name="PTV09A">
</package>
<package name="CDX5">
</package>
<package name="AIUR-06">
</package>
<package name="E5-13">
</package>
</packages>
</library>
<library name="caleb-ic">
<packages>
<package name="DIL-8">
</package>
<package name="TO92">
</package>
<package name="DIL-20">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="caleb-con-OST-termblock" package="EDZ350-2POS" value="CON-EDZ350-2"/>
<element name="J2" library="caleb-con-OST-termblock" package="EDZ350-2POS" value="CON-EDZ350-2"/>
<element name="J3" library="caleb-con-OST-termblock" package="EDZ350-2POS" value="CON-EDZ350-2"/>
<element name="R1" library="caleb-passive" package="R0400TH" value="1M"/>
<element name="R2" library="caleb-passive" package="R0400TH" value="1M"/>
<element name="R3" library="caleb-passive" package="R0400TH" value="2.2k"/>
<element name="R4" library="caleb-passive" package="R0400TH" value="2.2k"/>
<element name="R5" library="caleb-passive" package="R0400TH" value="1k"/>
<element name="R6" library="caleb-passive" package="R0400TH" value="22k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="caleb-passive" package="R0400TH" value="47k"/>
<element name="R8" library="caleb-passive" package="R0400TH" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="caleb-passive" package="R0400TH" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="caleb-passive" package="R0400TH" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="caleb-passive" package="R0400TH" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="caleb-passive" package="C5X2" value="10u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C2" library="caleb-passive" package="C5X2" value="10u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C3" library="caleb-passive" package="C5X2" value="10u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C4" library="caleb-passive" package="C5X2" value="10u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U1" library="caleb-ic" package="DIL-8" value="LM833"/>
<element name="Q1" library="caleb-ic" package="TO92" value="2N7000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="caleb-passive" package="CT6EP" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="caleb-passive" package="C5X2" value="100u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R13" library="caleb-passive" package="PTV09A" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="caleb-passive" package="C5X2" value="10u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U2" library="caleb-ic" package="TO92" value="78L10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="caleb-passive" package="CDX5" value="100p">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="caleb-passive" package="CDX5" value="0.22u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C10" library="caleb-passive" package="CDX5" value="1u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C11" library="caleb-passive" package="CDX5" value="1u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U3" library="caleb-ic" package="DIL-20" value="TPA3125">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="caleb-passive" package="AIUR-06" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="caleb-passive" package="AIUR-06" value="22u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="caleb-passive" package="E5-13" value="470u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="caleb-passive" package="E5-13" value="470u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="caleb-passive" package="CDX5" value="1u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C15" library="caleb-passive" package="CDX5" value="1u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C16" library="caleb-passive" package="CDX5" value="0.22u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C17" library="caleb-passive" package="CDX5" value="0.22u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C18" library="caleb-passive" package="CDX5" value="0.22u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C19" library="caleb-passive" package="CDX5" value="0.22u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C20" library="caleb-passive" package="CDX5" value="0.22u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C21" library="caleb-passive" package="C5X2" value="10u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C8" library="caleb-passive" package="CDX5" value="1u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C22" library="caleb-passive" package="CDX5" value="1u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C23" library="caleb-passive" package="CDX5" value="1000p">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C24" library="caleb-passive" package="CDX5" value="1000p">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R14" library="caleb-passive" package="R0400TH" value="3.3"/>
<element name="R15" library="caleb-passive" package="R0400TH" value="3.3"/>
<element name="C25" library="caleb-passive" package="CDX5" value="10000p">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C26" library="caleb-passive" package="CDX5" value="10000p">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C27" library="caleb-passive" package="CDX5" value="100p">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C28" library="caleb-passive" package="C5X2" value="10u">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R16" library="caleb-passive" package="R0400TH" value="47k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="POS"/>
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="C5" pad="NEG"/>
<contactref element="J2" pad="P$2"/>
<contactref element="R13" pad="T1"/>
<contactref element="R13" pad="T2"/>
<contactref element="R13" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="R11" pad="1"/>
<contactref element="C2" pad="NEG"/>
<contactref element="U2" pad="2"/>
<contactref element="C1" pad="NEG"/>
<contactref element="J1" pad="P$2"/>
<contactref element="C7" pad="P$2"/>
<contactref element="C9" pad="P$2"/>
<contactref element="U3" pad="8"/>
<contactref element="C14" pad="P$1"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="14"/>
<contactref element="C15" pad="P$2"/>
<contactref element="C20" pad="P$2"/>
<contactref element="C19" pad="P$2"/>
<contactref element="C18" pad="P$2"/>
<contactref element="C13" pad="-"/>
<contactref element="C12" pad="-"/>
<contactref element="C21" pad="NEG"/>
<contactref element="U3" pad="3"/>
<contactref element="C8" pad="P$1"/>
<contactref element="C22" pad="P$1"/>
<contactref element="C23" pad="P$1"/>
<contactref element="C24" pad="P$1"/>
<contactref element="C27" pad="P$1"/>
<contactref element="C26" pad="P$1"/>
<contactref element="U3" pad="11"/>
<contactref element="U3" pad="20"/>
<contactref element="C28" pad="NEG"/>
<contactref element="C25" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="Q1" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="C4" pad="POS"/>
</signal>
<signal name="N$7">
<contactref element="R4" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="R12" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="R12" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="1"/>
<contactref element="C5" pad="POS"/>
</signal>
<signal name="N$11">
<contactref element="C4" pad="NEG"/>
<contactref element="R13" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R13" pad="2"/>
<contactref element="C6" pad="NEG"/>
<contactref element="C27" pad="P$2"/>
</signal>
<signal name="N$13">
<contactref element="C6" pad="POS"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R6" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="NINV">
<contactref element="R7" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C10" pad="P$1"/>
</signal>
<signal name="N$17">
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="INV">
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="C11" pad="P$1"/>
</signal>
<signal name="VREF">
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="C2" pad="POS"/>
<contactref element="R11" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="10V">
<contactref element="R10" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="1"/>
<contactref element="C9" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="POS"/>
<contactref element="U2" pad="3"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="10"/>
<contactref element="J1" pad="P$1"/>
<contactref element="C20" pad="P$1"/>
<contactref element="C19" pad="P$1"/>
<contactref element="C18" pad="P$1"/>
<contactref element="C13" pad="+"/>
<contactref element="C12" pad="+"/>
<contactref element="U3" pad="16"/>
<contactref element="U3" pad="17"/>
<contactref element="C21" pad="POS"/>
<contactref element="U3" pad="15"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="INPUT">
<contactref element="J2" pad="P$1"/>
<contactref element="C3" pad="NEG"/>
<contactref element="C7" pad="P$1"/>
</signal>
<signal name="SPKR+">
<contactref element="J3" pad="P$1"/>
<contactref element="L2" pad="P$2"/>
<contactref element="C8" pad="P$2"/>
<contactref element="C24" pad="P$2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="SPKR-">
<contactref element="J3" pad="P$2"/>
<contactref element="L1" pad="P$2"/>
<contactref element="C22" pad="P$2"/>
<contactref element="C23" pad="P$2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="U3" pad="5"/>
<contactref element="C11" pad="P$2"/>
</signal>
<signal name="N$18">
<contactref element="U3" pad="4"/>
<contactref element="C10" pad="P$2"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="12"/>
<contactref element="L2" pad="P$1"/>
<contactref element="C17" pad="P$2"/>
</signal>
<signal name="N$20">
<contactref element="C14" pad="P$2"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="C15" pad="P$1"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="N$19">
<contactref element="C17" pad="P$1"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="N$21">
<contactref element="C16" pad="P$1"/>
<contactref element="U3" pad="18"/>
</signal>
<signal name="N$10">
<contactref element="L1" pad="P$1"/>
<contactref element="U3" pad="19"/>
<contactref element="C16" pad="P$2"/>
</signal>
<signal name="N$24">
<contactref element="C26" pad="P$2"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="C25" pad="P$2"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R16" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C28" pad="POS"/>
</signal>
<signal name="N$23">
</signal>
</signals>
</board>
</drawing>
</eagle>
