<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="103.104" y2="0" width="0" layer="20"/>
<wire x1="103.104" y1="0" x2="103.104" y2="46.66" width="0" layer="20"/>
<wire x1="103.104" y1="46.66" x2="0" y2="46.66" width="0" layer="20"/>
<wire x1="0" y1="46.66" x2="0" y2="0" width="0" layer="20"/>
<text>3G Module Prototype Board v1
Wickerbox Electronics
http://wickerbox.net/</text>
</plain>
<libraries>
<library name="SmartPrj">
<packages>
<package name="CALVUS_5BAND_SMD_A10340_0MM_EXCLUSION">
</package>
</packages>
</library>
<library name="v1-cellphone">
<description>Generated from &lt;b&gt;v1-cellphone.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="CON-COAX_BU-SMA-V">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
</package>
<package name="SMARTPRJ_CON-AMPHENOL_C707_10M006_512_2">
<description>&lt;b&gt;C707A SIMLOCK® 2.5 mm with wide solder tails&lt;/b&gt;&lt;p&gt;
Source: &lt;a href= "http://www.amphenol.info/downloads/C707_10M006_512_2.pdf"&gt;Data sheet&lt;/a&gt;</description>
</package>
<package name="AVR-5_TQFP44">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
<package name="SPARKFUN_SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="CELLPHONE_B3U-1000P">
<description>Omron B3U-1000P (Digi-Key #SW1020CT-ND)</description>
</package>
<package name="GSM_UC15_WITHOUT_EXCLUSION">
</package>
<package name="SPARKFUN-CONNECTORS_2X3-NS">
</package>
<package name="CELLPHONE_SPEAKER-6.4MM">
<description>Knowles Mini-Siren Speaker (SR6438NWS-000)
Digi-Key #423-1142-ND</description>
</package>
</packages>
</library>
<library name="rcl_custom">
<packages>
<package name="C1210K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 1210 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 3225</description>
</package>
<package name="0603-B">
<description>&lt;b&gt;0603 (metric 1608) normal 'IPC-B'&lt;/b&gt;
&lt;br&gt;In house package for nominal spacing based on IPC-7351A. Cross-checked against other packages.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-1000UF-25V">
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="2-SMD-5X3MM">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
<package name="9.7ELECTRET">
</package>
</packages>
</library>
<library name="con-hirose-microusb">
<packages>
<package name="ZX62D-B-5P8">
</package>
</packages>
</library>
<library name="testpad">
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TSSOP14">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 14&lt;/b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="max-viz">
<description>&lt;b&gt;PCB Libraries Packages&lt;/b&gt;&lt;p&gt;
\</description>
<packages>
<package name="SOT-23">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ANT1" library="SmartPrj" package="CALVUS_5BAND_SMD_A10340_0MM_EXCLUSION" value="CALVUS_5BAND_SMD_A103400MM_EXCLUSION">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="v1-cellphone" package="CON-COAX_BU-SMA-V" value="SMA">
<attribute name="PN" value="5-1814832-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="rcl_custom" package="0603-B" value="3.3nH 500mA 0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="v1-cellphone" package="SMARTPRJ_CON-AMPHENOL_C707_10M006_512_2" value="CCM03-3002 R102">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1463072 "/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl_custom" package="0603-B" value="3.9pF 100V 0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl_custom" package="0603-B" value="6.8nH 430mA 0603">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl_custom" package="0603-B" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl_custom" package="0603-B" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl_custom" package="0603-B" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="v1-cellphone" package="AVR-5_TQFP44" value="MEGA1284">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl_custom" package="0603-B" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="JST-2-SMD" value="BATTERY INPUT">
<attribute name="PROD_ID" value="CONN-08352"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="v1-cellphone" package="SPARKFUN_SOT23-5" value="MCP73831">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl_custom" package="0603-B" value="4.7uF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl_custom" package="0603-B" value="4.7uF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="CPOL-RADIAL-1000UF-25V" value="1mF 50V">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C13" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="fab" package="2-SMD-5X3MM" value="8MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="v1-cellphone" package="CELLPHONE_B3U-1000P" value="BUTTON">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0603" value="5V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIP-LED0603" value="3GSTAT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl_custom" package="0603-B" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X06_LOCK" value="FTDI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIP-LED0603" value="VBAT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl_custom" package="0603-B" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIP-LED0603" value="DEBUG">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl_custom" package="0603-B" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl_custom" package="0603-B" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl_custom" package="0603-B" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="con-hirose-microusb" package="ZX62D-B-5P8" value="ZX62D-B-5P8">
<attribute name="NAME"/>
</element>
<element name="U3" library="v1-cellphone" package="GSM_UC15_WITHOUT_EXCLUSION" value="GSM_UC15">
<attribute name="NAME"/>
</element>
<element name="LED5" library="adafruit" package="CHIP-LED0603" value="NETLIGHT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl_custom" package="0603-B" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl_custom" package="0603-B" value="33pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl_custom" package="0603-B" value="33pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl_custom" package="0603-B" value="33pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="v1-cellphone" package="SPARKFUN-CONNECTORS_2X3-NS" value="AVRISP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl_custom" package="0603-B" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl_custom" package="0603-B" value="18pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl_custom" package="0603-B" value="10pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl_custom" package="0603-B" value="33pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl_custom" package="0603-B" value="10pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl_custom" package="C1210K" value="100uF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="9.7ELECTRET" value="MIC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl_custom" package="0603-B" value="33pF  16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl_custom" package="0603-B" value="33pF  16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl_custom" package="0603-B" value="33pF  16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl_custom" package="0603-B" value="10pF  10V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl_custom" package="0603-B" value="10pF  16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="rcl_custom" package="0603-B" value="10pF  16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl_custom" package="0603-B" value="33pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl_custom" package="0603-B" value="33pF 10V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl_custom" package="0603-B" value="33pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="rcl_custom" package="0603-B" value="10pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="rcl_custom" package="0603-B" value="10pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="rcl_custom" package="0603-B" value="10pF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl_custom" package="0603-B" value="0 ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="rcl_custom" package="0603-B" value="4.7uF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP11" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP12" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP14" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP15" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="SparkFun-DigitalIC" package="TSSOP14" value="TXB0104PWR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="max-viz" package="SOT-23" value="NTR4501N-D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="max-viz" package="SOT-23" value="NTR4501N-D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl_custom" package="0603-B" value="4.99K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl_custom" package="0603-B" value="4.99K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl_custom" package="0603-B" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="rcl_custom" package="0603-B" value="10nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl_custom" package="0603-B" value="100nF 16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SP1" library="v1-cellphone" package="CELLPHONE_SPEAKER-6.4MM" value="SPEAKER">
<attribute name="NAME"/>
</element>
<element name="TP13" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="P5"/>
<contactref element="C5" pad="1"/>
<contactref element="J5" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="J1" pad="6"/>
<contactref element="C10" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="29"/>
<contactref element="U2" pad="28"/>
<contactref element="U2" pad="39"/>
<contactref element="U2" pad="18"/>
<contactref element="C12" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="J4" pad="6"/>
<contactref element="J4" pad="5"/>
<contactref element="S1" pad="P$1"/>
<contactref element="C40" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="U3" pad="8"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="X3" pad="C5"/>
<contactref element="C2" pad="2"/>
<contactref element="C26" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="U3" pad="42"/>
<contactref element="U3" pad="44"/>
<contactref element="U3" pad="45"/>
<contactref element="U3" pad="46"/>
<contactref element="U3" pad="47"/>
<contactref element="U3" pad="48"/>
<contactref element="U3" pad="49"/>
<contactref element="U3" pad="65"/>
<contactref element="U3" pad="67"/>
<contactref element="U3" pad="68"/>
<contactref element="U3" pad="81"/>
<contactref element="U3" pad="82"/>
<contactref element="U3" pad="83"/>
<contactref element="U3" pad="84"/>
<contactref element="U3" pad="85"/>
<contactref element="U3" pad="86"/>
<contactref element="U3" pad="87"/>
<contactref element="U3" pad="88"/>
<contactref element="U3" pad="89"/>
<contactref element="U3" pad="90"/>
<contactref element="U3" pad="91"/>
<contactref element="U3" pad="92"/>
<contactref element="U3" pad="93"/>
<contactref element="U3" pad="94"/>
<contactref element="U3" pad="95"/>
<contactref element="U3" pad="96"/>
<contactref element="U3" pad="97"/>
<contactref element="U3" pad="98"/>
<contactref element="U3" pad="99"/>
<contactref element="U3" pad="100"/>
<contactref element="U3" pad="101"/>
<contactref element="U3" pad="102"/>
<contactref element="U3" pad="103"/>
<contactref element="U3" pad="104"/>
<contactref element="U3" pad="105"/>
<contactref element="U3" pad="106"/>
<contactref element="U3" pad="107"/>
<contactref element="U3" pad="108"/>
<contactref element="R14" pad="2"/>
<contactref element="U4" pad="7"/>
<contactref element="Q2" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="C41" pad="2"/>
</signal>
<signal name="PROG">
<contactref element="U1" pad="5"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED3" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="SHLD">
<contactref element="J2" pad="P$1"/>
<contactref element="J2" pad="P$2"/>
<contactref element="J2" pad="P$3"/>
<contactref element="J2" pad="P$4"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="LED1" pad="C"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="5V">
<contactref element="C3" pad="1"/>
<contactref element="LED1" pad="A"/>
<contactref element="U1" pad="4"/>
<contactref element="J2" pad="P1"/>
<contactref element="J1" pad="2"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="VBAT">
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="C13" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="LED3" pad="A"/>
<contactref element="J5" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="U2" pad="17"/>
<contactref element="U2" pad="38"/>
<contactref element="U2" pad="27"/>
<contactref element="C12" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="C23" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="U3" pad="52"/>
<contactref element="U3" pad="53"/>
<contactref element="C21" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="U3" pad="50"/>
<contactref element="U3" pad="51"/>
<contactref element="U4" pad="14"/>
<contactref element="C41" pad="1"/>
</signal>
<signal name="BATTSTATUS">
<contactref element="U1" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="UC15STATUS">
<contactref element="LED2" pad="A"/>
<contactref element="U2" pad="16"/>
<contactref element="U4" pad="10"/>
</signal>
<signal name="SCK">
<contactref element="U2" pad="3"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U2" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="!RESET">
<contactref element="J1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="S1" pad="P$2"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="RXD0">
<contactref element="U2" pad="9"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="TXD0">
<contactref element="J4" pad="2"/>
<contactref element="U2" pad="10"/>
</signal>
<signal name="RXD1">
<contactref element="U2" pad="11"/>
<contactref element="TP15" pad="TP"/>
<contactref element="U4" pad="13"/>
</signal>
<signal name="TXD1">
<contactref element="U2" pad="12"/>
<contactref element="TP14" pad="TP"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="PA0">
<contactref element="U2" pad="37"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="PA1">
<contactref element="U2" pad="36"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="PA2">
<contactref element="U2" pad="35"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="PA3">
<contactref element="U2" pad="34"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="PA5">
<contactref element="U2" pad="32"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="PA7">
<contactref element="U2" pad="30"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="PA4">
<contactref element="U2" pad="33"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="PA6">
<contactref element="U2" pad="31"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="N$37">
<contactref element="LED2" pad="C"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="PB0">
<contactref element="U2" pad="40"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="PB1">
<contactref element="U2" pad="41"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="PB2">
<contactref element="U2" pad="42"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="PB3">
<contactref element="U2" pad="43"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="DEBUGLED">
<contactref element="U2" pad="44"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="LED4" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="C10" pad="1"/>
<contactref element="X2" pad="P$1"/>
<contactref element="U2" pad="7"/>
</signal>
<signal name="XTAL1">
<contactref element="X2" pad="P$2"/>
<contactref element="C14" pad="1"/>
<contactref element="U2" pad="8"/>
</signal>
<signal name="SETPWRKEY">
<contactref element="U2" pad="13"/>
<contactref element="TP12" pad="TP"/>
<contactref element="Q2" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="SETUC15RESET">
<contactref element="U2" pad="14"/>
<contactref element="TP11" pad="TP"/>
<contactref element="Q3" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="ANT">
<contactref element="C8" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="U3" pad="43"/>
</signal>
<signal name="SIM_VDD">
<contactref element="X3" pad="C1"/>
<contactref element="U3" pad="12"/>
<contactref element="TP6" pad="TP"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="SIM_DATA">
<contactref element="X3" pad="C7"/>
<contactref element="R3" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="TP9" pad="TP"/>
</signal>
<signal name="SIM_CLK">
<contactref element="R2" pad="1"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="SIM_RST">
<contactref element="R6" pad="1"/>
<contactref element="U3" pad="15"/>
</signal>
<signal name="SPK1P">
<contactref element="C36" pad="2"/>
<contactref element="C37" pad="1"/>
<contactref element="C33" pad="2"/>
<contactref element="C34" pad="1"/>
<contactref element="U3" pad="22"/>
<contactref element="SP1" pad="POS"/>
</signal>
<signal name="SIM_RSTR">
<contactref element="X3" pad="C2"/>
<contactref element="R6" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="SIM_CLKR">
<contactref element="X3" pad="C3"/>
<contactref element="R2" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="ANTENNA">
<contactref element="X1" pad="1"/>
<contactref element="ANT1" pad="FEED"/>
<contactref element="C8" pad="2"/>
<contactref element="L2" pad="2"/>
</signal>
<signal name="NETLIGHT">
<contactref element="LED5" pad="A"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="N$6">
<contactref element="LED5" pad="C"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="5"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="3"/>
<contactref element="L2" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C36" pad="1"/>
<contactref element="C33" pad="1"/>
<contactref element="C35" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="U3" pad="19"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U3" pad="13"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U3" pad="2"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="VDD_EXT">
<contactref element="U3" pad="7"/>
<contactref element="C39" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U3" pad="55"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="MIC1P">
<contactref element="C28" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="Q1" pad="+"/>
<contactref element="C31" pad="1"/>
<contactref element="C30" pad="2"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="MIC1N">
<contactref element="C28" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="Q1" pad="-"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="1"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="SPK1N">
<contactref element="U3" pad="21"/>
<contactref element="C37" pad="2"/>
<contactref element="C38" pad="1"/>
<contactref element="C34" pad="2"/>
<contactref element="C35" pad="1"/>
<contactref element="SP1" pad="NEG"/>
</signal>
<signal name="!UC15RESET">
<contactref element="U3" pad="17"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="PRESENCE">
<contactref element="U3" pad="11"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="N$20">
<contactref element="U3" pad="60"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U3" pad="61"/>
<contactref element="U4" pad="3"/>
</signal>
<signal name="N$23">
<contactref element="U3" pad="54"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="!PWRKEY">
<contactref element="Q2" pad="3"/>
<contactref element="U3" pad="18"/>
</signal>
<signal name="OE">
<contactref element="U4" pad="8"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="X3" pad="C6"/>
<contactref element="TP13" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
