<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="69.85" y1="0" x2="69.85" y2="10.668" width="0" layer="20"/>
<wire x1="69.85" y1="10.668" x2="0" y2="10.668" width="0" layer="20"/>
<wire x1="0" y1="10.668" x2="0.01" y2="0" width="0" layer="20"/>
<wire x1="0.01" y1="0" x2="69.85" y2="0" width="0" layer="20"/>
<text>Pixel Controller v1.5</text>
<text>Burdett 2013</text>
<hole x="2.54" y="5.334" drill="3.175"/>
<hole x="57.785" y="5.461" drill="3.175"/>
<text>GND</text>
<text>RAW</text>
<text>B. GND</text>
<text>CO</text>
<text>DO</text>
<text>VCC</text>
<text>RX</text>
<text>TX</text>
<text>DTR</text>
<text>VREG</text>
<text>Drain1</text>
<text>DIO-7</text>
<text>DIO-8</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>RX</text>
<text>TX</text>
<text>DTR</text>
<text>DO</text>
<text>CO</text>
<text>RAW</text>
<text>Drain1</text>
<text>A2</text>
<text>A2</text>
<text>MISO</text>
<text>RESET</text>
<text>RESET</text>
<text>MISO</text>
<text>B.GND</text>
<text>DIO-7</text>
<text>DIO-8</text>
<text>Pixel Controller v1.5</text>
<text>Burdett 2013</text>
<text>RAW</text>
<text>RAW</text>
<text>Drain2</text>
<text>Drain2</text>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="EIA3216">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="1X06">
</package>
<package name="SOT23-3">
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X01@1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="johns">
<packages>
<package name="BARRELJACK3.5">
<description>3.5mm outer diameter DC barrel jack</description>
</package>
</packages>
</library>
<library name="John">
<packages>
<package name="8-SOIC">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JOYSTICK_MINI_NO_DRILL">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C10" library="SparkFun" package="C0402" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C13" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun" package="C0402" value="10K">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun" package="C0402" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun" package="C0402" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C19" library="SparkFun" package="EIA3216" value="10uF">
<attribute name="NAME"/>
</element>
<element name="U1" library="SparkFun" package="TQFP32-08" value="ATMEGA328#"/>
<element name="FTDI" library="SparkFun" package="1X06" value="FTDI"/>
<element name="C2" library="SparkFun" package="C0402" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun" package="C0402" value="10K">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun" package="C0402" value="10K">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun" package="C0402" value="10K">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Electromechanical" package="JOYSTICK_MINI_NO_DRILL" value=""/>
<element name="R5" library="SparkFun" package="C0402" value="10K">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun" package="C0402" value="10K">
<attribute name="NAME"/>
</element>
<element name="U$1" library="johns" package="BARRELJACK3.5" value="POWERJACK3.5MM_OD"/>
<element name="C4" library="SparkFun" package="C0402" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun" package="C0402" value="22uF">
<attribute name="NAME"/>
</element>
<element name="U$3" library="SparkFun" package="SOT23-3" value="VREG_LDO_JOHN"/>
<element name="U$4" library="John" package="8-SOIC" value="FDS6910FDS6910"/>
<element name="JP5" library="pinhead" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="JP4" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="pinhead" package="1X01" value="">
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
<element name="Y1" library="SparkFun" package="CRYSTAL-SMD-5X3" value="16MHz"/>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="PWR">
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun" package="C0402" value="330">
<attribute name="NAME"/>
</element>
<element name="JP9" library="pinhead" package="1X01@1" value="">
<attribute name="VALUE"/>
</element>
<element name="JP11" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C13" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C19" pad="C"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="21"/>
<contactref element="FTDI" pad="5"/>
<contactref element="FTDI" pad="6"/>
<contactref element="JP2" pad="GND"/>
<contactref element="U$1" pad="P3"/>
<contactref element="U$3" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="AREF">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="15"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="TXO">
<contactref element="U1" pad="31"/>
<contactref element="FTDI" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="A"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="FTDI" pad="4"/>
<contactref element="U$3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="RAW">
<contactref element="C19" pad="A"/>
<contactref element="U$1" pad="P1"/>
<contactref element="U$3" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP9" pad="1"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="13"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="12"/>
<contactref element="JP6" pad="1"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="26"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="25"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="24"/>
</signal>
<signal name="A0">
<contactref element="U1" pad="23"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="JP2" pad="B"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="A"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
<contactref element="JP2" pad="CTR"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
<contactref element="JP2" pad="D"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
<contactref element="JP2" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="14"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="DTR">
<contactref element="FTDI" pad="1"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="RXI">
<contactref element="FTDI" pad="3"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="BATT_GND">
<contactref element="U$1" pad="P2"/>
<contactref element="U$4" pad="3"/>
<contactref element="U$4" pad="1"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="3"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="DRAIN2">
<contactref element="U$4" pad="7"/>
<contactref element="U$4" pad="8"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="DRAIN1">
<contactref element="U$4" pad="6"/>
<contactref element="U$4" pad="5"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="LED1" pad="C"/>
<contactref element="R8" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
