<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="85.395" y2="0" width="0" layer="20"/>
<wire x1="85.395" y1="0" x2="85.395" y2="48.25" width="0" layer="20"/>
<wire x1="85.395" y1="48.25" x2="0" y2="48.25" width="0" layer="20"/>
<wire x1="0" y1="48.25" x2="0" y2="0" width="0" layer="20"/>
<hole x="4.445" y="4.445" drill="1.5"/>
<hole x="81.28" y="4.445" drill="1.5"/>
<hole x="81.28" y="40.64" drill="1.5"/>
<text>TRIPLE-ETHERNET</text>
<text>(C) 2014 JOSH STONE</text>
<text>V1</text>
<text>PWR</text>
<text>CS0</text>
<text>CS1</text>
<text>CS2</text>
<text>INT0</text>
<text>INT1</text>
<text>INT2</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>+</text>
<hole x="64.135" y="44.7675" drill="1.5"/>
<hole x="42.8625" y="44.45" drill="1.5"/>
<hole x="19.685" y="44.45" drill="1.5"/>
</plain>
<libraries>
<library name="josh">
<packages>
<package name="TQFP-44">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="1X03-CLEANBIG">
</package>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MAGJACK">
</package>
<package name="1X12_NO_SILK">
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TSSOP8">
<description>&lt;b&gt;Plastic Small Outline&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="josh" package="TQFP-44" value="ENC424J600">
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0603" value="10 uF">
<attribute name="NAME"/>
</element>
<element name="R6" library="adafruit" package="R0603" value="12.4 k">
<attribute name="NAME"/>
</element>
<element name="R51" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R53" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C51" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C52" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="C53" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="R52" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R54" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R55" library="adafruit" package="R0603" value="10">
<attribute name="NAME"/>
</element>
<element name="C54" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="MAGJACK" value="MAGJACK"/>
<element name="R56" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="R57" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X12_NO_SILK" value="M12NO_SILK"/>
<element name="JP1" library="SparkFun-Connectors" package="1X12_NO_SILK" value="M12NO_SILK"/>
<element name="C10" library="adafruit" package="C0603" value="1 uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="adafruit" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
<element name="U$2" library="josh" package="TQFP-44" value="ENC424J600">
<attribute name="VALUE"/>
</element>
<element name="C11" library="adafruit" package="C0603" value="10 uF">
<attribute name="NAME"/>
</element>
<element name="R11" library="adafruit" package="R0603" value="12.4 k">
<attribute name="NAME"/>
</element>
<element name="R61" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R63" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C61" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C62" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="C63" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="R62" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R64" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R65" library="adafruit" package="R0603" value="10">
<attribute name="NAME"/>
</element>
<element name="C64" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="MAGJACK" value="MAGJACK"/>
<element name="R66" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="R67" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="U$3" library="josh" package="TQFP-44" value="ENC424J600">
<attribute name="VALUE"/>
</element>
<element name="C18" library="adafruit" package="C0603" value="10 uF">
<attribute name="NAME"/>
</element>
<element name="R20" library="adafruit" package="R0603" value="12.4 k">
<attribute name="NAME"/>
</element>
<element name="R71" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R73" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C71" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C72" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="C73" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="R72" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R74" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R75" library="adafruit" package="R0603" value="10">
<attribute name="NAME"/>
</element>
<element name="C74" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="MAGJACK" value="MAGJACK"/>
<element name="R76" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="R77" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="VALUE"/>
</element>
<element name="R28" library="adafruit" package="R0603" value="600">
<attribute name="NAME"/>
</element>
<element name="INT0" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="INT1" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="INT2" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="texas" package="TSSOP8" value="CDCS502">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="adafruit" package="HC49/S" value="25 mHz">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="INT3" library="adafruit" package="1X03-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="adafruit" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="adafruit" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="adafruit" package="C0603" value="1 nF">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="100">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="P$1"/>
<contactref element="C3" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U$1" pad="P$13"/>
<contactref element="U$1" pad="P$14"/>
<contactref element="U$1" pad="P$19"/>
<contactref element="U$1" pad="P$22"/>
<contactref element="C54" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="J1" pad="12"/>
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="M2"/>
<contactref element="J1" pad="M1"/>
<contactref element="U$1" pad="P$33"/>
<contactref element="U$1" pad="P$42"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="C11" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="U$2" pad="P$13"/>
<contactref element="U$2" pad="P$14"/>
<contactref element="U$2" pad="P$19"/>
<contactref element="U$2" pad="P$22"/>
<contactref element="C64" pad="2"/>
<contactref element="C61" pad="2"/>
<contactref element="J2" pad="12"/>
<contactref element="J2" pad="10"/>
<contactref element="J2" pad="M2"/>
<contactref element="J2" pad="M1"/>
<contactref element="U$2" pad="P$33"/>
<contactref element="U$2" pad="P$42"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="C18" pad="2"/>
<contactref element="R20" pad="1"/>
<contactref element="U$3" pad="P$13"/>
<contactref element="U$3" pad="P$14"/>
<contactref element="U$3" pad="P$19"/>
<contactref element="U$3" pad="P$22"/>
<contactref element="C74" pad="2"/>
<contactref element="C71" pad="2"/>
<contactref element="J3" pad="12"/>
<contactref element="J3" pad="10"/>
<contactref element="J3" pad="M2"/>
<contactref element="J3" pad="M1"/>
<contactref element="U$3" pad="P$33"/>
<contactref element="U$3" pad="P$42"/>
<contactref element="R28" pad="1"/>
<contactref element="INT0" pad="3"/>
<contactref element="INT1" pad="3"/>
<contactref element="INT2" pad="3"/>
<contactref element="U$1" pad="P$32"/>
<contactref element="U$2" pad="P$32"/>
<contactref element="U$3" pad="P$32"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="U$1" pad="P$12"/>
<contactref element="U$1" pad="P$15"/>
<contactref element="U$1" pad="P$18"/>
<contactref element="R52" pad="2"/>
<contactref element="R54" pad="2"/>
<contactref element="R55" pad="2"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$44"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U$2" pad="P$12"/>
<contactref element="U$2" pad="P$15"/>
<contactref element="U$2" pad="P$18"/>
<contactref element="R62" pad="2"/>
<contactref element="R64" pad="2"/>
<contactref element="R65" pad="2"/>
<contactref element="U$2" pad="P$4"/>
<contactref element="U$2" pad="P$44"/>
<contactref element="U$3" pad="P$12"/>
<contactref element="U$3" pad="P$15"/>
<contactref element="U$3" pad="P$18"/>
<contactref element="R72" pad="2"/>
<contactref element="R74" pad="2"/>
<contactref element="R75" pad="2"/>
<contactref element="U$3" pad="P$4"/>
<contactref element="U$3" pad="P$44"/>
<contactref element="LED1" pad="A"/>
<contactref element="INT0" pad="1"/>
<contactref element="INT1" pad="1"/>
<contactref element="INT2" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="JP2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$16"/>
<contactref element="R51" pad="2"/>
<contactref element="C53" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$17"/>
<contactref element="R53" pad="2"/>
<contactref element="C52" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R51" pad="1"/>
<contactref element="C51" pad="1"/>
<contactref element="R53" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$21"/>
<contactref element="R52" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="P$20"/>
<contactref element="R54" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R55" pad="1"/>
<contactref element="C54" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="C52" pad="2"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="C53" pad="2"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="11"/>
<contactref element="R56" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="J1" pad="9"/>
<contactref element="R57" pad="2"/>
</signal>
<signal name="AD7">
<contactref element="U$1" pad="P$8"/>
<contactref element="U$2" pad="P$8"/>
<contactref element="U$3" pad="P$8"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="AD6">
<contactref element="U$1" pad="P$7"/>
<contactref element="U$2" pad="P$7"/>
<contactref element="U$3" pad="P$7"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="AD5">
<contactref element="U$1" pad="P$6"/>
<contactref element="U$2" pad="P$6"/>
<contactref element="U$3" pad="P$6"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="AD4">
<contactref element="U$1" pad="P$5"/>
<contactref element="U$2" pad="P$5"/>
<contactref element="U$3" pad="P$5"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="AD3">
<contactref element="U$1" pad="P$41"/>
<contactref element="U$2" pad="P$41"/>
<contactref element="U$3" pad="P$41"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="AD2">
<contactref element="U$1" pad="P$40"/>
<contactref element="U$2" pad="P$40"/>
<contactref element="U$3" pad="P$40"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="AD1">
<contactref element="JP2" pad="7"/>
<contactref element="U$1" pad="P$39"/>
<contactref element="U$2" pad="P$39"/>
<contactref element="U$3" pad="P$39"/>
</signal>
<signal name="AD0">
<contactref element="U$1" pad="P$38"/>
<contactref element="U$2" pad="P$38"/>
<contactref element="U$3" pad="P$38"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="SI/RD/RW">
<contactref element="U$1" pad="P$36"/>
<contactref element="U$2" pad="P$36"/>
<contactref element="U$3" pad="P$36"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="AD8">
<contactref element="U$1" pad="P$25"/>
<contactref element="U$2" pad="P$25"/>
<contactref element="U$3" pad="P$25"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="AD9">
<contactref element="U$1" pad="P$26"/>
<contactref element="U$2" pad="P$26"/>
<contactref element="U$3" pad="P$26"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="AD10">
<contactref element="U$1" pad="P$27"/>
<contactref element="U$2" pad="P$27"/>
<contactref element="U$3" pad="P$27"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="AD11">
<contactref element="U$1" pad="P$28"/>
<contactref element="U$2" pad="P$28"/>
<contactref element="U$3" pad="P$28"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="AD12">
<contactref element="U$1" pad="P$29"/>
<contactref element="U$2" pad="P$29"/>
<contactref element="U$3" pad="P$29"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="AD13">
<contactref element="U$1" pad="P$30"/>
<contactref element="U$2" pad="P$30"/>
<contactref element="U$3" pad="P$30"/>
<contactref element="JP1" pad="11"/>
</signal>
<signal name="AD14">
<contactref element="U$1" pad="P$31"/>
<contactref element="U$2" pad="P$31"/>
<contactref element="U$3" pad="P$31"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="SO/WR/EN">
<contactref element="JP1" pad="12"/>
<contactref element="U$1" pad="P$35"/>
<contactref element="U$2" pad="P$35"/>
<contactref element="U$3" pad="P$35"/>
</signal>
<signal name="SCK/AL">
<contactref element="U$1" pad="P$37"/>
<contactref element="U$2" pad="P$37"/>
<contactref element="U$3" pad="P$37"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$38">
<contactref element="U$1" pad="P$43"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="U$2" pad="P$11"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="U$2" pad="P$16"/>
<contactref element="R61" pad="2"/>
<contactref element="C63" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U$2" pad="P$17"/>
<contactref element="R63" pad="2"/>
<contactref element="C62" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R61" pad="1"/>
<contactref element="C61" pad="1"/>
<contactref element="R63" pad="1"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="U$2" pad="P$21"/>
<contactref element="R62" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U$2" pad="P$20"/>
<contactref element="R64" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R65" pad="1"/>
<contactref element="C64" pad="1"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$25">
<contactref element="C62" pad="2"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$26">
<contactref element="C63" pad="2"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$27">
<contactref element="J2" pad="11"/>
<contactref element="R66" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="J2" pad="9"/>
<contactref element="R67" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="U$2" pad="P$43"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="U$3" pad="P$11"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="U$3" pad="P$16"/>
<contactref element="R71" pad="2"/>
<contactref element="C73" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="U$3" pad="P$17"/>
<contactref element="R73" pad="2"/>
<contactref element="C72" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R71" pad="1"/>
<contactref element="C71" pad="1"/>
<contactref element="R73" pad="1"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="N$37">
<contactref element="U$3" pad="P$21"/>
<contactref element="R72" pad="1"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="U$3" pad="P$20"/>
<contactref element="R74" pad="1"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="R75" pad="1"/>
<contactref element="C74" pad="1"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="N$41">
<contactref element="C72" pad="2"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="N$42">
<contactref element="C73" pad="2"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="R76">
<contactref element="J3" pad="11"/>
<contactref element="R76" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="J3" pad="9"/>
<contactref element="R77" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="U$3" pad="P$43"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="CS/CS0">
<contactref element="U$1" pad="P$34"/>
<contactref element="INT3" pad="1"/>
</signal>
<signal name="CS/CS1">
<contactref element="U$2" pad="P$34"/>
<contactref element="INT3" pad="2"/>
</signal>
<signal name="CS/CS2">
<contactref element="U$3" pad="P$34"/>
<contactref element="INT3" pad="3"/>
</signal>
<signal name="N$51">
<contactref element="LED1" pad="C"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="U$3" pad="P$24"/>
<contactref element="INT2" pad="2"/>
</signal>
<signal name="N$58">
<contactref element="U$2" pad="P$24"/>
<contactref element="INT1" pad="2"/>
</signal>
<signal name="N$59">
<contactref element="U$1" pad="P$24"/>
<contactref element="INT0" pad="2"/>
</signal>
<signal name="LEDA0">
<contactref element="R56" pad="1"/>
<contactref element="U$1" pad="P$10"/>
</signal>
<signal name="LEDB0">
<contactref element="R57" pad="1"/>
<contactref element="U$1" pad="P$9"/>
</signal>
<signal name="LEDB1">
<contactref element="U$2" pad="P$9"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="LEDA1">
<contactref element="U$2" pad="P$10"/>
<contactref element="R66" pad="1"/>
</signal>
<signal name="LEDB2">
<contactref element="U$3" pad="P$9"/>
<contactref element="R77" pad="1"/>
</signal>
<signal name="LEDA2">
<contactref element="U$3" pad="P$10"/>
<contactref element="R76" pad="1"/>
</signal>
<signal name="N$64">
<contactref element="Q4" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$77">
<contactref element="IC1" pad="8"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="ETHCLK">
<contactref element="IC1" pad="6"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="CLKOUT0">
<contactref element="U$1" pad="P$23"/>
</signal>
<signal name="CLKOUT1">
<contactref element="U$2" pad="P$23"/>
</signal>
<signal name="CLKOUT2">
<contactref element="U$3" pad="P$23"/>
</signal>
<signal name="N$2">
<contactref element="C6" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
