<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.652" y2="0" width="0" layer="20"/>
<wire x1="33.652" y1="0" x2="33.652" y2="20" width="0" layer="20"/>
<wire x1="33.652" y1="20" x2="0" y2="20" width="0" layer="20"/>
<wire x1="0" y1="20" x2="0" y2="0" width="0" layer="20"/>
<text>V.1</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>PWM</text>
<text>1</text>
<text>2</text>
<text>John loves Anya
and our baby boy</text>
<text>3</text>
<text>Blower</text>
<text>Servo</text>
</plain>
<libraries>
<library name="HeaterMeterPI">
<description>Generated from &lt;b&gt;HeaterMeterPI.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="RJ45-8-1H">
<description>Amphenol RJHSE-5080 no LED
Mouser 523-RJHSE-5080</description>
</package>
</packages>
</library>
<library name="2.5mm inline screw mono jack">
<description>Generated from &lt;b&gt;HeaterMeterPI.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="CUI-MJ-2508">
<description>CUI Inc MJ-2508 and MJ-2508N (non-threaded)

DigiKey Part CP-2508-ND and CP-2508N-ND</description>
</package>
</packages>
</library>
<library name="AMP_MTATC">
<packages>
<package name="1X05MTA">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="2.5mm inline screw mono jack" package="CUI-MJ-2508" value="AUDIO-MONO"/>
<element name="JP3" library="2.5mm inline screw mono jack" package="CUI-MJ-2508" value="AUDIO-MONO"/>
<element name="U$1" library="HeaterMeterPI" package="RJ45-8-1H" value="RJ45-8"/>
<element name="J2" library="AMP_MTATC" package="1X05MTA" value="">
<attribute name="NAME"/>
</element>
<element name="JP2" library="2.5mm inline screw mono jack" package="CUI-MJ-2508" value="AUDIO-MONO"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="U$1" pad="8"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GROUND">
<contactref element="U$1" pad="4"/>
<contactref element="J2" pad="1"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="SERVO">
<contactref element="U$1" pad="6"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="BLOWER+">
<contactref element="U$1" pad="5"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="PROBE1">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="PROBE2">
<contactref element="U$1" pad="2"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="J2" pad="4"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="7"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
