<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="50.8" x2="0" y2="0.0125" width="0" layer="20"/>
<wire x1="0" y1="0.0125" x2="50.79" y2="0.0125" width="0" layer="20"/>
<wire x1="50.79" y1="0.0125" x2="50.79" y2="50.8" width="0" layer="20"/>
<wire x1="50.79" y1="50.8" x2="0" y2="50.8" width="0" layer="20"/>
<text>INT1</text>
<text>INT0</text>
<text>CS1</text>
<text>CS0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>5</text>
<text>7</text>
<text>8</text>
<text>6</text>
<text>4</text>
<text>0</text>
<text>AL</text>
<text>WR</text>
<text>3v3</text>
<text>GND</text>
<text>RD</text>
<text>ETH0</text>
<text>ETH1</text>
<hole x="3.65125" y="47.14875" drill="2"/>
<hole x="36.195" y="47.46625" drill="2"/>
<hole x="5.08" y="2.54" drill="2"/>
<text>Double Ethernet</text>
<text>base board v1 (c) 2015 Josh Stone</text>
<hole x="47.14875" y="3.4925" drill="2"/>
<text>LINK</text>
<text>LINK</text>
<text>ACT</text>
<text>ACT</text>
</plain>
<libraries>
<library name="josh">
<packages>
<package name="TQFP-44">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MAGJACK">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;B&gt;CRYSTAL&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are no longer used in our catalog.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NOTRACE">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="josh" package="TQFP-44" value="ENC424J600">
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="C0603" value="10 uF">
<attribute name="NAME"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="100">
<attribute name="NAME"/>
</element>
<element name="C8" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C7" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-FreqCtrl" package="HC49US" value="25 mHz"/>
<element name="R6" library="adafruit" package="R0603" value="12.4 k">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C1" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="C4" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="R8" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R7" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R5" library="adafruit" package="R0603" value="10">
<attribute name="NAME"/>
</element>
<element name="C6" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="MAGJACK" value="MAGJACK"/>
<element name="R2" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="R9" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="C10" library="adafruit" package="C0603" value="1 uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="adafruit" package="C0603" value="0.1 uF">
<attribute name="NAME"/>
</element>
<element name="C5" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
<element name="PWR" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="adafruit" package="R0603" value="600">
<attribute name="NAME"/>
</element>
<element name="SV1" library="pinhead" package="2X07" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="josh" package="TQFP-44" value="ENC424J600">
<attribute name="VALUE"/>
</element>
<element name="C11" library="adafruit" package="C0603" value="10 uF">
<attribute name="NAME"/>
</element>
<element name="R10" library="adafruit" package="R0603" value="100">
<attribute name="NAME"/>
</element>
<element name="C12" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C13" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="Q2" library="SparkFun-FreqCtrl" package="HC49US" value="25 mHz"/>
<element name="R11" library="adafruit" package="R0603" value="12.4 k">
<attribute name="NAME"/>
</element>
<element name="R12" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R13" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C14" library="adafruit" package="C0603" value="10 pF">
<attribute name="NAME"/>
</element>
<element name="C15" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="C16" library="adafruit" package="C0603" value="6.8 nF">
<attribute name="NAME"/>
</element>
<element name="R14" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R15" library="adafruit" package="R0603" value="49.9">
<attribute name="NAME"/>
</element>
<element name="R16" library="adafruit" package="R0603" value="10">
<attribute name="NAME"/>
</element>
<element name="C17" library="adafruit" package="C0603" value="0.01 uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="MAGJACK" value="MAGJACK"/>
<element name="R17" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="R18" library="adafruit" package="R0603" value="330">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun-Retired" package="SJ_2S-NOTRACE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="SparkFun-Retired" package="SJ_2S-NOTRACE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="SparkFun-Retired" package="SJ_2S-NOTRACE" value=""/>
<element name="C18" library="adafruit" package="C0603" value="100 uF">
<attribute name="NAME"/>
</element>
<element name="C19" library="adafruit" package="C0603" value="100 uF">
<attribute name="NAME"/>
</element>
<element name="C20" library="adafruit" package="C0603" value="100 uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="P$11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="U$1" pad="P$12"/>
<contactref element="U$1" pad="P$15"/>
<contactref element="U$1" pad="P$18"/>
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$44"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="PWR" pad="A"/>
<contactref element="U$1" pad="P$31"/>
<contactref element="U$1" pad="P$30"/>
<contactref element="U$1" pad="P$29"/>
<contactref element="U$1" pad="P$28"/>
<contactref element="U$1" pad="P$27"/>
<contactref element="U$1" pad="P$26"/>
<contactref element="SV1" pad="13"/>
<contactref element="U$2" pad="P$12"/>
<contactref element="U$2" pad="P$15"/>
<contactref element="U$2" pad="P$18"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="U$2" pad="P$4"/>
<contactref element="U$2" pad="P$44"/>
<contactref element="U$2" pad="P$31"/>
<contactref element="U$2" pad="P$30"/>
<contactref element="U$2" pad="P$29"/>
<contactref element="U$2" pad="P$28"/>
<contactref element="U$2" pad="P$27"/>
<contactref element="U$2" pad="P$26"/>
<contactref element="C20" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$16"/>
<contactref element="R3" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$17"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="P$21"/>
<contactref element="R8" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="P$20"/>
<contactref element="R7" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="N$6">
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="11"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="J1" pad="9"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="AD7">
<contactref element="U$1" pad="P$8"/>
<contactref element="U$2" pad="P$8"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="AD6">
<contactref element="U$1" pad="P$7"/>
<contactref element="U$2" pad="P$7"/>
<contactref element="SV1" pad="4"/>
</signal>
<signal name="AD5">
<contactref element="U$1" pad="P$6"/>
<contactref element="U$2" pad="P$6"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="AD4">
<contactref element="U$1" pad="P$5"/>
<contactref element="U$2" pad="P$5"/>
<contactref element="SV1" pad="6"/>
</signal>
<signal name="AD3">
<contactref element="U$1" pad="P$41"/>
<contactref element="U$2" pad="P$41"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="AD2">
<contactref element="U$1" pad="P$40"/>
<contactref element="U$2" pad="P$40"/>
<contactref element="SV1" pad="8"/>
</signal>
<signal name="AD1">
<contactref element="U$1" pad="P$39"/>
<contactref element="U$2" pad="P$39"/>
<contactref element="SV1" pad="7"/>
</signal>
<signal name="AD0">
<contactref element="U$1" pad="P$38"/>
<contactref element="U$2" pad="P$38"/>
<contactref element="SV1" pad="10"/>
</signal>
<signal name="SI/RD/RW">
<contactref element="U$1" pad="P$36"/>
<contactref element="U$2" pad="P$36"/>
<contactref element="SV1" pad="12"/>
</signal>
<signal name="SO/WR/EN">
<contactref element="U$1" pad="P$35"/>
<contactref element="SV1" pad="11"/>
<contactref element="U$2" pad="P$35"/>
</signal>
<signal name="SCK/AL">
<contactref element="U$1" pad="P$37"/>
<contactref element="U$2" pad="P$37"/>
<contactref element="SV1" pad="9"/>
</signal>
<signal name="N$38">
<contactref element="U$1" pad="P$43"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="CS/CS0">
<contactref element="U$1" pad="P$34"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="PWR" pad="C"/>
<contactref element="R28" pad="2"/>
</signal>
<signal name="LEDA0">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="P$10"/>
</signal>
<signal name="LEDB0">
<contactref element="R9" pad="1"/>
<contactref element="U$1" pad="P$9"/>
</signal>
<signal name="INT/SPISEL0">
<contactref element="U$1" pad="P$24"/>
<contactref element="JP1" pad="1"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="U$2" pad="P$2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R10" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="Q2" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="N$26">
<contactref element="U$2" pad="P$11"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="U$2" pad="P$16"/>
<contactref element="R12" pad="2"/>
<contactref element="C16" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="U$2" pad="P$17"/>
<contactref element="R13" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="R12" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$30">
<contactref element="U$2" pad="P$21"/>
<contactref element="R14" pad="1"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="U$2" pad="P$20"/>
<contactref element="R15" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$32">
<contactref element="R16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$33">
<contactref element="C15" pad="2"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="N$34">
<contactref element="C16" pad="2"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="N$35">
<contactref element="J2" pad="11"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="J2" pad="9"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="U$2" pad="P$43"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="CS/CS1">
<contactref element="U$2" pad="P$34"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="LEDA1">
<contactref element="R17" pad="1"/>
<contactref element="U$2" pad="P$10"/>
</signal>
<signal name="LEDB1">
<contactref element="R18" pad="1"/>
<contactref element="U$2" pad="P$9"/>
</signal>
<signal name="N$41">
</signal>
<signal name="N$42">
</signal>
<signal name="N$43">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="N$46">
</signal>
<signal name="INT/SPISEL1">
<contactref element="U$2" pad="P$24"/>
<contactref element="JP1" pad="4"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="CLOCKOUT1">
<contactref element="U$2" pad="P$23"/>
</signal>
<signal name="CLOCKOUT0">
<contactref element="U$1" pad="P$23"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$1"/>
<contactref element="C3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U$1" pad="P$13"/>
<contactref element="U$1" pad="P$14"/>
<contactref element="U$1" pad="P$19"/>
<contactref element="U$1" pad="P$22"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="C11" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="U$2" pad="P$13"/>
<contactref element="U$2" pad="P$14"/>
<contactref element="U$2" pad="P$19"/>
<contactref element="U$2" pad="P$22"/>
<contactref element="C14" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="J2" pad="12"/>
<contactref element="J2" pad="10"/>
<contactref element="J2" pad="M2"/>
<contactref element="J2" pad="M1"/>
<contactref element="U$2" pad="P$32"/>
<contactref element="SJ1" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="J1" pad="12"/>
<contactref element="J1" pad="10"/>
<contactref element="J1" pad="M2"/>
<contactref element="J1" pad="M1"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="U$1" pad="P$32"/>
<contactref element="U$1" pad="P$33"/>
<contactref element="U$1" pad="P$42"/>
<contactref element="SV1" pad="14"/>
<contactref element="U$2" pad="P$33"/>
<contactref element="U$2" pad="P$42"/>
<contactref element="SJ3" pad="1"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
</signal>
<signal name="AD8">
<contactref element="SV1" pad="2"/>
<contactref element="U$1" pad="P$25"/>
<contactref element="U$2" pad="P$25"/>
<contactref element="SJ3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
