<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.07" y2="0" width="0" layer="20"/>
<wire x1="25.07" y1="0" x2="25.07" y2="20.31" width="0" layer="20"/>
<wire x1="25.07" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<text>ESC CALIBRATOR</text>
<text>G</text>
<text>G</text>
<text>DEPEW DESIGNS</text>
<text>2.15.15</text>
<text>Note: Only M1</text>
<text>BEC Connected to RX</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="M1" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M2" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M3" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M4" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M5" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M6" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M7" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M8" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX" library="SparkFun" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="adafruit" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="SIG">
<contactref element="M1" pad="3"/>
<contactref element="M2" pad="3"/>
<contactref element="M3" pad="3"/>
<contactref element="M4" pad="3"/>
<contactref element="M5" pad="3"/>
<contactref element="M6" pad="3"/>
<contactref element="M7" pad="3"/>
<contactref element="M8" pad="3"/>
<contactref element="RX" pad="3"/>
</signal>
<signal name="GND">
<contactref element="M1" pad="1"/>
<contactref element="M2" pad="1"/>
<contactref element="M3" pad="1"/>
<contactref element="M4" pad="1"/>
<contactref element="M5" pad="1"/>
<contactref element="M6" pad="1"/>
<contactref element="M7" pad="1"/>
<contactref element="M8" pad="1"/>
<contactref element="RX" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="5V">
<contactref element="RX" pad="2"/>
<contactref element="M1" pad="2"/>
<contactref element="PWR" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="PWR" pad="C"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
