<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="32" y2="0" width="0" layer="20"/>
<wire x1="32" y1="0" x2="32" y2="29" width="0" layer="20"/>
<wire x1="32" y1="29" x2="0" y2="29" width="0" layer="20"/>
<wire x1="0" y1="29" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="pdm_mic_st">
<packages>
<package name="HLGA">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,2">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 3.2 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="pdm_mic_st" package="HLGA" value="MP045DT2"/>
<element name="C1" library="adafruit" package="C0805K" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X03" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H2" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H3" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="H4" library="holes" package="3,2" value="MOUNT-HOLE3.2"/>
<element name="JP3" library="pinhead" package="1X04" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="A"/>
<contactref element="U$1" pad="PIN_VDD"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="C"/>
<contactref element="U$1" pad="PIN_GND1"/>
<contactref element="U$1" pad="PIN_GND0"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="PIN_DOUT"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="PIN_CLK"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="PIN_LR"/>
<contactref element="JP2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
