<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="-0.34" y1="33.56" x2="21.66" y2="41.56" width="0" layer="20" curve="-150.0004"/>
<wire x1="21.66" y1="41.56" x2="43.66" y2="33.56" width="0" layer="20" curve="-150.0004"/>
<wire x1="-0.34" y1="33.56" x2="21.66" y2="1.56" width="0" layer="20" curve="60.000023"/>
<wire x1="43.66" y1="33.56" x2="21.66" y2="1.56" width="0" layer="20" curve="-60.000023"/>
<hole x="6.36" y="42.806" drill="3.2"/>
<hole x="36.052" y="43.06" drill="3.2"/>
<text>Time</text>
<text>Until</text>
<text>We can </text>
<text>See each other</text>
<text>AGAIN</text>
</plain>
<libraries>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL12">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
<package name="0603-RES">
</package>
<package name="LED-0603">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="CRYSTAL-SMD-5X3">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="BATTCON_12MM_PTH">
</package>
</packages>
</library>
<library name="Testing">
<packages>
<package name="QFN-44-NOPAD_1:1-OUTFAKES">
</package>
<package name="USB-AB-MICRO-SMD-V03-IN&amp;OUT">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C10" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="C13" library="SparkFun" package="EIA3216" value="10uF"/>
<element name="R11" library="SparkFun" package="0603-RES" value="1K"/>
<element name="LED1" library="SparkFun" package="LED-0603" value="Red"/>
<element name="R2" library="SparkFun" package="0603-RES" value="10K"/>
<element name="C3" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="C1" library="SparkFun" package="0603-CAP" value="0.1uF"/>
<element name="U2" library="SparkFun" package="SOT23-5" value="MIC5219"/>
<element name="U3" library="Testing" package="QFN-44-NOPAD_1:1-OUTFAKES" value="ATMEGA32U4"/>
<element name="Y1" library="SparkFun" package="CRYSTAL-SMD-5X3" value="16MHz"/>
<element name="C2" library="SparkFun" package="0603-CAP" value="22pF"/>
<element name="C4" library="SparkFun" package="0603-CAP" value="22pF"/>
<element name="C5" library="SparkFun" package="0603-CAP" value="1uF"/>
<element name="R5" library="SparkFun" package="0603-RES" value="22"/>
<element name="R7" library="SparkFun" package="0603-RES" value="22"/>
<element name="X1" library="Testing" package="USB-AB-MICRO-SMD-V03-IN&amp;OUT" value=""/>
<element name="U$4" library="SparkFun-Displays" package="DIL12" value="7-SEGMENT-4DIGIT-COUNTER-HP-BUBBLE">
<attribute name="STOREFRONT" value="COM-12710"/>
</element>
<element name="U4" library="SparkFun" package="SO08" value="DS1307"/>
<element name="BAT2" library="SparkFun" package="BATTCON_12MM_PTH" value=""/>
<element name="R1" library="SparkFun" package="0603-RES" value="330"/>
<element name="R3" library="SparkFun" package="0603-RES" value="330"/>
<element name="R8" library="SparkFun" package="0603-RES" value="330"/>
<element name="R9" library="SparkFun" package="0603-RES" value="330"/>
<element name="U$1" library="SparkFun-Displays" package="DIL12" value="7-SEGMENT-4DIGIT-COUNTER-HP-BUBBLE">
<attribute name="STOREFRONT" value="COM-12710"/>
</element>
<element name="R10" library="SparkFun" package="0603-RES" value="330"/>
<element name="R12" library="SparkFun" package="0603-RES" value="330"/>
<element name="R13" library="SparkFun" package="0603-RES" value="330"/>
<element name="R14" library="SparkFun" package="0603-RES" value="330"/>
<element name="Y2" library="SparkFun" package="CRYSTAL-SMD-5X3" value="32.768"/>
<element name="C7" library="SparkFun" package="0603-CAP" value="22pF"/>
<element name="C9" library="SparkFun" package="0603-CAP" value="22pF"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C13" pad="C"/>
<contactref element="C10" pad="2"/>
<contactref element="LED1" pad="C"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U3" pad="15"/>
<contactref element="U3" pad="43"/>
<contactref element="U3" pad="35"/>
<contactref element="U3" pad="23"/>
<contactref element="U3" pad="5"/>
<contactref element="U3" pad="33"/>
<contactref element="C5" pad="1"/>
<contactref element="X1" pad="GND1"/>
<contactref element="U4" pad="4"/>
<contactref element="BAT2" pad="GND"/>
<contactref element="C7" pad="2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="C1" pad="2"/>
<contactref element="U3" pad="42"/>
</signal>
<signal name="RESET">
<contactref element="R2" pad="1"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="N$38">
<contactref element="R11" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="U3" pad="14"/>
<contactref element="U3" pad="34"/>
<contactref element="U3" pad="24"/>
<contactref element="U3" pad="44"/>
<contactref element="C10" pad="1"/>
<contactref element="C13" pad="A"/>
<contactref element="U2" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="U4" pad="8"/>
</signal>
<signal name="RAW">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="X1" pad="VBUS1"/>
</signal>
<signal name="PD5">
<contactref element="R8" pad="1"/>
<contactref element="U3" pad="22"/>
</signal>
<signal name="N$1">
<contactref element="Y1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="17"/>
</signal>
<signal name="N$2">
<contactref element="Y1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="N$4">
<contactref element="U3" pad="6"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="UVCC">
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="D-">
<contactref element="U3" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="D+">
<contactref element="U3" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="2"/>
<contactref element="X1" pad="D-1"/>
</signal>
<signal name="N$8">
<contactref element="R5" pad="2"/>
<contactref element="X1" pad="D+1"/>
</signal>
<signal name="SQW">
<contactref element="U4" pad="7"/>
</signal>
<signal name="SCL">
<contactref element="U3" pad="18"/>
<contactref element="U4" pad="6"/>
</signal>
<signal name="SDA">
<contactref element="U3" pad="19"/>
<contactref element="U4" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="U4" pad="1"/>
<contactref element="Y2" pad="3"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U4" pad="2"/>
<contactref element="Y2" pad="1"/>
<contactref element="C9" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="U4" pad="3"/>
<contactref element="BAT2" pad="VCC@1"/>
</signal>
<signal name="N$9">
<contactref element="U$4" pad="6"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$4" pad="4"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="U$4" pad="10"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U$4" pad="1"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="U$1" pad="6"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="U$1" pad="4"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="U$1" pad="10"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="U$1" pad="1"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="PF7">
<contactref element="U3" pad="36"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="PF6">
<contactref element="U3" pad="37"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="PF5">
<contactref element="U3" pad="38"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="PF4">
<contactref element="U3" pad="39"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="PF1">
<contactref element="U3" pad="40"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="PF0">
<contactref element="U3" pad="41"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="PD2">
<contactref element="U3" pad="20"/>
<contactref element="U$4" pad="11"/>
</signal>
<signal name="PD3">
<contactref element="U3" pad="21"/>
<contactref element="U$4" pad="12"/>
</signal>
<signal name="PD4">
<contactref element="U3" pad="25"/>
<contactref element="U$4" pad="9"/>
</signal>
<signal name="PC6">
<contactref element="U3" pad="31"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="PD7">
<contactref element="U3" pad="27"/>
<contactref element="U$4" pad="7"/>
</signal>
<signal name="PE6">
<contactref element="U3" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="PB4">
<contactref element="U3" pad="28"/>
<contactref element="U$1" pad="12"/>
</signal>
<signal name="PB5">
<contactref element="U3" pad="29"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="PB6">
<contactref element="U3" pad="30"/>
</signal>
<signal name="PB7">
<contactref element="U3" pad="12"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="PD6">
<contactref element="U3" pad="26"/>
<contactref element="U$4" pad="8"/>
</signal>
<signal name="PC7">
<contactref element="U3" pad="32"/>
<contactref element="U$1" pad="9"/>
</signal>
<signal name="PB0">
<contactref element="U3" pad="8"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PB1">
<contactref element="U3" pad="9"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="PB2">
<contactref element="U3" pad="10"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="PB3">
<contactref element="U3" pad="11"/>
<contactref element="U$4" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
