<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="38.1" x2="0" y2="3.5921" width="0" layer="20"/>
<wire x1="0" y1="3.5921" x2="3.5921" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3.5921" y1="0" x2="23.233509375" y2="0" width="0" layer="20"/>
<wire x1="23.233509375" y1="0" x2="27.28" y2="4.046490625" width="0" layer="20" curve="90"/>
<wire x1="27.28" y1="4.046490625" x2="27.28" y2="37.88558125" width="0" layer="20"/>
<wire x1="27.28" y1="37.88558125" x2="23.19558125" y2="41.97" width="0" layer="20" curve="90"/>
<wire x1="23.19558125" y1="41.97" x2="3.87" y2="41.97" width="0" layer="20"/>
<wire x1="3.87" y1="41.97" x2="0" y2="38.1" width="0" layer="20" curve="90"/>
<text>jordanmills</text>
<text>RFM69W/
HCW/LoRa
1.0</text>
<text>ANT</text>
</plain>
<libraries>
<library name="SHF-105-01-X-D-SM">
<packages>
<package name="SHF-105-01-X-D-SM">
<description>0.050"X0.050" SHROUDED TERMINAL STRIP ASSEMBLY, 10PINS.</description>
</package>
</packages>
</library>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RFM69HCW-XXXS2">
</package>
<package name="RFM69W-XXXS2">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="U.FL">
</package>
</packages>
</library>
<library name="Gadgeteer">
<packages>
<package name="GADGETEER_LOGO_SMALL">
</package>
<package name="HOLE3.2">
<description>3.2mm mounting hole</description>
</package>
<package name="LABEL_S">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SHF-105-01-X-D-SM" package="SHF-105-01-X-D-SM" value="SHF-105-01-X-D-SM"/>
<element name="U2" library="SparkFun-RF" package="RFM69HCW-XXXS2" value="RFM69HCW">
<attribute name="PROD_ID" value="IC-11997, IC-12053"/>
</element>
<element name="U3" library="SparkFun-RF" package="RFM69W-XXXS2" value="RFM69HW"/>
<element name="X1" library="adafruit" package="U.FL" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Gadgeteer" package="GADGETEER_LOGO_SMALL" value=""/>
<element name="U$3" library="Gadgeteer" package="HOLE3.2" value=""/>
<element name="U$4" library="Gadgeteer" package="LABEL_S" value=""/>
<element name="U$1" library="Gadgeteer" package="HOLE3.2" value=""/>
<element name="U$5" library="Gadgeteer" package="HOLE3.2" value=""/>
<element name="U$6" library="Gadgeteer" package="HOLE3.2" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3.3V">
<contactref element="J1" pad="1"/>
<contactref element="U2" pad="13"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="10"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="10"/>
<contactref element="U3" pad="11"/>
<contactref element="X1" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="U2" pad="1"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="DIO0">
<contactref element="J1" pad="3"/>
<contactref element="U2" pad="14"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="4"/>
<contactref element="U2" pad="6"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="NSS">
<contactref element="J1" pad="5"/>
<contactref element="U3" pad="15"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="7"/>
<contactref element="U3" pad="14"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="8"/>
<contactref element="U3" pad="13"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="9"/>
<contactref element="U3" pad="12"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="ANT">
<contactref element="U2" pad="9"/>
<contactref element="U3" pad="10"/>
<contactref element="X1" pad="3"/>
<contactref element="J2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
