<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="-1.27" y1="0" x2="15.545" y2="0" width="0" layer="20"/>
<wire x1="15.545" y1="0" x2="15.545" y2="26.025" width="0" layer="20"/>
<wire x1="15.545" y1="26.025" x2="-1.27" y2="26.025" width="0" layer="20"/>
<wire x1="-1.27" y1="26.025" x2="-1.27" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C7.5B3">
<description>&lt;B&gt;MKS3&lt;/B&gt;, 10 x 3 mm, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="eagle-ltspice">
<description>Default symbols for import LTspice schematics&lt;p&gt;
2012-10-29 alf@cadsoft.de&lt;br&gt;</description>
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="burr-brown">
<description>&lt;b&gt;Burr-Brown Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;Smal Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPDT">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="esp8266modules">
<packages>
<package name="ESP01">
<description>ESP8266 Module 01</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name=".1UF" library="capacitor-wima" package="C7.5B3" value=""/>
<element name="4.7K" library="eagle-ltspice" package="0204/7" value="">
<attribute name="SPICEPREFIX" value="R"/>
<attribute name="SPICEMODEL" value="NONE"/>
</element>
<element name="IC1" library="burr-brown" package="SOT223" value="REG1117">
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="14P6981"/>
<attribute name="OC_FARNELL" value="1097566"/>
<attribute name="MPN" value="REG1117"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="SWITCH-SPDT" value="">
<attribute name="PROD_ID" value="SWCH-08261"/>
</element>
<element name="TMP" library="pinhead" package="1X03" value=""/>
<element name="TMP1" library="pinhead" package="1X03" value=""/>
<element name="TMP2" library="pinhead" package="1X03" value=""/>
<element name="TR" library="pinhead" package="1X02" value=""/>
<element name="U$1" library="esp8266modules" package="ESP01" value="ESP01"/>
<element name="VG" library="pinhead" package="1X02" value=""/>
</elements>
<signals>
<signal name="TX">
<contactref element="TR" pad="1"/>
<contactref element="U$1" pad="TX"/>
</signal>
<signal name="RX">
<contactref element="TR" pad="2"/>
<contactref element="U$1" pad="RX"/>
</signal>
<signal name="VCC">
<contactref element="VG" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="GND">
<contactref element="VG" pad="2"/>
<contactref element="TMP" pad="3"/>
<contactref element="TMP2" pad="3"/>
<contactref element="TMP1" pad="3"/>
<contactref element="S1" pad="3"/>
<contactref element="U$1" pad="GND"/>
<contactref element="IC1" pad="1"/>
<contactref element=".1UF" pad="2"/>
</signal>
<signal name="3.3">
<contactref element="TMP" pad="1"/>
<contactref element="TMP2" pad="1"/>
<contactref element="TMP1" pad="1"/>
<contactref element="U$1" pad="CH_PD"/>
<contactref element="U$1" pad="RST"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="S1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="4.7K" pad="2"/>
<contactref element=".1UF" pad="1"/>
</signal>
<signal name="DATA">
<contactref element="TMP" pad="2"/>
<contactref element="TMP2" pad="2"/>
<contactref element="TMP1" pad="2"/>
<contactref element="U$1" pad="GPIO2"/>
<contactref element="4.7K" pad="1"/>
</signal>
<signal name="GPIO0">
<contactref element="S1" pad="2"/>
<contactref element="U$1" pad="GPIO0"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
