<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0.508" y1="0" x2="56.566" y2="0" width="0" layer="20"/>
<wire x1="56.566" y1="0" x2="56.566" y2="18.532" width="0" layer="20"/>
<wire x1="56.566" y1="18.532" x2="0.508" y2="18.532" width="0" layer="20"/>
<wire x1="0.508" y1="18.532" x2="0.508" y2="0" width="0" layer="20"/>
<text>XTAL</text>
<text>ATtiny Programming 
Adapter</text>
<text>Spa Electronics</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CAP-PTH-SMALL">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AVRISP-BOX">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-PTH">
</package>
</packages>
</library>
<library name="con-3m">
<description>&lt;b&gt;3M Connectors&lt;/b&gt;&lt;p&gt;
PCMCIA-CompactFlash Connectors&lt;p&gt;
Zero Insertion Force Socked&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="214-3339-00-0602J">
<description>&lt;b&gt;3M TEXTOOL 14 pol. DIP&lt;/b&gt; Lever actuated zero insertion force mechanism &lt;p&gt;
Hersteller: 3M TEXTOOL&lt;br&gt;
Herstellerbez.:  214-3339-00-0602J&lt;br&gt;
Farnell Best.-Nr.: 4666290&lt;br&gt;
Source: http://www.3M.com/ehpd</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="CAP-PTH-SMALL" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="ISP" library="adafruit" package="AVRISP-BOX" value="AVRISP-BOX">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.4" value="10K">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="DIP08" value="TINY25/45/85/13">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Y1" library="SparkFun-FreqCtrl" package="RESONATOR-PTH" value=""/>
<element name="ZX1" library="con-3m" package="214-3339-00-0602J" value="TINY24/44/84">
<attribute name="OC_FARNELL" value="1247151"/>
<attribute name="MF" value="3M"/>
<attribute name="MPN" value="214-3339-00-0602J"/>
<attribute name="OC_NEWARK" value="85K7793"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="ISP" pad="2"/>
<contactref element="R1" pad="P$1"/>
<contactref element="U1" pad="8"/>
<contactref element="C1" pad="2"/>
<contactref element="ZX1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="ISP" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="C1" pad="1"/>
<contactref element="Y1" pad="2"/>
<contactref element="ZX1" pad="14"/>
</signal>
<signal name="MOSI">
<contactref element="ISP" pad="4"/>
<contactref element="U1" pad="5"/>
<contactref element="ZX1" pad="7"/>
</signal>
<signal name="MISO">
<contactref element="ISP" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="ZX1" pad="8"/>
</signal>
<signal name="SCK">
<contactref element="ISP" pad="3"/>
<contactref element="U1" pad="7"/>
<contactref element="ZX1" pad="9"/>
</signal>
<signal name="RESET">
<contactref element="ISP" pad="5"/>
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="ZX1" pad="4"/>
</signal>
<signal name="XTAL1">
<contactref element="ZX1" pad="2"/>
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="XTAL2">
<contactref element="ZX1" pad="3"/>
<contactref element="Y1" pad="3"/>
<contactref element="U1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
