<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>Techno</text>
<circle x="9.525" y="9.525" radius="9.525" width="0.002540625" layer="20"/>
<circle x="5.715" y="16.51" radius="0.898025" width="0.002540625" layer="20"/>
<circle x="13.335" y="16.51" radius="0.898025" width="0.002540625" layer="20"/>
<circle x="13.335" y="2.54" radius="0.898025" width="0.002540625" layer="20"/>
<circle x="5.715" y="2.54" radius="0.898025" width="0.002540625" layer="20"/>
<text>blogy</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="1X01-CLEANBIG">
</package>
<package name="SOT23-6">
</package>
<package name="RGBLED5050">
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_12MM">
</package>
<package name="TACTILE-SWITCH-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP2" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="adafruit" package="1X01-CLEANBIG" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="100n"/>
<element name="IC1" library="adafruit" package="SOT23-6" value="ATTINY10">
<attribute name="NAME"/>
</element>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_12MM" value="">
<attribute name="PROD_ID" value="BATT-08044"/>
</element>
<element name="LED1" library="adafruit" package="RGBLED5050" value="RGBLED5050"/>
<element name="R1" library="adafruit" package="R0805" value="1kΩ"/>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-SWITCH-SMD" value="SWITCH-MOMENTARY-2SMD">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="R0805" value="1kΩ"/>
<element name="R3" library="adafruit" package="R0805" value="1kΩ"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="IC1" pad="5"/>
<contactref element="LED1" pad="3"/>
<contactref element="LED1" pad="1"/>
<contactref element="LED1" pad="2"/>
<contactref element="BAT1" pad="PWR@1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="4"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="IC1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="S2" pad="1"/>
<contactref element="IC1" pad="6"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="S2" pad="3"/>
<contactref element="JP2" pad="1"/>
<contactref element="BAT1" pad="GND"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="6"/>
</signal>
<signal name="N$9">
</signal>
</signals>
</board>
</drawing>
</eagle>
