<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="5.08" x2="56.896" y2="5.08" width="0" layer="20"/>
<wire x1="56.896" y1="5.08" x2="56.896" y2="50.8" width="0" layer="20"/>
<wire x1="56.896" y1="50.8" x2="0" y2="50.8" width="0" layer="20"/>
<wire x1="0" y1="50.8" x2="0" y2="5.08" width="0" layer="20"/>
<hole x="3.302" y="8.382" drill="3.048"/>
<hole x="53.594" y="8.382" drill="3.048"/>
<text>GND</text>
<text>VIN</text>
<text>5V-60V</text>
<text>10A MAX</text>
<text>GND</text>
<text>IN0</text>
<text>IN1</text>
<text>IN2</text>
<text>IN3</text>
<text>3V3</text>
<hole x="3.302" y="47.498" drill="3.048"/>
<hole x="53.594" y="47.498" drill="3.048"/>
<text>AM1117
3.3V</text>
<text>http://github.com/pimvanpelt/
4 Port MOSFET Board
version 1.0</text>
<text>C1</text>
<text>C2</text>
<text>VIN</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>Use external Regulator
if VIN &gt; 15V; Short VIN
to VCC to use VIN.</text>
<text>To Ext
Reg</text>
<text>From Ext
Reg</text>
<text>VIN</text>
<text>VIN</text>
<text>VIN</text>
<text>VIN</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>P0</text>
<text>P1</text>
<text>P2</text>
<text>P3</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="SCREWTERMINAL-5MM-2">
<description>&lt;h3&gt;Screw Terminal  5mm Pitch -2 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 5mm/197mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="fuses">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SH23,5A">
<description>&lt;b&gt;FUSE HOLDER&lt;/b&gt;&lt;p&gt; grid 23,5 mm, isolated cap&lt;p&gt; Ordered from Banggood (pim@ipng.nl)</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="FQP30N06L">
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="fuses" package="SH23,5A" value="SH23,5A"/>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-IC-Power" package="SOT223" value="V_REG_LD1117VXXLD1117-SMD">
<attribute name="PROD_ID" value="VREG-13917"/>
</element>
<element name="C1" library="SparkFun-Retired" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="C2" library="SparkFun-Retired" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
</element>
<element name="Q1" library="FQP30N06L" package="TO220V" value="FQP30N06L">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" N-Channel 60V 32A _Tc_ 79W _Tc_ Through Hole TO-220-3 "/>
<attribute name="MF" value="ON Semiconductor"/>
<attribute name="MP" value="FQP30N06L"/>
<attribute name="PACKAGE" value="TO-220 ON Semiconductor"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="Q2" library="FQP30N06L" package="TO220V" value="FQP30N06L">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" N-Channel 60V 32A _Tc_ 79W _Tc_ Through Hole TO-220-3 "/>
<attribute name="MF" value="ON Semiconductor"/>
<attribute name="MP" value="FQP30N06L"/>
<attribute name="PACKAGE" value="TO-220 ON Semiconductor"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="Q3" library="FQP30N06L" package="TO220V" value="FQP30N06L">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" N-Channel 60V 32A _Tc_ 79W _Tc_ Through Hole TO-220-3 "/>
<attribute name="MF" value="ON Semiconductor"/>
<attribute name="MP" value="FQP30N06L"/>
<attribute name="PACKAGE" value="TO-220 ON Semiconductor"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="Q4" library="FQP30N06L" package="TO220V" value="FQP30N06L">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" N-Channel 60V 32A _Tc_ 79W _Tc_ Through Hole TO-220-3 "/>
<attribute name="MF" value="ON Semiconductor"/>
<attribute name="MP" value="FQP30N06L"/>
<attribute name="PACKAGE" value="TO-220 ON Semiconductor"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="">
<attribute name="SF_SKU" value="PRT-08432"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VIN+">
<contactref element="U$1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="J3" pad="1"/>
<contactref element="C1" pad="C"/>
<contactref element="U$2" pad="1"/>
<contactref element="C2" pad="C"/>
<contactref element="J2" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="Q1" pad="3"/>
<contactref element="Q4" pad="3"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="J9" pad="1"/>
<contactref element="J10" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="3"/>
<contactref element="C1" pad="A"/>
<contactref element="J9" pad="2"/>
</signal>
<signal name="IN3">
<contactref element="J3" pad="5"/>
<contactref element="Q4" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="IN2">
<contactref element="J3" pad="4"/>
<contactref element="Q3" pad="1"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="IN1">
<contactref element="J3" pad="3"/>
<contactref element="Q2" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="IN0">
<contactref element="J3" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="VCCIO">
<contactref element="J3" pad="6"/>
<contactref element="U$2" pad="2"/>
<contactref element="C2" pad="A"/>
</signal>
<signal name="VIN">
<contactref element="U$1" pad="2"/>
<contactref element="J8" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J6" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="J10" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="Q4" pad="2"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="Q3" pad="2"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q2" pad="2"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="2"/>
<contactref element="J5" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
