<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.1">
<drawing>
<board>
<plain>
<wire x1="-1.25" y1="77" x2="20.75" y2="77" width="0" layer="20"/>
<wire x1="20.75" y1="77" x2="20.75" y2="59" width="0" layer="20"/>
<wire x1="20.75" y1="59" x2="-1.25" y2="59" width="0" layer="20"/>
<wire x1="-1.25" y1="59" x2="-1.25" y2="77" width="0" layer="20"/>
<text>GPS BREAKOUT BOARD
uBlox M8 series
SIM28 series</text>
<text>K1FM
rev a</text>
<text>ANTON</text>
<text>VCC_RF</text>
<text>SDA</text>
<text>SCL</text>
<text>RES</text>
<text>EXT_I</text>
<text>TIMEP</text>
<text>RXD</text>
<text>TXD</text>
<text>+</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Ava">
<packages>
<package name="UBLOX_MAX">
<description>uBlox MAX</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="samacsys_parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="1575AT43A0040E">
<description>&lt;b&gt;1575AT43A0040E&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="VALUE"/>
</element>
<element name="GPS1" library="Ava" package="UBLOX_MAX" value="UBLOX_MAX"/>
<element name="GPS-ANT" library="SparkFun-Connectors" package="1X02" value="GPS ANT">
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0603" value="0.47uF">
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
<element name="ANT-CHIP" library="samacsys_parts" package="1575AT43A0040E" value="ANT1">
<attribute name="DESCRIPTION" value="Tri-Band GPS, BDS, and GLNSS, Low Cost, Linearly Polarized, Omnidirectional Chip Antenna"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="JOHANSON TECHNOLOGY"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="1575AT43A0040E"/>
<attribute name="MOUSER_PART_NUMBER" value="609-1575AT43A0040E"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=609-1575AT43A0040E"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="SparkFun-Connectors" package="1X02" value="POWER">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="GPS1" pad="10_GND"/>
<contactref element="GPS1" pad="12_GND"/>
<contactref element="GPS-ANT" pad="1"/>
<contactref element="GPS1" pad="15_RESERVED"/>
<contactref element="C10" pad="2"/>
<contactref element="POWER" pad="2"/>
<contactref element="GPS1" pad="1_GND"/>
</signal>
<signal name="N$6">
<contactref element="GPS1" pad="11_RF_IN"/>
<contactref element="GPS-ANT" pad="2"/>
<contactref element="ANT-CHIP" pad="1"/>
</signal>
<signal name="3V">
<contactref element="GPS1" pad="9_V_RESET"/>
<contactref element="GPS1" pad="8_VCC"/>
<contactref element="GPS1" pad="7_VCC_IO"/>
<contactref element="C10" pad="1"/>
<contactref element="GPS1" pad="6_V_BCKP"/>
<contactref element="POWER" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="GPS1" pad="4_TIMEPULSE"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="GPS1" pad="3_RXD1"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="GPS1" pad="2_TXD1"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="GPS1" pad="5_EXTINT0"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="J1" pad="1"/>
<contactref element="GPS1" pad="18_RESERVED"/>
</signal>
<signal name="N$8">
<contactref element="J1" pad="2"/>
<contactref element="GPS1" pad="17_SCL2"/>
</signal>
<signal name="N$9">
<contactref element="J1" pad="3"/>
<contactref element="GPS1" pad="16_SDA2"/>
</signal>
<signal name="N$10">
<contactref element="GPS1" pad="13_ANTON"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="4"/>
<contactref element="GPS1" pad="14_VCC_RF"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
