<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="13.97" x2="0" y2="46.99" width="0" layer="20"/>
<wire x1="0" y1="46.99" x2="11.43" y2="58.42" width="0" layer="20" curve="-90"/>
<wire x1="11.43" y1="58.42" x2="44.45" y2="58.42" width="0" layer="20"/>
<wire x1="44.45" y1="58.42" x2="54.61" y2="48.26" width="0" layer="20" curve="-90"/>
<wire x1="54.61" y1="48.26" x2="54.61" y2="11.43" width="0" layer="20"/>
<wire x1="54.61" y1="11.43" x2="43.18" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="43.18" y1="0" x2="12.7" y2="0" width="0" layer="20"/>
<wire x1="12.7" y1="0" x2="0" y2="13.97" width="0" layer="20" curve="-95.452618"/>
<text>Kinetis QFP-100 breakout</text>
<text>Power routed to MK24 pins</text>
<text>May be pin compatible with</text>
<text>J-link</text>
<hole x="7.62" y="53.34" drill="3.2"/>
<hole x="7.62" y="5.08" drill="3.2"/>
<hole x="48.26" y="5.08" drill="3.2"/>
<hole x="48.26" y="53.34" drill="3.2"/>
<text>(@'.')@ @('.'@)</text>
<text>some other K series</text>
</plain>
<libraries>
<library name="talkbacksies">
<description>talkbacksies</description>
<packages>
<package name="SINGLE-100MIL-HOLE">
</package>
<package name="0402">
</package>
<package name="JLINK-SEGGER">
</package>
</packages>
</library>
<library name="MK24FN1M0VLL12">
<packages>
<package name="LQFP-100_14X14X1.7">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GND" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="JLINK-5V" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE">
<attribute name="NAME"/>
</element>
<element name="MK24" library="MK24FN1M0VLL12" package="LQFP-100_14X14X1.7" value="MK24FN1M0VLL12">
<attribute name="MANUFACTURER_PART_NUMBER" value="mk24fn1m0vll12"/>
<attribute name="MAXFREQUENCY" value="120"/>
<attribute name="FLASHKB" value="1024"/>
<attribute name="CPU" value="ARM Cortex-M4F"/>
<attribute name="PINCOUNT" value="100"/>
<attribute name="PACKAGE" value="LQFP"/>
<attribute name="SRAMKB" value="256"/>
<attribute name="VENDOR" value="FREESCALE"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWD-CLK-PULLDOWN" library="talkbacksies" package="0402" value="RES-10K-0402">
<attribute name="NAME"/>
</element>
<element name="SWD-DIO-PULLUP" library="talkbacksies" package="0402" value="RES-10K-0402">
<attribute name="NAME"/>
</element>
<element name="SWD-RESET-PULLUP" library="talkbacksies" package="0402" value="RES-10K-0402">
<attribute name="NAME"/>
</element>
<element name="PTE0" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="USB0_DP" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTD7" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="U$102" library="talkbacksies" package="JLINK-SEGGER" value="JLINK-SEGGER"/>
<element name="USB0_DM" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VOUT33" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VREGIN" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="ADC0_DP1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="ADC0_DM1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="ADC1_DP1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="ADC1_DM1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PGA0_DP" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PGA0_DM" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PGA1_DP" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PGA1_DM" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VDDA" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VREFH" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VREFL" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VSSA" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VREF_OUT" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE">
<attribute name="NAME"/>
</element>
<element name="DAC0_OUT" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="XTAL32" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="EXTAL32" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE2" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VBAT" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE24" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE25" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE26" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA0" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA2" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA3" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA4" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA5" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE3" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VDD3" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VSS3" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA12" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA13" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA14" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA15" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA16" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA17" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VDD4" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VSS4" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE4" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA18" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTA19" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="RESET_B" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB0" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB2" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB3" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB9" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB10" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB11" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE5" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VSS5" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VDD5" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB16" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB17" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB18" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB19" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB20" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB21" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB22" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTB23" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTE6" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC0" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC2" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC3" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VSS6" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VDD6" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC4" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC5" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC6" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC7" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VDD" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC8" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC9" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC10" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PCT11" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC12" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC13" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC14" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC15" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VSS7" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VDD7" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VSS" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC16" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC17" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTC18" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTD0" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTD1" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTD2" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTD3" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTD4" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTD5" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="PTD6" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="VCC" library="talkbacksies" package="SINGLE-100MIL-HOLE" value="SINGLE-100MIL-HOLE"/>
<element name="22" library="talkbacksies" package="0402" value="CAP-0.1UF-16V-X7R-0402"/>
<element name="40" library="talkbacksies" package="0402" value="CAP-0.1UF-16V-X7R-0402"/>
<element name="48" library="talkbacksies" package="0402" value="CAP-0.1UF-16V-X7R-0402"/>
<element name="61" library="talkbacksies" package="0402" value="CAP-0.1UF-16V-X7R-0402"/>
<element name="75" library="talkbacksies" package="0402" value="CAP-0.1UF-16V-X7R-0402"/>
<element name="89" library="talkbacksies" package="0402" value="CAP-0.1UF-16V-X7R-0402"/>
</elements>
<signals>
<signal name="VDD">
<contactref element="VDD4" pad="P$1"/>
<contactref element="MK24" pad="48"/>
<contactref element="VDD3" pad="P$1"/>
<contactref element="MK24" pad="40"/>
<contactref element="VDDA" pad="P$1"/>
<contactref element="MK24" pad="22"/>
<contactref element="VDD" pad="P$1"/>
<contactref element="MK24" pad="8"/>
<contactref element="VDD5" pad="P$1"/>
<contactref element="MK24" pad="61"/>
<contactref element="VDD6" pad="P$1"/>
<contactref element="MK24" pad="75"/>
<contactref element="VDD7" pad="P$1"/>
<contactref element="MK24" pad="89"/>
<contactref element="VCC" pad="P$1"/>
<contactref element="U$102" pad="P$1"/>
<contactref element="SWD-DIO-PULLUP" pad="1"/>
<contactref element="SWD-RESET-PULLUP" pad="1"/>
<contactref element="22" pad="1"/>
<contactref element="40" pad="1"/>
<contactref element="48" pad="1"/>
<contactref element="61" pad="1"/>
<contactref element="75" pad="1"/>
<contactref element="89" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="PTE1" pad="P$1"/>
<contactref element="MK24" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="PTE2" pad="P$1"/>
<contactref element="MK24" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="PTE3" pad="P$1"/>
<contactref element="MK24" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="PTE4" pad="P$1"/>
<contactref element="MK24" pad="5"/>
</signal>
<signal name="PTE5">
<contactref element="PTE5" pad="P$1"/>
<contactref element="MK24" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="PTE6" pad="P$1"/>
<contactref element="MK24" pad="7"/>
</signal>
<signal name="N$10">
<contactref element="USB0_DP" pad="P$1"/>
<contactref element="MK24" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="USB0_DM" pad="P$1"/>
<contactref element="MK24" pad="11"/>
</signal>
<signal name="N$12">
<contactref element="VOUT33" pad="P$1"/>
<contactref element="MK24" pad="12"/>
</signal>
<signal name="N$13">
<contactref element="VREGIN" pad="P$1"/>
<contactref element="MK24" pad="13"/>
</signal>
<signal name="N$14">
<contactref element="ADC0_DP1" pad="P$1"/>
<contactref element="MK24" pad="14"/>
</signal>
<signal name="N$15">
<contactref element="ADC0_DM1" pad="P$1"/>
<contactref element="MK24" pad="15"/>
</signal>
<signal name="N$16">
<contactref element="ADC1_DP1" pad="P$1"/>
<contactref element="MK24" pad="16"/>
</signal>
<signal name="N$17">
<contactref element="ADC1_DM1" pad="P$1"/>
<contactref element="MK24" pad="17"/>
</signal>
<signal name="N$18">
<contactref element="PGA0_DP" pad="P$1"/>
<contactref element="MK24" pad="18"/>
</signal>
<signal name="N$19">
<contactref element="PGA0_DM" pad="P$1"/>
<contactref element="MK24" pad="19"/>
</signal>
<signal name="N$20">
<contactref element="PGA1_DP" pad="P$1"/>
<contactref element="MK24" pad="20"/>
</signal>
<signal name="N$21">
<contactref element="PGA1_DM" pad="P$1"/>
<contactref element="MK24" pad="21"/>
</signal>
<signal name="N$23">
<contactref element="VREFH" pad="P$1"/>
<contactref element="MK24" pad="23"/>
</signal>
<signal name="N$24">
<contactref element="VREFL" pad="P$1"/>
<contactref element="MK24" pad="24"/>
</signal>
<signal name="N$26">
<contactref element="VREF_OUT" pad="P$1"/>
<contactref element="MK24" pad="26"/>
</signal>
<signal name="N$27">
<contactref element="DAC0_OUT" pad="P$1"/>
<contactref element="MK24" pad="27"/>
</signal>
<signal name="N$28">
<contactref element="XTAL32" pad="P$1"/>
<contactref element="MK24" pad="28"/>
</signal>
<signal name="N$29">
<contactref element="EXTAL32" pad="P$1"/>
<contactref element="MK24" pad="29"/>
</signal>
<signal name="N$30">
<contactref element="VBAT" pad="P$1"/>
<contactref element="MK24" pad="30"/>
</signal>
<signal name="N$31">
<contactref element="PTE24" pad="P$1"/>
<contactref element="MK24" pad="31"/>
</signal>
<signal name="N$32">
<contactref element="PTE25" pad="P$1"/>
<contactref element="MK24" pad="32"/>
</signal>
<signal name="N$33">
<contactref element="PTE26" pad="P$1"/>
<contactref element="MK24" pad="33"/>
</signal>
<signal name="N$34">
<contactref element="PTA0" pad="P$1"/>
<contactref element="MK24" pad="34"/>
<contactref element="U$102" pad="P$9"/>
<contactref element="SWD-CLK-PULLDOWN" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="PTA1" pad="P$1"/>
<contactref element="MK24" pad="35"/>
</signal>
<signal name="N$36">
<contactref element="PTA2" pad="P$1"/>
<contactref element="MK24" pad="36"/>
<contactref element="U$102" pad="P$13"/>
</signal>
<signal name="N$37">
<contactref element="PTA3" pad="P$1"/>
<contactref element="MK24" pad="37"/>
<contactref element="U$102" pad="P$7"/>
<contactref element="SWD-DIO-PULLUP" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="PTA4" pad="P$1"/>
<contactref element="MK24" pad="38"/>
</signal>
<signal name="N$39">
<contactref element="PTA5" pad="P$1"/>
<contactref element="MK24" pad="39"/>
</signal>
<signal name="N$42">
<contactref element="PTA12" pad="P$1"/>
<contactref element="MK24" pad="42"/>
</signal>
<signal name="N$43">
<contactref element="PTA13" pad="P$1"/>
<contactref element="MK24" pad="43"/>
</signal>
<signal name="N$44">
<contactref element="PTA14" pad="P$1"/>
<contactref element="MK24" pad="44"/>
</signal>
<signal name="N$45">
<contactref element="PTA15" pad="P$1"/>
<contactref element="MK24" pad="45"/>
</signal>
<signal name="N$46">
<contactref element="PTA16" pad="P$1"/>
<contactref element="MK24" pad="46"/>
</signal>
<signal name="N$47">
<contactref element="PTA17" pad="P$1"/>
<contactref element="MK24" pad="47"/>
</signal>
<signal name="N$50">
<contactref element="PTA18" pad="P$1"/>
<contactref element="MK24" pad="50"/>
</signal>
<signal name="N$1">
<contactref element="PTE0" pad="P$1"/>
<contactref element="MK24" pad="1"/>
</signal>
<signal name="N$51">
<contactref element="RESET_B" pad="P$1"/>
<contactref element="U$102" pad="P$15"/>
<contactref element="SWD-RESET-PULLUP" pad="2"/>
<contactref element="MK24" pad="52"/>
</signal>
<signal name="N$52">
<contactref element="PTB0" pad="P$1"/>
<contactref element="MK24" pad="53"/>
</signal>
<signal name="N$53">
<contactref element="PTB1" pad="P$1"/>
<contactref element="MK24" pad="54"/>
</signal>
<signal name="N$54">
<contactref element="PTB2" pad="P$1"/>
<contactref element="MK24" pad="55"/>
</signal>
<signal name="N$55">
<contactref element="PTB3" pad="P$1"/>
<contactref element="MK24" pad="56"/>
</signal>
<signal name="N$56">
<contactref element="PTB9" pad="P$1"/>
<contactref element="MK24" pad="57"/>
</signal>
<signal name="N$57">
<contactref element="PTB10" pad="P$1"/>
<contactref element="MK24" pad="58"/>
</signal>
<signal name="N$58">
<contactref element="PTB11" pad="P$1"/>
<contactref element="MK24" pad="59"/>
</signal>
<signal name="N$61">
<contactref element="PTB16" pad="P$1"/>
<contactref element="MK24" pad="62"/>
</signal>
<signal name="N$62">
<contactref element="PTB17" pad="P$1"/>
<contactref element="MK24" pad="63"/>
</signal>
<signal name="N$63">
<contactref element="PTB18" pad="P$1"/>
<contactref element="MK24" pad="64"/>
</signal>
<signal name="N$64">
<contactref element="PTB19" pad="P$1"/>
<contactref element="MK24" pad="65"/>
</signal>
<signal name="N$65">
<contactref element="PTB20" pad="P$1"/>
<contactref element="MK24" pad="66"/>
</signal>
<signal name="N$66">
<contactref element="PTB21" pad="P$1"/>
<contactref element="MK24" pad="67"/>
</signal>
<signal name="N$67">
<contactref element="PTB22" pad="P$1"/>
<contactref element="MK24" pad="68"/>
</signal>
<signal name="N$68">
<contactref element="PTB23" pad="P$1"/>
<contactref element="MK24" pad="69"/>
</signal>
<signal name="N$69">
<contactref element="PTC0" pad="P$1"/>
<contactref element="MK24" pad="70"/>
</signal>
<signal name="N$70">
<contactref element="PTC1" pad="P$1"/>
<contactref element="MK24" pad="71"/>
</signal>
<signal name="N$71">
<contactref element="PTC2" pad="P$1"/>
<contactref element="MK24" pad="72"/>
</signal>
<signal name="N$72">
<contactref element="PTC3" pad="P$1"/>
<contactref element="MK24" pad="73"/>
</signal>
<signal name="N$75">
<contactref element="PTC4" pad="P$1"/>
<contactref element="MK24" pad="76"/>
</signal>
<signal name="N$76">
<contactref element="PTC5" pad="P$1"/>
<contactref element="MK24" pad="77"/>
</signal>
<signal name="N$77">
<contactref element="PTC6" pad="P$1"/>
<contactref element="MK24" pad="78"/>
</signal>
<signal name="N$78">
<contactref element="PTC7" pad="P$1"/>
<contactref element="MK24" pad="79"/>
</signal>
<signal name="N$79">
<contactref element="PTC8" pad="P$1"/>
<contactref element="MK24" pad="80"/>
</signal>
<signal name="N$80">
<contactref element="PTC9" pad="P$1"/>
<contactref element="MK24" pad="81"/>
</signal>
<signal name="N$81">
<contactref element="PTC10" pad="P$1"/>
<contactref element="MK24" pad="82"/>
</signal>
<signal name="N$82">
<contactref element="PCT11" pad="P$1"/>
<contactref element="MK24" pad="83"/>
</signal>
<signal name="N$83">
<contactref element="PTC12" pad="P$1"/>
<contactref element="MK24" pad="84"/>
</signal>
<signal name="N$84">
<contactref element="PTC13" pad="P$1"/>
<contactref element="MK24" pad="85"/>
</signal>
<signal name="N$85">
<contactref element="PTC14" pad="P$1"/>
<contactref element="MK24" pad="86"/>
</signal>
<signal name="N$86">
<contactref element="PTC15" pad="P$1"/>
<contactref element="MK24" pad="87"/>
</signal>
<signal name="N$89">
<contactref element="PTC16" pad="P$1"/>
<contactref element="MK24" pad="90"/>
</signal>
<signal name="N$90">
<contactref element="PTC17" pad="P$1"/>
<contactref element="MK24" pad="91"/>
</signal>
<signal name="N$91">
<contactref element="PTC18" pad="P$1"/>
<contactref element="MK24" pad="92"/>
</signal>
<signal name="N$92">
<contactref element="PTD0" pad="P$1"/>
<contactref element="MK24" pad="93"/>
</signal>
<signal name="N$93">
<contactref element="PTD1" pad="P$1"/>
<contactref element="MK24" pad="94"/>
</signal>
<signal name="N$94">
<contactref element="PTD2" pad="P$1"/>
<contactref element="MK24" pad="95"/>
</signal>
<signal name="N$95">
<contactref element="PTD3" pad="P$1"/>
<contactref element="MK24" pad="96"/>
</signal>
<signal name="N$96">
<contactref element="PTD4" pad="P$1"/>
<contactref element="MK24" pad="97"/>
</signal>
<signal name="N$97">
<contactref element="PTD5" pad="P$1"/>
<contactref element="MK24" pad="98"/>
</signal>
<signal name="N$98">
<contactref element="PTD6" pad="P$1"/>
<contactref element="MK24" pad="99"/>
</signal>
<signal name="N$99">
<contactref element="PTD7" pad="P$1"/>
<contactref element="MK24" pad="100"/>
</signal>
<signal name="N$100">
<contactref element="PTA19" pad="P$1"/>
<contactref element="MK24" pad="51"/>
</signal>
<signal name="GND">
<contactref element="GND" pad="P$1"/>
<contactref element="U$102" pad="P$4"/>
<contactref element="SWD-CLK-PULLDOWN" pad="1"/>
<contactref element="VSS5" pad="P$1"/>
<contactref element="MK24" pad="60"/>
<contactref element="VSS6" pad="P$1"/>
<contactref element="MK24" pad="74"/>
<contactref element="VSS4" pad="P$1"/>
<contactref element="MK24" pad="49"/>
<contactref element="VSS" pad="P$1"/>
<contactref element="MK24" pad="9"/>
<contactref element="VSSA" pad="P$1"/>
<contactref element="MK24" pad="25"/>
<contactref element="VSS3" pad="P$1"/>
<contactref element="MK24" pad="41"/>
<contactref element="VSS7" pad="P$1"/>
<contactref element="MK24" pad="88"/>
<contactref element="22" pad="2"/>
<contactref element="40" pad="2"/>
<contactref element="48" pad="2"/>
<contactref element="61" pad="2"/>
<contactref element="75" pad="2"/>
<contactref element="89" pad="2"/>
</signal>
<signal name="N$101">
<contactref element="U$102" pad="P$19"/>
<contactref element="JLINK-5V" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
