<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="20.86" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2" y1="0" x2="48.8" y2="0" width="0" layer="20"/>
<wire x1="48.8" y1="0" x2="50.8" y2="2" width="0" layer="20" curve="90"/>
<wire x1="50.8" y1="2" x2="50.8" y2="20.86" width="0" layer="20"/>
<wire x1="50.8" y1="20.86" x2="48.8" y2="22.86" width="0" layer="20" style="dashdot" curve="90"/>
<wire x1="48.8" y1="22.86" x2="2" y2="22.86" width="0" layer="20"/>
<wire x1="2" y1="22.86" x2="0" y2="20.86" width="0" layer="20" curve="90"/>
<text>LoRa</text>
<text>By: Dan Watson
syncchannel.blogspot.com</text>
<text>2/8/2016
Rev A</text>
<text>PWR</text>
<hole x="48.5775" y="20.7645" drill="2.6"/>
<hole x="48.5775" y="2.0955" drill="2.6"/>
<text>DIO0</text>
<text>GND</text>
<text>DIO2</text>
<text>DIO3</text>
<text>DIO5</text>
<text>RFM
RST</text>
<text>DIO4</text>
<text>NSS</text>
<text>DIO1</text>
<text>3.3V</text>
<text>C1</text>
<text>C2</text>
<text>C3</text>
<text>R1</text>
<text>RFM95/96(W)</text>
<text>For Adafruit Feather
RFM95/96(W) FeatherWing</text>
<text>Transceiver</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
<package name="SMA_EDGELAUNCH">
</package>
</packages>
</library>
<library name="adafruit2">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12_NO_SILK">
</package>
<package name="1X16_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
<package name="FIDUCIAL-1X2">
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2,8-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 2.8 mm, round</description>
</package>
</packages>
</library>
<library name="_CustomParts">
<packages>
<package name="RFM95W">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3528">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X05">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="adafruit" package="C0603" value="100nF"/>
<element name="JP1" library="SparkFun-Connectors" package="1X12_NO_SILK" value=""/>
<element name="JP2" library="SparkFun-Connectors" package="1X16_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="RED"/>
<element name="R1" library="adafruit2" package="R0603" value="680"/>
<element name="H1" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="H2" library="holes" package="2,8-PAD" value="MOUNT-PAD-ROUND2.8"/>
<element name="C2" library="adafruit" package="C0603" value="1uF"/>
<element name="U$2" library="_CustomParts" package="RFM95W" value="RFM95W"/>
<element name="X1" library="adafruit" package="SMA_EDGELAUNCH" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="EIA3528" value="47uF">
<attribute name="PROD_ID" value="CAP-08310"/>
</element>
<element name="JP3" library="pinhead" package="2X05" value="">
<attribute name="VALUE"/>
</element>
<element name="FID1" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
<element name="FID2" library="SparkFun-Aesthetics" package="FIDUCIAL-1X2" value="FIDUCIAL1X2"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP2" pad="4"/>
<contactref element="LED2" pad="C"/>
<contactref element="H2" pad="B2,8"/>
<contactref element="H1" pad="B2,8"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$2" pad="P$10"/>
<contactref element="X1" pad="GND@4"/>
<contactref element="X1" pad="GND@3"/>
<contactref element="X1" pad="GND@2"/>
<contactref element="X1" pad="GND@1"/>
<contactref element="C1" pad="C"/>
<contactref element="JP3" pad="3"/>
<contactref element="U$2" pad="P$8"/>
</signal>
<signal name="3V">
<contactref element="JP2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$2" pad="P$13"/>
<contactref element="C1" pad="A"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="LED2" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="JP2" pad="12"/>
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="MISO">
<contactref element="JP2" pad="13"/>
<contactref element="U$2" pad="P$2"/>
</signal>
<signal name="SCK">
<contactref element="JP2" pad="11"/>
<contactref element="U$2" pad="P$4"/>
</signal>
<signal name="NSS">
<contactref element="U$2" pad="P$5"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="RFM_RST">
<contactref element="U$2" pad="P$6"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="DIO5">
<contactref element="U$2" pad="P$7"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="ANT">
<contactref element="U$2" pad="P$9"/>
<contactref element="X1" pad="P"/>
</signal>
<signal name="DIO3">
<contactref element="U$2" pad="P$11"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="DIO4">
<contactref element="U$2" pad="P$12"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="DIO0">
<contactref element="U$2" pad="P$14"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="DIO1">
<contactref element="U$2" pad="P$15"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="DIO2">
<contactref element="U$2" pad="P$16"/>
<contactref element="JP3" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
