<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<text>METER GROUNDS</text>
<text>METER MOVEMENT</text>
<text>LED BACKLIGHT</text>
<text>B17 METER TESTER CAPE</text>
<text>DCA 2/08/18</text>
<text>REV B</text>
<text>B17 METER TESTER TESTS RED AND BLUE
 BACKLIGHTS AND METER MOVEMENT
ON UP TO FOUR METERS AT A TIME.

CONNECTIONS:
M1 - METER 1 MOVEMENT
M1_GND - METER 1 GROUND
M1R - METER 1 RED LED
M1B - METER 1 BLUE LED

SAME PATTERN FOR ALL METERS

</text>
<text>PRESS TO
START/STOP TEST</text>
<text>POWER/STATUS</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="BEAGLEBONE_SHIELD">
</package>
<package name="DO-1N4148">
</package>
</packages>
</library>
<library name="Doug_1">
<packages>
<package name="10MA_CURRENT_REGULATOR">
</package>
</packages>
</library>
<library name="1 Sami MS 010716">
<packages>
<package name="C0603_ST0">
<description>SMD Package 0603 (metric 1608). Footprint STANDARD ST0 - Maximum Clearance between SMDs. 
Chip standard dimensions: L0.063" x W0.031" (L1.60mm x W0.80mm). 
SMD size 0.037.5" x 0.043" (0.9525mm x 1.0922mm). 
SMD coordinates X = +/- 0.03475" (+/- 0.88265mm). 
Clearance between SMDs 0.032" (0.8128mm). 
Package outline dimensions L0.121" x W0.057" (3.0734mm x 1.4478mm).</description>
</package>
<package name="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3">
<description>Pad for 20 AWG stranded wire, dia 0.120", drill 0.052", shape Round - with Outline</description>
</package>
<package name="SOIC-08-0.15&quot;W_ST1">
<description>SOIC-08 Package, 3.9mm (0.153") body width, Standard size footprint ST1;
Device Dimensions max: L5.0mm x W4.0mm (0.19685" x 0.15748");
Device tip to tip dimensions max: 6.2mm (0.2441");
Pitch 1.27mm (0.05");
Leads width max: 0.51mm (0.020");
Lead Landing area max: 0.9mm x 0.51mm (0.03543" x 0.020");
Outline dimensions: L5.2mm x W3.9mm (0.2047" x 0.1535");
SMD size 0.70mm x 1.7mm (0.02756" x 0.06693");
SMDs are located at Y = +/- 2.95mm (0.11614");
Clearance between adjacent SMDs 0.57mm (0.02244");
Clearance between SMDs under device 4.2mm (0.16535").</description>
</package>
<package name="C1206_ST1">
<description>SMD Package 1206 (metric 1608). Footprint STANDARD ST1.
Chip standard dimensions: L0.126" x W0.063" (L3.20mm x W1.60mm). 
SMD size 0.070" x 0.075" (1.778mm x 1.905mm). 
SMD coordinates X = +/- 0.065" (+/-1.651mm). 
Clearance between SMDs 0.060" (1.524mm). 
Package outline dimensions L0.214" x W0.089" (5.4356mm x 2.2606mm).</description>
</package>
</packages>
</library>
<library name="1 Sami MS 081412">
<packages>
<package name="C0603">
</package>
</packages>
</library>
<library name="1 Sami MS">
<packages>
<package name="C0603">
</package>
</packages>
</library>
<library name="1 Sami MS 072716">
<packages>
<package name="C0805_ST0">
<description>SMD Package 0805 (metric 2012). Footprint STANDARD ST0 - Maximum Clearance between SMDs. 
Chip standard dimensions: L0.079" x W0.049" (L2.00mm x W1.25mm). 
SMD size 0.047" x 0.060" (1.1938mm x 1.524mm). 
SMD coordinates X = +/- 0.0435" (+/- 1.1049mm). 
Clearance between SMDs 0.040" (1.016mm). 
Package outline dimensions L0.148" x W0.074" (3.7592mm x 1.8796mm).</description>
</package>
<package name="C0805_ST1">
<description>SMD Package 0805 (metric 2012). Footprint STANDARD ST1. 
Chip standard dimensions: L0.079" x W0.049" (L2.00mm x W1.25mm). 
SMD size 0.052" x 0.060" (1.3208mm x 1.524mm). 
SMD coordinates X = +/- 0.041" (+/- 1.0414mm). 
Clearance between SMDs 0.030" (0.762mm). 
Package outline dimensions L0.148" x W0.074" (3.7592mm x 1.8796mm).</description>
</package>
<package name="CAP-POL_SMD-CASE_6.3X5.5_5.7_5.8_6.3_7.7_8MM-LG*2">
<description>Capacitor, Electrolytic, Aluminum Can type, Surface Mount, Standard (Nominal) Package LG Footprint; Fits NIC_NACE, NIC_NACZ, Jianghai_HVF, Nichicon, Can Sizes (DxL) 6.3x5.5mm, 6.3x5.7mm, 6.3x5.8mm 6.3x6.3mm, 6.3x7.7mm &amp; 6.3x8mm;
SMDs are aligned on X axis; Polarity + sign is under pad;
Device Base Dimensions max : 6.8mm x 6.8mm (0.2677" x 0.2677");
Device Can diameter max: 6.8mm (0.2677");
Outline dimensions: 7.0mm (0.2756") x 7.0mm (0.2756");
Lead Footprint area max: 0.8mm x 3.0mm (0.0315" x 0.11811");
SMD dimensions: 3.7mm x 1.4mm (0.14567" x 0.055118");
SMD locations: +/- 2.7mm (0.1063");
Clearance between SMDs: 1.7mm (0.06693");</description>
</package>
<package name="SOT-23">
<description>SOT23 package, Standard  footprint version. SMD dimensions 0.8mm x 0.9mm (0.0315" x 0.03543").
SMD coordinates: SMD1 &amp; SMD2 = +/- 0.96mm (0.0378"), SMDs 1,2 &amp; SMD3 = +/-1.015mm (0.04").
Clearance between SMD1 &amp; SMD2 = 1.12mm (0.044"), Clearance between SMD1,2 &amp; SMD3 = 1.14mm (0.0448")</description>
</package>
<package name="LOGO_MS-340X177MIL">
<description>MidNite Logo, size X=0.340"  Y=0.177". The M Lower left corner Located at (0, 0). Imported from the main bitmap file badgegrey2 using: Scaled, Mil, and a scale factor of 0.25.</description>
</package>
<package name="SWITCH-TACT_TL3301-6X6MM">
<description>TACT Switch SMT - 6mm x 6mm</description>
</package>
<package name="C0805_LT-OLD">
<description>SMD Package 0805 (metric 2012). Lite Footprint (Old package).
Chip standard dimensions: L0.079" x W0.049" (L2.00mm x W1.25mm). 
SMD size 0.035" x 0.056" (0.889mm x 1.4224mm). 
SMD coordinates X = +/- 0.0375" (+/- 0.9525mm). 
Clearance between SMDs 0.040" (1.016mm). 
Package outline dimensions L0.125" x W0.071" (3.175mm x 1.8034mm).</description>
</package>
</packages>
</library>
<library name="zetex">
<description>&lt;b&gt;Zetex Power MOS FETs, Bridges, Diodes&lt;/b&gt;&lt;p&gt;
http://www.zetex.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT-23">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="adafruit" package="BEAGLEBONE_SHIELD" value="BEAGLEBONE_OUTLINE">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="Doug_1" package="10MA_CURRENT_REGULATOR" value="NSI50010YT1G">
<attribute name="DESC" value="10ma Current Regulator"/>
<attribute name="PACK" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q9" library="1 Sami MS 072716" package="SOT-23" value="MMBT2907A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="1 Sami MS 010716" package="C0603_ST0" value="10R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="R20" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="M1R" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="Q2" library="Doug_1" package="10MA_CURRENT_REGULATOR" value="NSI50010YT1G">
<attribute name="DESC" value="10ma Current Regulator"/>
<attribute name="PACK" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q10" library="1 Sami MS 072716" package="SOT-23" value="MMBT2907A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="1 Sami MS 010716" package="C0603_ST0" value="10R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="R21" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="M1B" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="Q3" library="Doug_1" package="10MA_CURRENT_REGULATOR" value="NSI50010YT1G">
<attribute name="DESC" value="10ma Current Regulator"/>
<attribute name="PACK" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q11" library="1 Sami MS 072716" package="SOT-23" value="MMBT2907A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="1 Sami MS 010716" package="C0603_ST0" value="10R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="R22" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="M2R" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="Q4" library="Doug_1" package="10MA_CURRENT_REGULATOR" value="NSI50010YT1G">
<attribute name="DESC" value="10ma Current Regulator"/>
<attribute name="PACK" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q12" library="1 Sami MS 072716" package="SOT-23" value="MMBT2907A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="1 Sami MS 010716" package="C0603_ST0" value="10R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="R23" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="M2B" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="Q5" library="Doug_1" package="10MA_CURRENT_REGULATOR" value="NSI50010YT1G">
<attribute name="DESC" value="10ma Current Regulator"/>
<attribute name="PACK" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q13" library="1 Sami MS 072716" package="SOT-23" value="MMBT2907A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="1 Sami MS 010716" package="C0603_ST0" value="10R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="R24" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="M3R" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="Q6" library="Doug_1" package="10MA_CURRENT_REGULATOR" value="NSI50010YT1G">
<attribute name="DESC" value="10ma Current Regulator"/>
<attribute name="PACK" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q14" library="1 Sami MS 072716" package="SOT-23" value="MMBT2907A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="1 Sami MS 010716" package="C0603_ST0" value="10R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="R25" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="M3B" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="Q7" library="Doug_1" package="10MA_CURRENT_REGULATOR" value="NSI50010YT1G">
<attribute name="DESC" value="10ma Current Regulator"/>
<attribute name="PACK" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q15" library="1 Sami MS 072716" package="SOT-23" value="MMBT2907A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="1 Sami MS 010716" package="C0603_ST0" value="10R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="R26" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="M4R" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="Q8" library="Doug_1" package="10MA_CURRENT_REGULATOR" value="NSI50010YT1G">
<attribute name="DESC" value="10ma Current Regulator"/>
<attribute name="PACK" value=""/>
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q16" library="1 Sami MS 072716" package="SOT-23" value="MMBT2907A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="1 Sami MS 010716" package="C0603_ST0" value="10R0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="R27" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="M4B" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="M4_GND" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="M3_GND" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="M2_GND" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="M1_GND" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="M1" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="BP_M1+">
<attribute name="NAME"/>
</element>
<element name="M2" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="BP_M2+">
<attribute name="NAME"/>
</element>
<element name="M3" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="BP_M2+">
<attribute name="NAME"/>
</element>
<element name="M4" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="BP_M4+">
<attribute name="NAME"/>
</element>
<element name="R1" library="1 Sami MS 081412" package="C0603" value="3K0">
<attribute name="DESC" value="Resistor, 10K Ohm, 1%, 0.1W, SMD Package 0603, Yageo RC0603FR-0710KL or Nippon NRC06F1002TRF"/>
<attribute name="PN" value="4-118-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="1 Sami MS 081412" package="C0603" value="1K0">
<attribute name="DESC" value="Resistor, 1K, 1%, 0.1W, SMD Package 0603, Yageo RC0603FR-071KL"/>
<attribute name="PN" value="4-111-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="1 Sami MS" package="C0603" value="0.1uF">
<attribute name="DESC" value="Capacitor, 0.1uF 50V, X7R, SMD Package 0603, AVX 06035C104KAT2A or Nippon NMC0603X7R104K50RPF"/>
<attribute name="PN" value="2-058-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="1 Sami MS 081412" package="C0603" value="3K0">
<attribute name="DESC" value="Resistor, 10K Ohm, 1%, 0.1W, SMD Package 0603, Yageo RC0603FR-0710KL or Nippon NRC06F1002TRF"/>
<attribute name="PN" value="4-118-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="1 Sami MS 081412" package="C0603" value="1K0">
<attribute name="DESC" value="Resistor, 1K, 1%, 0.1W, SMD Package 0603, Yageo RC0603FR-071KL"/>
<attribute name="PN" value="4-111-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="1 Sami MS" package="C0603" value="0.1uF">
<attribute name="DESC" value="Capacitor, 0.1uF 50V, X7R, SMD Package 0603, AVX 06035C104KAT2A or Nippon NMC0603X7R104K50RPF"/>
<attribute name="PN" value="2-058-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="1 Sami MS 081412" package="C0603" value="3K0">
<attribute name="DESC" value="Resistor, 10K Ohm, 1%, 0.1W, SMD Package 0603, Yageo RC0603FR-0710KL or Nippon NRC06F1002TRF"/>
<attribute name="PN" value="4-118-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="1 Sami MS 081412" package="C0603" value="1K0">
<attribute name="DESC" value="Resistor, 1K, 1%, 0.1W, SMD Package 0603, Yageo RC0603FR-071KL"/>
<attribute name="PN" value="4-111-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="1 Sami MS" package="C0603" value="0.1uF">
<attribute name="DESC" value="Capacitor, 0.1uF 50V, X7R, SMD Package 0603, AVX 06035C104KAT2A or Nippon NMC0603X7R104K50RPF"/>
<attribute name="PN" value="2-058-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="1 Sami MS 081412" package="C0603" value="3K0">
<attribute name="DESC" value="Resistor, 10K Ohm, 1%, 0.1W, SMD Package 0603, Yageo RC0603FR-0710KL or Nippon NRC06F1002TRF"/>
<attribute name="PN" value="4-118-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="1 Sami MS 081412" package="C0603" value="1K0">
<attribute name="DESC" value="Resistor, 1K, 1%, 0.1W, SMD Package 0603, Yageo RC0603FR-071KL"/>
<attribute name="PN" value="4-111-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="1 Sami MS" package="C0603" value="0.1uF">
<attribute name="DESC" value="Capacitor, 0.1uF 50V, X7R, SMD Package 0603, AVX 06035C104KAT2A or Nippon NMC0603X7R104K50RPF"/>
<attribute name="PN" value="2-058-1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="1 Sami MS 072716" package="CAP-POL_SMD-CASE_6.3X5.5_5.7_5.8_6.3_7.7_8MM-LG*2" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="1 Sami MS 072716" package="CAP-POL_SMD-CASE_6.3X5.5_5.7_5.8_6.3_7.7_8MM-LG*2" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="1 Sami MS 072716" package="C0805_ST1" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="1 Sami MS 072716" package="C0805_ST1" value=".1uf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="1 Sami MS 072716" package="C0805_ST1" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="1 Sami MS 072716" package="C0805_ST1" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="1 Sami MS 072716" package="LOGO_MS-340X177MIL" value=""/>
<element name="SW1" library="1 Sami MS 072716" package="SWITCH-TACT_TL3301-6X6MM" value="SWITCH-PUSH_BUTTON-SPST_4PIN2TACT_TL3301_GULL-6X6MM-CONN1&amp;2_3&amp;4">
<attribute name="NAME"/>
</element>
<element name="R19" library="1 Sami MS 010716" package="C0603_ST0" value="10K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="1 Sami MS 072716" package="C0805_LT-OLD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value="1-133-1"/>
</element>
<element name="R36" library="1 Sami MS 010716" package="C0603_ST0" value="RESISTORC0603-ST0/FOL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="PN" value=""/>
</element>
<element name="C14" library="1 Sami MS 072716" package="C0805_ST0" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SYS_5V" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="LED_SUPPLY" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="SYS_GND" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
<element name="U1" library="1 Sami MS 010716" package="SOIC-08-0.15&quot;W_ST1" value="IC-TIMER_NE5551SOIC8-0.15&quot;W-ST">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="1 Sami MS 010716" package="C0603_ST0" value="1K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="1 Sami MS 010716" package="C0603_ST0" value="22K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="1 Sami MS 072716" package="C0805_ST1" value=".01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="1 Sami MS 010716" package="C1206_ST1" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="adafruit" package="DO-1N4148" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="adafruit" package="DO-1N4148" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q24" library="zetex" package="SOT-23" value="">
<attribute name="OC_NEWARK" value="25R4555"/>
<attribute name="MPN" value="DSS20201L-7"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1710688"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R11" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q23" library="zetex" package="SOT-23" value="">
<attribute name="OC_NEWARK" value="25R4555"/>
<attribute name="MPN" value="DSS20201L-7"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1710688"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q22" library="zetex" package="SOT-23" value="">
<attribute name="OC_NEWARK" value="25R4555"/>
<attribute name="MPN" value="DSS20201L-7"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1710688"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q21" library="zetex" package="SOT-23" value="">
<attribute name="OC_NEWARK" value="25R4555"/>
<attribute name="MPN" value="DSS20201L-7"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1710688"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q20" library="zetex" package="SOT-23" value="">
<attribute name="OC_NEWARK" value="25R4555"/>
<attribute name="MPN" value="DSS20201L-7"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1710688"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q19" library="zetex" package="SOT-23" value="">
<attribute name="OC_NEWARK" value="25R4555"/>
<attribute name="MPN" value="DSS20201L-7"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1710688"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q18" library="zetex" package="SOT-23" value="">
<attribute name="OC_NEWARK" value="25R4555"/>
<attribute name="MPN" value="DSS20201L-7"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1710688"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="Q17" library="zetex" package="SOT-23" value="">
<attribute name="OC_NEWARK" value="25R4555"/>
<attribute name="MPN" value="DSS20201L-7"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1710688"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R14" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="1 Sami MS 010716" package="C0603_ST0" value="47K0">
<attribute name="PN" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="1 Sami MS 010716" package="C1206_ST1" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+8V" library="1 Sami MS 010716" package="PAD_DI120-DR52_RND-20AWG_STR_WIRE*3" value="">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="47"/>
<contactref element="U$1" pad="48"/>
<contactref element="U$1" pad="89"/>
<contactref element="U$1" pad="90"/>
<contactref element="U$1" pad="91"/>
<contactref element="U$1" pad="92"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$1" pad="47"/>
<contactref element="U$1" pad="48"/>
<contactref element="U$1" pad="89"/>
<contactref element="U$1" pad="91"/>
<contactref element="U$1" pad="90"/>
<contactref element="U$1" pad="92"/>
<contactref element="M1_GND" pad="1"/>
<contactref element="M2_GND" pad="1"/>
<contactref element="M3_GND" pad="1"/>
<contactref element="M4_GND" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="C1" pad="NEG"/>
<contactref element="C10" pad="2"/>
<contactref element="C2" pad="NEG"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="SYS_GND" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="Q24" pad="2"/>
<contactref element="Q23" pad="2"/>
<contactref element="Q17" pad="2"/>
<contactref element="Q18" pad="2"/>
<contactref element="Q19" pad="2"/>
<contactref element="Q20" pad="2"/>
<contactref element="Q21" pad="2"/>
<contactref element="Q22" pad="2"/>
</signal>
<signal name="VDD_3V3EXP">
<contactref element="U$1" pad="50"/>
</signal>
<signal name="VDD_5V">
<contactref element="U$1" pad="51"/>
<contactref element="U$1" pad="52"/>
</signal>
<signal name="AIN0">
<contactref element="U$1" pad="85"/>
</signal>
<signal name="N$2">
<contactref element="Q9" pad="3"/>
<contactref element="R28" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R28" pad="2"/>
<contactref element="M1R" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="Q9" pad="1"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="4"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="Q10" pad="3"/>
<contactref element="R29" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R29" pad="2"/>
<contactref element="M1B" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="Q10" pad="1"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="Q11" pad="3"/>
<contactref element="R30" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R30" pad="2"/>
<contactref element="M2R" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="Q11" pad="1"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="12"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="Q12" pad="3"/>
<contactref element="R31" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R31" pad="2"/>
<contactref element="M2B" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="Q12" pad="1"/>
<contactref element="R23" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="Q13" pad="3"/>
<contactref element="R32" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R32" pad="2"/>
<contactref element="M3R" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="Q13" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="R24" pad="1"/>
<contactref element="Q21" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="Q14" pad="3"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R33" pad="2"/>
<contactref element="M3B" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="Q14" pad="1"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="Q15" pad="3"/>
<contactref element="R34" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="R34" pad="2"/>
<contactref element="M4R" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="Q15" pad="1"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="N$35">
<contactref element="R26" pad="1"/>
<contactref element="Q23" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="Q16" pad="3"/>
<contactref element="R35" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R35" pad="2"/>
<contactref element="M4B" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="Q16" pad="1"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="U$1" pad="22"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="LED_SUPPLY">
<contactref element="Q8" pad="P$2_ANODE"/>
<contactref element="Q1" pad="P$2_ANODE"/>
<contactref element="Q2" pad="P$2_ANODE"/>
<contactref element="Q3" pad="P$2_ANODE"/>
<contactref element="Q4" pad="P$2_ANODE"/>
<contactref element="Q5" pad="P$2_ANODE"/>
<contactref element="Q6" pad="P$2_ANODE"/>
<contactref element="Q7" pad="P$2_ANODE"/>
<contactref element="C1" pad="POS"/>
<contactref element="C10" pad="1"/>
<contactref element="LED_SUPPLY" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="Q8" pad="P$1_CATHODE"/>
<contactref element="Q16" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="Q1" pad="P$1_CATHODE"/>
<contactref element="Q9" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="Q2" pad="P$1_CATHODE"/>
<contactref element="Q10" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="Q3" pad="P$1_CATHODE"/>
<contactref element="Q11" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="Q4" pad="P$1_CATHODE"/>
<contactref element="Q12" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="Q5" pad="P$1_CATHODE"/>
<contactref element="Q13" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="Q6" pad="P$1_CATHODE"/>
<contactref element="Q14" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="Q7" pad="P$1_CATHODE"/>
<contactref element="Q15" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="R23" pad="1"/>
<contactref element="Q20" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="R25" pad="1"/>
<contactref element="Q22" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="U$1" pad="6"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="BP_M1+">
<contactref element="R1" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="M1" pad="1"/>
</signal>
<signal name="METER_DRIVE_1">
<contactref element="R1" pad="2"/>
<contactref element="U$1" pad="60"/>
</signal>
<signal name="METER_DRIVE_2">
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="62"/>
</signal>
<signal name="METER_DRIVE_3">
<contactref element="R3" pad="2"/>
<contactref element="U$1" pad="19"/>
</signal>
<signal name="METER_DRIVE_4">
<contactref element="R4" pad="2"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="BP_M2+">
<contactref element="R2" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="M2" pad="1"/>
</signal>
<signal name="BP_M3+">
<contactref element="R3" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="M3" pad="1"/>
</signal>
<signal name="BP_M4+">
<contactref element="R4" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="M4" pad="1"/>
</signal>
<signal name="I2C2_SCL">
<contactref element="U$1" pad="65"/>
</signal>
<signal name="I2C2_SDA">
<contactref element="U$1" pad="66"/>
</signal>
<signal name="3.3V_SUPPLY">
<contactref element="U$1" pad="49"/>
<contactref element="C2" pad="POS"/>
<contactref element="C9" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="START_TEST">
<contactref element="R19" pad="2"/>
<contactref element="U$1" pad="43"/>
<contactref element="SW1" pad="3"/>
<contactref element="SW1" pad="4"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="D3" pad="1"/>
<contactref element="R36" pad="2"/>
</signal>
<signal name="PILOT_LIGHT">
<contactref element="R36" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="SYS_5V">
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="4"/>
<contactref element="R10" pad="1"/>
<contactref element="D1" pad="A"/>
<contactref element="C13" pad="1"/>
<contactref element="U$1" pad="53"/>
<contactref element="SYS_5V" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="7"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$45">
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="2"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="U1" pad="3"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="C12" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="8V_SUPPLY">
<contactref element="D2" pad="C"/>
<contactref element="C13" pad="2"/>
<contactref element="+8V" pad="1"/>
</signal>
<signal name="N$47">
<contactref element="R11" pad="2"/>
<contactref element="Q24" pad="3"/>
</signal>
<signal name="N$48">
<contactref element="Q24" pad="1"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$49">
<contactref element="U$1" pad="20"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="R12" pad="2"/>
<contactref element="Q23" pad="3"/>
</signal>
<signal name="N$51">
<contactref element="U$1" pad="18"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="U$1" pad="16"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$53">
<contactref element="U$1" pad="14"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="N$54">
<contactref element="R22" pad="1"/>
<contactref element="Q19" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="R14" pad="2"/>
<contactref element="Q22" pad="3"/>
</signal>
<signal name="N$59">
<contactref element="Q21" pad="3"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="Q20" pad="3"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="Q19" pad="3"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$61">
<contactref element="R21" pad="1"/>
<contactref element="Q18" pad="1"/>
</signal>
<signal name="N$62">
<contactref element="R18" pad="1"/>
<contactref element="Q18" pad="3"/>
</signal>
<signal name="N$63">
<contactref element="R20" pad="1"/>
<contactref element="Q17" pad="1"/>
</signal>
<signal name="N$64">
<contactref element="R13" pad="1"/>
<contactref element="Q17" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
