<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="52.3" y1="29.01" x2="1.04" y2="29.01" width="0" layer="20"/>
<wire x1="1.04" y1="29.01" x2="1.04" y2="1" width="0" layer="20"/>
<wire x1="1.04" y1="1" x2="52.3" y2="1" width="0" layer="20"/>
<wire x1="52.3" y1="1" x2="52.3" y2="29.01" width="0" layer="20"/>
<text>GND</text>
<text>5V</text>
<text>3.3V</text>
<text>Vin</text>
<text>RST</text>
<text>GND</text>
<text>A0</text>
<text>A1</text>
<text>~5</text>
<text>4</text>
<text>~11</text>
<text>~10</text>
<text>~9</text>
<text>8</text>
<text>7</text>
<text>~6</text>
<text>12</text>
<text>13</text>
<text>ATTINY PROGRAMMER</text>
<text>ATTINY PROGRAMMER</text>
<text>Rev 7</text>
<text>Designed by:  MrSwirlyEyes</text>
</plain>
<libraries>
<library name="PiB_leds">
<packages>
<package name="LEDC2012X120_LED-0805">
<description>CHIP, 2 X 1.25 X 1.2 mm body
&lt;p&gt;CHIP package with body size 2 X 1.25 X 1.2 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_connectors">
<packages>
<package name="HDRV2W64P254_1X2_508X254X838B">
<description>Single-row, 2-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 5.08 X 2.54 X 8.38 mm body
&lt;p&gt;Single-row (1X2), 2-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with overall size 5.08 X 2.54 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
<package name="1X04-VERT-MALE">
</package>
<package name="HDRV6W64P254_1X6_1524X254X838B">
<description>Single-row, 6-pin Pin Header (Male) Straight, 2.54 mm (0.10 in) col pitch, 5.84 mm mating length, 15.24 X 2.54 X 8.38 mm body
&lt;p&gt;Single-row (1X6), 6-pin Pin Header (Male) Straight package with 2.54 mm (0.10 in) col pitch, 0.64 mm lead width, 3.05 mm tail length and 5.84 mm mating length with overall size 15.24 X 2.54 X 8.38 mm, pin pattern - clockwise from top left&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_resistors">
<packages>
<package name="RESC2012X60_SMD-0805">
<description>CHIP, 2 X 1.25 X 0.6 mm body
&lt;p&gt;CHIP package with body size 2 X 1.25 X 0.6 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_capacitors">
<packages>
<package name="_AE_PTH-DIA5-LS2-H5">
</package>
</packages>
</library>
<library name="PiB_ic_microcontrollers">
<packages>
<package name="DIP787W45P254L831H533Q8B_DIP-8_CONNECTOR">
<description>8-DIP, 2.54 mm (0.10 in) pitch, 7.874 mm (0.31 in) span, 8.3185 X 6.604 X 5.334 mm body
&lt;p&gt;8-pin DIP package with 2.54 mm (0.10 in) pitch, 7.874 mm (0.31 in) span with body size 8.3185 X 6.604 X 5.334 mm&lt;/p&gt;</description>
</package>
<package name="DIP794W46P254L1919H533Q14B_DIP-14_CONNECTOR">
<description>14-DIP, 2.54 mm (0.10 in) pitch, 7.94 mm (0.31 in) span, 19.19 X 6.605 X 5.33 mm body
&lt;p&gt;14-pin DIP package with 2.54 mm (0.10 in) pitch, 7.94 mm (0.31 in) span with body size 19.19 X 6.605 X 5.33 mm&lt;/p&gt;</description>
</package>
<package name="DIP794W46P254L1919H533Q14B">
<description>14-DIP, 2.54 mm (0.10 in) pitch, 7.94 mm (0.31 in) span, 19.19 X 6.605 X 5.33 mm body
&lt;p&gt;14-pin DIP package with 2.54 mm (0.10 in) pitch, 7.94 mm (0.31 in) span with body size 19.19 X 6.605 X 5.33 mm&lt;/p&gt;</description>
</package>
<package name="DIP794W46P254L2573H533Q20B_DIP-20_CONNECTOR">
<description>20-DIP, 2.54 mm (0.10 in) pitch, 7.94 mm (0.31 in) span, 25.735 X 6.605 X 5.33 mm body
&lt;p&gt;20-pin DIP package with 2.54 mm (0.10 in) pitch, 7.94 mm (0.31 in) span with body size 25.735 X 6.605 X 5.33 mm&lt;/p&gt;</description>
</package>
<package name="DIP794W46P254L2573H533Q20B">
<description>20-DIP, 2.54 mm (0.10 in) pitch, 7.94 mm (0.31 in) span, 25.735 X 6.605 X 5.33 mm body
&lt;p&gt;20-pin DIP package with 2.54 mm (0.10 in) pitch, 7.94 mm (0.31 in) span with body size 25.735 X 6.605 X 5.33 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="PiB_logo">
<packages>
<package name="PIB-LOGO">
</package>
<package name="MRSWIRLYEYES-LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="PiB_capacitors" package="_AE_PTH-DIA5-LS2-H5" value="10uF/50V">
<attribute name="DATASHEET" value="https://industrial.panasonic.com/cdbs/www-data/pdf/RDF0000/ABA0000C1050.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en/capacitors/aluminum-electrolytic-capacitors/58?k=P828-ND"/>
<attribute name="DISTPN" value="P828-ND"/>
<attribute name="MFR" value="Panasonic Electronic Components"/>
<attribute name="MPN" value="ECE-A1HKA100"/>
</element>
<element name="ATTINYX4" library="PiB_ic_microcontrollers" package="DIP794W46P254L1919H533Q14B_DIP-14_CONNECTOR" value="ATtiny84">
<attribute name="DATASHEET" value="ATTINY24A,44A,84A Complete"/>
<attribute name="DATASHEET_CONNECTOR" value="http://www.assmann-wsw.com/fileadmin/datasheets/ASS_0810_CO.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=ATTINY84A-PU-ND"/>
<attribute name="DISTLINK_CONNECTOR" value="https://www.digikey.com/products/en?keywords=AE9989-ND"/>
<attribute name="DISTPN" value="ATTINY84A-PU-ND"/>
<attribute name="DISTPN_CONNECTOR" value="AE9989-ND"/>
<attribute name="DIST_CONNECTOR" value="Digikey"/>
<attribute name="MFR" value="Microchip Technology"/>
<attribute name="MFR_CONNECTOR" value="Assmann WSW Components"/>
<attribute name="MPN" value="ATTINY84A-PU"/>
<attribute name="MPN_CONNECTOR" value="A 14-LC-TT"/>
<attribute name="VALUE" value="ATtiny84"/>
</element>
<element name="ATTINYX5" library="PiB_ic_microcontrollers" package="DIP787W45P254L831H533Q8B_DIP-8_CONNECTOR" value="ATtiny85">
<attribute name="DATASHEET" value="http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en589893"/>
<attribute name="DATASHEET_CONNECTOR" value="http://www.assmann-wsw.com/fileadmin/datasheets/ASS_0810_CO.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=ATTINY85-20PU-ND"/>
<attribute name="DISTLINK_CONNECTOR" value="https://www.digikey.com/products/en?keywords=AE9986-ND"/>
<attribute name="DISTPN" value="ATTINY85-20PU-ND"/>
<attribute name="DISTPN_CONNECTOR" value="AE9986-ND"/>
<attribute name="DIST_CONNECTOR" value="Digikey"/>
<attribute name="MFR" value="Microchip Technology"/>
<attribute name="MFR_CONNECTOR" value="Assmann WSW Components"/>
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="MPN_CONNECTOR" value="A 08-LC-TT"/>
<attribute name="VALUE" value="ATtiny85"/>
</element>
<element name="ATTINYX313" library="PiB_ic_microcontrollers" package="DIP794W46P254L2573H533Q20B_DIP-20_CONNECTOR" value="ATtiny4313">
<attribute name="DATASHEET" value="http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en590457"/>
<attribute name="DATASHEET_CONNECTOR" value="http://www.assmann-wsw.com/fileadmin/datasheets/ASS_0810_CO.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=ATTINY4313-PU-ND"/>
<attribute name="DISTLINK_CONNECTOR" value="https://www.digikey.com/products/en?keywords=AE9998-ND"/>
<attribute name="DISTPN" value="ATTINY4313-PU-ND"/>
<attribute name="DISTPN_CONNECTOR" value="AE9998-ND"/>
<attribute name="DIST_CONNECTOR" value="Digikey"/>
<attribute name="MFR" value="Microchip Technology"/>
<attribute name="MFR_CONNECTOR" value="Assmann WSW Components"/>
<attribute name="MPN" value="ATTINY4313-PU"/>
<attribute name="MPN_CONNECTOR" value="A 20-LC-TT"/>
<attribute name="VALUE" value="ATtiny4313"/>
</element>
<element name="LED1" library="PiB_leds" package="LEDC2012X120_LED-0805" value="BLUE">
<attribute name="DATASHEET" value="http://optoelectronics.liteon.com/upload/download/DS-22-99-0226/LTST-C170TBKT.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=160-1579-1-ND"/>
<attribute name="DISTPN" value="160-1579-1-ND"/>
<attribute name="MFR" value="Lite-On Inc."/>
<attribute name="MPN" value="LTST-C170TBKT"/>
</element>
<element name="R1" library="PiB_resistors" package="RESC2012X60_SMD-0805" value="10K">
<attribute name="DATASHEET" value="http://www.yageo.com/documents/recent/PYu-RC_Group_51_RoHS_L_9.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=311-10KARCT-ND"/>
<attribute name="DISTPN" value="311-10KARCT-ND"/>
<attribute name="MFR" value="Yageo"/>
<attribute name="MPN" value="RC0805JR-0710KL"/>
</element>
<element name="ANALOG" library="PiB_connectors" package="HDRV2W64P254_1X2_508X254X838B" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://drawings-pdf.s3.amazonaws.com/C10436.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=S1012E-02-ND"/>
<attribute name="DISTPN" value="S1012E-02-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PEC02SAAN"/>
<attribute name="VALUE" value="PTH VERT MALE"/>
</element>
<element name="LOWER_DIGITAL" library="PiB_connectors" package="1X04-VERT-MALE" value="1x04 VERT MALE">
<attribute name="DATASHEET" value="http://www.sullinscorp.com/catalogs/77_PAGE108-109_.100_MALE_HDR.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=PEC04SAAN"/>
<attribute name="DISTPN" value="S1012E-04-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PEC04SAAN"/>
</element>
<element name="POWER" library="PiB_connectors" package="HDRV6W64P254_1X6_1524X254X838B" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://drawings-pdf.s3.amazonaws.com/C10436.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=PEC06SAAN"/>
<attribute name="DISTPN" value="S1012E-06-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PEC06SAAN"/>
</element>
<element name="UPPER_DIGITAL" library="PiB_connectors" package="HDRV6W64P254_1X6_1524X254X838B" value="PTH VERT MALE">
<attribute name="DATASHEET" value="https://drawings-pdf.s3.amazonaws.com/C10436.pdf"/>
<attribute name="DIST" value="Digikey"/>
<attribute name="DISTLINK" value="https://www.digikey.com/products/en?keywords=PEC06SAAN"/>
<attribute name="DISTPN" value="S1012E-06-ND"/>
<attribute name="MFR" value="Sullins Connector Solutions"/>
<attribute name="MPN" value="PEC06SAAN"/>
</element>
<element name="U$1" library="PiB_logo" package="PIB-LOGO" value=""/>
<element name="U$2" library="PiB_logo" package="MRSWIRLYEYES-LOGO" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="ATTINYX313" pad="10"/>
<contactref element="ATTINYX5" pad="4"/>
<contactref element="ATTINYX4" pad="14"/>
<contactref element="POWER" pad="4"/>
<contactref element="POWER" pad="5"/>
<contactref element="C1" pad="-"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SS">
<contactref element="ATTINYX5" pad="1"/>
<contactref element="ATTINYX4" pad="4"/>
<contactref element="ATTINYX313" pad="1"/>
<contactref element="UPPER_DIGITAL" pad="4"/>
</signal>
<signal name="RESET">
<contactref element="C1" pad="+"/>
<contactref element="POWER" pad="1"/>
</signal>
<signal name="5V">
<contactref element="ATTINYX313" pad="20"/>
<contactref element="ATTINYX4" pad="1"/>
<contactref element="ATTINYX5" pad="8"/>
<contactref element="LED1" pad="A"/>
<contactref element="POWER" pad="3"/>
</signal>
<signal name="A1">
<contactref element="ANALOG" pad="2"/>
</signal>
<signal name="A0">
<contactref element="ANALOG" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="ATTINYX5" pad="5"/>
<contactref element="ATTINYX4" pad="7"/>
<contactref element="ATTINYX313" pad="17"/>
<contactref element="UPPER_DIGITAL" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="ATTINYX5" pad="6"/>
<contactref element="ATTINYX4" pad="8"/>
<contactref element="ATTINYX313" pad="18"/>
<contactref element="UPPER_DIGITAL" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="ATTINYX5" pad="7"/>
<contactref element="ATTINYX4" pad="9"/>
<contactref element="ATTINYX313" pad="19"/>
<contactref element="UPPER_DIGITAL" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="LED1" pad="K"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="D6">
<contactref element="LOWER_DIGITAL" pad="2"/>
</signal>
<signal name="D7">
<contactref element="LOWER_DIGITAL" pad="1"/>
</signal>
<signal name="D9">
<contactref element="UPPER_DIGITAL" pad="5"/>
</signal>
<signal name="D8">
<contactref element="UPPER_DIGITAL" pad="6"/>
</signal>
<signal name="D5">
<contactref element="LOWER_DIGITAL" pad="3"/>
</signal>
<signal name="D4">
<contactref element="LOWER_DIGITAL" pad="4"/>
</signal>
<signal name="VIN">
<contactref element="POWER" pad="6"/>
</signal>
<signal name="3.3V">
<contactref element="POWER" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
