<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="3.74205625" y1="10.244253125" x2="3.13245625" y2="11.463453125" width="0.254" layer="20"/>
<wire x1="3.13245625" y1="11.463453125" x2="2.37043125" y2="17.085384375" width="0.254" layer="20"/>
<wire x1="2.37043125" y1="17.085384375" x2="2.742946875" y2="18.253709375" width="0.254" layer="20"/>
<wire x1="2.742946875" y1="18.253709375" x2="11.26045625" y2="25.687453125" width="0.254" layer="20"/>
<wire x1="11.26045625" y1="25.687453125" x2="11.26045625" y2="26.093853125" width="0.254" layer="20"/>
<wire x1="11.26045625" y1="26.093853125" x2="11.05725625" y2="28.938653125" width="0.254" layer="20"/>
<wire x1="11.05725625" y1="28.938653125" x2="11.26045625" y2="29.548253125" width="0.254" layer="20"/>
<wire x1="11.26045625" y1="29.548253125" x2="20.60765625" y2="38.285853125" width="0.254" layer="20"/>
<wire x1="20.60765625" y1="38.285853125" x2="20.60765625" y2="38.895453125" width="0.254" layer="20"/>
<wire x1="20.60765625" y1="38.895453125" x2="20.81085625" y2="41.333853125" width="0.254" layer="20"/>
<wire x1="20.81085625" y1="41.333853125" x2="21.01405625" y2="41.943453125" width="0.254" layer="20"/>
<wire x1="21.01405625" y1="41.943453125" x2="21.21725625" y2="42.349853125" width="0.254" layer="20"/>
<wire x1="21.21725625" y1="42.349853125" x2="28.53245625" y2="46.820253125" width="0.254" layer="20"/>
<wire x1="28.53245625" y1="46.820253125" x2="28.53245625" y2="47.226653125" width="0.254" layer="20"/>
<wire x1="28.53245625" y1="47.226653125" x2="26.70365625" y2="51.087453125" width="0.254" layer="20"/>
<wire x1="26.70365625" y1="51.087453125" x2="26.70365625" y2="51.900253125" width="0.254" layer="20"/>
<wire x1="26.70365625" y1="51.900253125" x2="28.53245625" y2="57.793053125" width="0.254" layer="20"/>
<wire x1="28.53245625" y1="57.793053125" x2="28.93885625" y2="57.996253125" width="0.254" layer="20"/>
<wire x1="28.93885625" y1="57.996253125" x2="32.79965625" y2="54.948253125" width="0.254" layer="20"/>
<wire x1="32.79965625" y1="54.948253125" x2="33.20605625" y2="54.338653125" width="0.254" layer="20"/>
<wire x1="33.20605625" y1="54.338653125" x2="34.93325625" y2="50.173053125" width="0.254" layer="20"/>
<wire x1="34.93325625" y1="50.173053125" x2="35.13645625" y2="49.969853125" width="0.254" layer="20"/>
<wire x1="35.13645625" y1="49.969853125" x2="37.47325625" y2="51.087453125" width="0.254" layer="20"/>
<wire x1="37.47325625" y1="51.087453125" x2="37.67645625" y2="51.087453125" width="0.254" layer="20"/>
<wire x1="37.67645625" y1="51.087453125" x2="40.31805625" y2="48.445853125" width="0.254" layer="20"/>
<wire x1="40.31805625" y1="48.445853125" x2="40.72445625" y2="48.445853125" width="0.254" layer="20"/>
<wire x1="40.72445625" y1="48.445853125" x2="56.57405625" y2="73.033053125" width="0.254" layer="20"/>
<wire x1="56.57405625" y1="73.033053125" x2="56.77725625" y2="73.236253125" width="0.254" layer="20"/>
<wire x1="56.77725625" y1="73.236253125" x2="57.99645625" y2="73.439453125" width="0.254" layer="20"/>
<wire x1="57.99645625" y1="73.439453125" x2="58.19965625" y2="73.236253125" width="0.254" layer="20"/>
<wire x1="58.19965625" y1="73.236253125" x2="58.80925625" y2="71.813853125" width="0.254" layer="20"/>
<wire x1="58.80925625" y1="71.813853125" x2="58.80925625" y2="71.407453125" width="0.254" layer="20"/>
<wire x1="58.80925625" y1="71.407453125" x2="47.83645625" y2="47.633053125" width="0.254" layer="20"/>
<wire x1="47.83645625" y1="47.633053125" x2="48.03965625" y2="47.226653125" width="0.254" layer="20"/>
<wire x1="48.03965625" y1="47.226653125" x2="53.93245625" y2="49.868253125" width="0.254" layer="20"/>
<wire x1="53.93245625" y1="49.868253125" x2="55.05005625" y2="50.122253125" width="0.254" layer="20"/>
<wire x1="55.05005625" y1="50.122253125" x2="57.23445625" y2="49.919053125" width="0.254" layer="20"/>
<wire x1="57.23445625" y1="49.919053125" x2="57.18365625" y2="48.039453125" width="0.254" layer="20"/>
<wire x1="57.18365625" y1="48.039453125" x2="51.08765625" y2="39.505053125" width="0.254" layer="20"/>
<wire x1="51.08765625" y1="39.505053125" x2="51.08765625" y2="38.895453125" width="0.254" layer="20"/>
<wire x1="51.08765625" y1="38.895453125" x2="52.51005625" y2="32.799453125" width="0.254" layer="20"/>
<wire x1="52.51005625" y1="32.799453125" x2="55.15165625" y2="16.746653125" width="0.254" layer="20"/>
<wire x1="55.15165625" y1="16.746653125" x2="54.74525625" y2="9.634653125" width="0.254" layer="20"/>
<wire x1="54.74525625" y1="9.634653125" x2="54.54205625" y2="9.228253125" width="0.254" layer="20"/>
<wire x1="54.54205625" y1="9.228253125" x2="49.25885625" y2="6.789853125" width="0.254" layer="20"/>
<wire x1="49.25885625" y1="6.789853125" x2="48.24285625" y2="6.789853125" width="0.254" layer="20"/>
<wire x1="48.24285625" y1="6.789853125" x2="44.17885625" y2="9.228253125" width="0.254" layer="20"/>
<wire x1="44.17885625" y1="9.228253125" x2="43.56925625" y2="10.041053125" width="0.254" layer="20"/>
<wire x1="43.56925625" y1="10.041053125" x2="37.87965625" y2="20.201053125" width="0.254" layer="20"/>
<wire x1="37.87965625" y1="20.201053125" x2="37.47325625" y2="20.201053125" width="0.254" layer="20"/>
<wire x1="37.47325625" y1="20.201053125" x2="32.61345" y2="3.674290625" width="0.254" layer="20"/>
<wire x1="32.61345" y1="3.674290625" x2="30.716984375" y2="2.116559375" width="0.254" layer="20"/>
<wire x1="30.716984375" y1="2.116559375" x2="11.22688125" y2="4.554959375" width="0.254" layer="20"/>
<wire x1="11.22688125" y1="4.554959375" x2="9.7197125" y2="6.688509375" width="0.254" layer="20"/>
<wire x1="9.7197125" y1="6.688509375" x2="9.8719625" y2="11.175925" width="0.254" layer="20"/>
<wire x1="9.8719625" y1="11.175925" x2="9.143875" y2="14.122046875" width="0.254" layer="20"/>
<wire x1="9.143875" y1="14.122046875" x2="5.31685625" y2="10.041053125" width="0.254" layer="20"/>
<wire x1="5.31685625" y1="10.041053125" x2="3.74205625" y2="10.244253125" width="0.254" layer="20"/>
<wire x1="30.36125625" y1="48.445853125" x2="32.90125625" y2="49.258653125" width="0.4064" layer="20"/>
<wire x1="32.90125625" y1="49.258653125" x2="31.58045625" y2="53.170253125" width="0.4064" layer="20"/>
<wire x1="31.58045625" y1="53.170253125" x2="30.36125625" y2="54.135453125" width="0.4064" layer="20"/>
<wire x1="30.36125625" y1="54.135453125" x2="29.75165625" y2="53.932253125" width="0.4064" layer="20"/>
<wire x1="29.75165625" y1="53.932253125" x2="28.93885625" y2="51.290653125" width="0.4064" layer="20"/>
<wire x1="28.93885625" y1="51.290653125" x2="30.15805625" y2="48.445853125" width="0.4064" layer="20"/>
<text>UVicorn</text>
<text>Alien +   Spippy</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<wire x1="50.62560625" y1="46.64666875" x2="53.419325" y2="48.08585625" width="0.4064" layer="20"/>
<wire x1="53.419325" y1="48.08585625" x2="54.943171875" y2="48.170515625" width="0.4064" layer="20"/>
<wire x1="54.943171875" y1="48.170515625" x2="54.51988125" y2="47.239275" width="0.4064" layer="20"/>
<wire x1="54.51988125" y1="47.239275" x2="52.488084375" y2="45.0381625" width="0.4064" layer="20"/>
<wire x1="52.488084375" y1="45.0381625" x2="50.7102625" y2="46.562009375" width="0.4064" layer="20"/>
<text>v4.5 2018</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CR2032-EDIT">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPST-SMD-A">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="SparkFun-AnalogIC" package="SO08" value="">
<attribute name="DIGIKEY_PART_ID" value="ICM7555CBAZ-TCT-ND"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="DIGIKEY_PART_ID" value="P100BZCT-ND"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="1k">
<attribute name="DIGIKEY_PART_ID" value="P1KBZCT-ND"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="DIGIKEY_PART_ID" value="P100BZCT-ND"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="DIGIKEY_PART_ID" value="P100BZCT-ND"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="100">
<attribute name="VALUE"/>
<attribute name="DIGIKEY_PART_ID" value="P100BZCT-ND"/>
</element>
<element name="G1" library="adafruit" package="CR2032-EDIT" value="">
<attribute name="DIGIKEY_PART_ID" value="BK-913-ND"/>
</element>
<element name="G2" library="adafruit" package="CR2032-EDIT" value="">
<attribute name="DIGIKEY_PART_ID" value="BK-913-ND"/>
</element>
<element name="D1" library="led" package="LED5MM" value="UV-30mA"/>
<element name="D2" library="led" package="LED5MM" value="UV-30mA"/>
<element name="D3" library="led" package="LED5MM" value="UV-30mA"/>
<element name="D4" library="led" package="LED5MM" value="WHITE-30mA">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="1UF">
<attribute name="DIGIKEY_PART_ID" value="1276-1946-1-ND"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="1M">
<attribute name="DIGIKEY_PART_ID" value="P1MBZCT-ND"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="SWITCH-SPST-SMD-A" value="">
<attribute name="PROD_ID" value="SWCH-10651"/>
<attribute name="DIGIKEY_PART_ID" value="679-1847-1-ND"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="AXIAL-0.3EZ" value="SET">
<attribute name="DIGIKEY_PART_ID" value="P1MBZCT-ND"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="G1" pad="-"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="THRESHOLD">
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="4"/>
<contactref element="R5" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="D3" pad="A"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="OUT">
<contactref element="IC1" pad="3"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="G1" pad="+1"/>
<contactref element="G2" pad="-"/>
</signal>
<signal name="DISCHARGE">
<contactref element="IC1" pad="7"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$6">
<contactref element="G2" pad="+1"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="K"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R3" pad="1"/>
<contactref element="D3" pad="K"/>
</signal>
<signal name="N$2">
<contactref element="D4" pad="K"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="K"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
