<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="1.4" y1="0" x2="16.3" y2="0" width="0" layer="20"/>
<wire x1="16.3" y1="0" x2="16.3" y2="16.4" width="0" layer="20"/>
<wire x1="16.3" y1="16.4" x2="1.4" y2="16.4" width="0" layer="20"/>
<wire x1="1.4" y1="16.4" x2="1.4" y2="0" width="0" layer="20"/>
<text>VASST Lab
Copyright 2017</text>
<hole x="3.4" y="14.4" drill="3.2"/>
<hole x="14.3" y="14.4" drill="3.2"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch: 1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="70543-04">
<description>&lt;b&gt;C-Grid SL Connector&lt;/b&gt;&lt;p&gt;
 vertical, 4 pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="SENSOR" library="SparkFun-Connectors" package="1X04_1.27MM" value="LPPB041NGCN-RC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONTROLLER" library="con-molex" package="70543-04" value="70543-04">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="SENSOR" pad="1"/>
<contactref element="CONTROLLER" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="CONTROLLER" pad="2"/>
<contactref element="SENSOR" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="SENSOR" pad="3"/>
<contactref element="CONTROLLER" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="CONTROLLER" pad="4"/>
<contactref element="SENSOR" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
