<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.496" y2="0" width="0.1524" layer="20"/>
<wire x1="31.496" y1="0" x2="31.496" y2="21.209" width="0.1524" layer="20"/>
<wire x1="31.496" y1="21.209" x2="0" y2="21.209" width="0.1524" layer="20"/>
<wire x1="0" y1="21.209" x2="0" y2="0" width="0.1524" layer="20"/>
<text>VCC  MOSI GND</text>
<text>MISO CLK !RST</text>
<text>Accerometer/Magnetometer Sensor Board
v1 2-5-20</text>
<text>chip@seeinsights.com</text>
<text>INT2 INT1 EN AN VCC GND</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="FIDUCIAL-MICRO">
<description>&lt;h3&gt;Fiducial - Circle, 0.25in&lt;/h3&gt;
&lt;p&gt;Point-of-reference for pick-and-place machines and other optical instruments.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FIDUCIAL&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="MOSFETs">
<packages>
<package name="SO8-GW300">
<description>&lt;b&gt;Standard SO-8 Gull-Wing Package for IRF7101 MOSFET&lt;/b&gt;&lt;p&gt;

http://www.irf.com/product-info/datasheets/data/irf9310pbf.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Custom Components">
<packages>
<package name="TC2030-MCP-NL">
</package>
<package name="QFN16_3X3-L">
</package>
</packages>
</library>
<library name="MF_Discrete_Semiconductor">
<packages>
<package name="SOD-123">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Diodes in SOD-123 Standard.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="MF_Connectors">
<packages>
<package name="PTH_2.54MM_01X06">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for 2.54MM Pitch Header 6 Position. Based on 4UCON 00834.&lt;br&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER">
<attribute name="DESIGNER" value=""/>
<attribute name="REV" value=""/>
</element>
<element name="ATTINY85" library="SparkFun" package="SO08-EIAJ" value="ATTINY85">
<attribute name="MPN" value="ATTINY85-20SUR"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="PWR-SWITCH" library="MOSFETs" package="SO8-GW300" value="IRF9310PBF">
<attribute name="MPN" value="IRF9310PBF"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="MPN" value="MF-RES-0805-100K"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="FD1" library="SparkFun-Aesthetics" package="FIDUCIAL-MICRO" value="FIDUCIALUFIDUCIAL">
<attribute name="POPULATE" value="0"/>
</element>
<element name="FD2" library="SparkFun-Aesthetics" package="FIDUCIAL-MICRO" value="FIDUCIALUFIDUCIAL">
<attribute name="POPULATE" value="0"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="100k">
<attribute name="MPN" value="MF-RES-0805-100K"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="ICSP" library="Custom Components" package="TC2030-MCP-NL" value="TCP2030-MCP-NL">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="MPN" value="MF-RES-0805-1K"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="FD3" library="SparkFun-Aesthetics" package="FIDUCIAL-MICRO" value="FIDUCIALUFIDUCIAL">
<attribute name="POPULATE" value="0"/>
</element>
<element name="FD4" library="SparkFun-Aesthetics" package="FIDUCIAL-MICRO" value="FIDUCIALUFIDUCIAL">
<attribute name="POPULATE" value="0"/>
</element>
<element name="U1" library="Custom Components" package="QFN16_3X3-L" value="FXOS8700CQR1QFN16_3X3-L">
<attribute name="BUILT_BY" value="EMA_Jessica"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="FXOS8700CQR1"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="NXP"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="4.7k">
<attribute name="MPN" value="MF-RES-0805-4.7K"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="4.7k">
<attribute name="MPN" value="MF-RES-0805-4.7K"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-4.7uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="MPN" value="MF-CAP-0805-0.1uF"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="MPN" value="MF-RES-0805-1K"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="MPN" value="MF-RES-0805-1K"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-11622"/>
</element>
<element name="D4" library="MF_Discrete_Semiconductor" package="SOD-123" value="BAT42">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-BAT42"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-BAT42"/>
</element>
<element name="J2" library="MF_Connectors" package="PTH_2.54MM_01X06" value="MF-CON-2.54mm-01x06">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="LABEL01" value=""/>
<attribute name="LABEL02" value=""/>
<attribute name="LABEL03" value=""/>
<attribute name="LABEL04" value=""/>
<attribute name="LABEL05" value=""/>
<attribute name="LABEL06" value=""/>
<attribute name="MPN" value="MF-CON-2.54mm-01x06"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-2.54mm-01x06"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="ATTINY85" pad="4"/>
<contactref element="C1" pad="2"/>
<contactref element="ICSP" pad="6"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U1" pad="12"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="10"/>
<contactref element="C11" pad="2"/>
<contactref element="J2" pad="P$1"/>
<contactref element="U1" pad="16"/>
</signal>
<signal name="SDA">
<contactref element="ATTINY85" pad="5"/>
<contactref element="ICSP" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="GPIO3">
<contactref element="ATTINY85" pad="3"/>
</signal>
<signal name="!TINY-RST">
<contactref element="ATTINY85" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="ICSP" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="ATTINY85" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="PWR-SWITCH" pad="8"/>
<contactref element="PWR-SWITCH" pad="7"/>
<contactref element="PWR-SWITCH" pad="6"/>
<contactref element="PWR-SWITCH" pad="5"/>
<contactref element="C5" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U1" pad="14"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="D4" pad="ANODE"/>
</signal>
<signal name="!EN!">
<contactref element="PWR-SWITCH" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="NC1">
</signal>
<signal name="VSS(GND)">
</signal>
<signal name="MISO">
<contactref element="ATTINY85" pad="6"/>
<contactref element="ICSP" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="C6" pad="1"/>
<contactref element="PWR-SWITCH" pad="3"/>
<contactref element="PWR-SWITCH" pad="2"/>
<contactref element="PWR-SWITCH" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="P$2"/>
</signal>
<signal name="ANALOG">
<contactref element="ATTINY85" pad="2"/>
<contactref element="J2" pad="P$3"/>
</signal>
<signal name="ENABLE">
<contactref element="R5" pad="2"/>
<contactref element="J2" pad="P$4"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="2"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="4"/>
<contactref element="R8" pad="1"/>
<contactref element="ATTINY85" pad="7"/>
<contactref element="ICSP" pad="3"/>
</signal>
<signal name="INT1">
<contactref element="R6" pad="1"/>
<contactref element="J2" pad="P$5"/>
</signal>
<signal name="INT2">
<contactref element="R4" pad="1"/>
<contactref element="J2" pad="P$6"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="8"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="11"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="9"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="2"/>
<contactref element="ICSP" pad="2"/>
<contactref element="D4" pad="CATHODE"/>
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
