<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="10" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2" y1="0" x2="10.5" y2="0" width="0" layer="20"/>
<wire x1="18.5" y1="0" x2="27" y2="0" width="0" layer="20"/>
<wire x1="27" y1="0" x2="29" y2="2" width="0" layer="20" curve="90"/>
<wire x1="29" y1="2" x2="29" y2="10" width="0" layer="20"/>
<wire x1="29" y1="10" x2="0" y2="10" width="0" layer="20"/>
<hole x="27" y="2" drill="2"/>
<hole x="2" y="2" drill="2"/>
<text>3.3v</text>
<text>1/2 B</text>
<text>CHG</text>
<text>GND</text>
<text>+</text>
<text>-</text>
<wire x1="10.5" y1="0" x2="10.5" y2="3.95" width="0" layer="20"/>
<wire x1="10.5" y1="3.95" x2="11" y2="4.45" width="0" layer="20" curve="-90"/>
<wire x1="11" y1="4.45" x2="18" y2="4.45" width="0" layer="20"/>
<wire x1="18" y1="4.45" x2="18.5" y2="3.95" width="0" layer="20" curve="-90"/>
<wire x1="18.5" y1="3.95" x2="18.5" y2="0" width="0" layer="20"/>
<wire x1="10.5" y1="3.95" x2="10.5" y2="4" width="0" layer="20"/>
<text>OSHWatch Power Board v1.0</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Microchip_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 11:22:31</description>
<packages>
<package name="SOT95P280X110-5N">
</package>
</packages>
</library>
<library name="con-jst2">
<description>&lt;b&gt;J.S.T. Connectors&lt;/b&gt;&lt;p&gt;
J.S.T Mfg Co.,Ltd.&lt;p&gt;
http://www.jst-mfg.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SM02B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, side entry type&lt;/b&gt;</description>
</package>
<package name="SM04B-SRSS-TB">
<description>&lt;b&gt;Shrouded Header, side entry type&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Connectors">
<packages>
<package name="UB-MC5BR3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="0805" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value="4.7µH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-PowerIC" package="SOT23-5" value="MAX1555">
<attribute name="VALUE"/>
</element>
<element name="U2" library="Microchip_By_element14_Batch_1" package="SOT95P280X110-5N" value="MCP1603T-330I/OS">
<attribute name="OC_NEWARK" value="22K1332"/>
<attribute name="SUPPLIER" value="Microchip"/>
<attribute name="MPN" value="MCP1603T-330I/OS"/>
<attribute name="OC_FARNELL" value="1439373"/>
<attribute name="PACKAGE" value="SOT23-5"/>
</element>
<element name="X1" library="con-jst2" package="SM02B-SRSS-TB" value="Battery 150mAh">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-jst2" package="SM04B-SRSS-TB" value="Output">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value="4.7µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="Connectors" package="UB-MC5BR3" value="USB-MICRO-B"/>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="X2" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="S$3"/>
<contactref element="J1" pad="S$6"/>
<contactref element="J1" pad="S$1"/>
<contactref element="J1" pad="S$4"/>
<contactref element="J1" pad="S$5"/>
<contactref element="J1" pad="S$2"/>
</signal>
<signal name="V_BATT">
<contactref element="X1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="V_USB">
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="L1" pad="1"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="L1" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="X2" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="IND">
<contactref element="X2" pad="3"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="CHG">
<contactref element="U1" pad="3"/>
<contactref element="X2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
