<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.2">
<drawing>
<board>
<plain>
<wire x1="1.143" y1="0.762" x2="46.025" y2="0.762" width="0" layer="20"/>
<wire x1="46.025" y1="0.762" x2="46.101" y2="0.762" width="0" layer="20"/>
<wire x1="46.101" y1="0.762" x2="46.025" y2="0.762" width="0" layer="20"/>
<text>GND</text>
<text>5V</text>
<text>+12</text>
<text>-GND</text>
<text>EV-H</text>
<text>EV-L</text>
<text>LeafCAN</text>
<wire x1="1.143" y1="32.131" x2="46.101" y2="32.131" width="0" layer="20"/>
<wire x1="46.101" y1="32.131" x2="46.101" y2="0.762" width="0" layer="20"/>
<wire x1="46.101" y1="0.762" x2="46.025" y2="0.762" width="0" layer="20"/>
<wire x1="46.025" y1="0.762" x2="46.101" y2="0.762" width="0" layer="20"/>
<wire x1="46.101" y1="0.762" x2="46.025" y2="0.762" width="0" layer="20"/>
<wire x1="46.025" y1="0.762" x2="1.143" y2="0.762" width="0" layer="20"/>
<wire x1="1.143" y1="0.762" x2="1.143" y2="32.131" width="0" layer="20"/>
<text>V2+oled</text>
<text>-GND</text>
<text>+5</text>
<text>ENCS</text>
<text>ENCB</text>
<text>ENCA</text>
<text>PC5</text>
<text>PC4</text>
<text>PC3</text>
</plain>
<libraries>
<library name="_hhn_at90can32_64_128_v2">
<packages>
<package name="TQFP64-0.8MM">
<description>Thin Plasic Quad Flat Package&lt;b&gt; TQFP64, pad center spacing 0.8mm&lt;/b&gt;&lt;p&gt;
Updated from atml.lbr 17.01.2005 alf@cadsoft.de (tplace/tdocu modified)</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
<package name="TC26H">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
<package name="0805">
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="NX3225">
</package>
<package name="TC33X">
</package>
</packages>
</library>
<library name="ohw-logo">
<packages>
<package name="OSHW_10X200_NOTEXT">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="JST-4-PTH">
</package>
<package name="1X16">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="_hhn_at90can32_64_128_v2" package="TQFP64-0.8MM" value="AT90CAN128-16AI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun" package="SO08" value="MCP2551">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun" package="0805" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun" package="0805" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun" package="0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun" package="0805" value="22pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ICSP" library="SparkFun" package="2X03" value="ICSP">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun" package="0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun" package="0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun" package="0805" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y3" library="SparkFun" package="TC26H" value="32768Hz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="SparkFun" package="SOT223" value="MIC2920">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="adafruit" package="NX3225" value="16000"/>
<element name="LOGO2" library="ohw-logo" package="OSHW_10X200_NOTEXT" value="OSHW_LOGO_10MILX0200-NT"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="JST-4-PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X16" value="2x16 LED/OLED Display">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun" package="0805" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun" package="0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun" package="0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO3" library="ohw-logo" package="OSHW_10X200_NOTEXT" value="OSHW_LOGO_10MILX0200-NT"/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONT" library="adafruit" package="TC33X" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="SparkFun" package="SOT23-3" value="NUP2105">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="TYPE" value="Dual Line CAN Bus Protector"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="JST-4-PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="JST-4-PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="24"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="53"/>
<contactref element="U1" pad="63"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="ICSP" pad="6"/>
<contactref element="C3" pad="1"/>
<contactref element="Q1" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="Q1" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP3" pad="16"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="CONT" pad="1"/>
<contactref element="Q3" pad="3"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="N$1">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="Y3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="19"/>
<contactref element="Y3" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U2" pad="3"/>
<contactref element="C5" pad="2"/>
<contactref element="ICSP" pad="2"/>
<contactref element="U1" pad="64"/>
<contactref element="C8" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U1" pad="52"/>
<contactref element="C10" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP3" pad="15"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="CONT" pad="3"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="RXCAN">
<contactref element="U1" pad="31"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="TXCAN">
<contactref element="U1" pad="30"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="8"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="EV-CANH">
<contactref element="U2" pad="7"/>
<contactref element="JP2" pad="3"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="EV-CANL">
<contactref element="U2" pad="6"/>
<contactref element="JP2" pad="4"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="ICSP" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="ICSP" pad="3"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="RST">
<contactref element="ICSP" pad="5"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="MOSI">
<contactref element="ICSP" pad="4"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="LCD-RS">
<contactref element="U1" pad="7"/>
<contactref element="JP3" pad="13"/>
</signal>
<signal name="LCD-EN">
<contactref element="U1" pad="8"/>
<contactref element="JP3" pad="11"/>
</signal>
<signal name="LCD-D4">
<contactref element="U1" pad="13"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="LCD-D5">
<contactref element="U1" pad="14"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="LCD-D6">
<contactref element="U1" pad="15"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="LCD-D7">
<contactref element="U1" pad="16"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="TXD1">
<contactref element="U1" pad="28"/>
</signal>
<signal name="RXD1">
<contactref element="U1" pad="27"/>
</signal>
<signal name="+12V">
<contactref element="C9" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="JP2" pad="2"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="23"/>
<contactref element="C3" pad="2"/>
<contactref element="Q1" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="26"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="25"/>
</signal>
<signal name="LITE">
<contactref element="U1" pad="17"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="LCD-RW">
<contactref element="U1" pad="9"/>
<contactref element="JP3" pad="12"/>
</signal>
<signal name="PC5">
<contactref element="U1" pad="40"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="ENCA">
<contactref element="U1" pad="35"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="ENCB">
<contactref element="U1" pad="36"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="ENCS">
<contactref element="U1" pad="37"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="SPKR">
<contactref element="U1" pad="5"/>
</signal>
<signal name="PC3">
<contactref element="U1" pad="38"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="PC4">
<contactref element="U1" pad="39"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="JP3" pad="1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="R4" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="JP3" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="LCD-C">
<contactref element="CONT" pad="2"/>
<contactref element="JP3" pad="14"/>
</signal>
<signal name="N$4">
<contactref element="JP5" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="JP5" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="JP5" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
