<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.3.2">
<drawing>
<board>
<plain>
<wire x1="2.8575" y1="21.59" x2="31.75" y2="21.59" width="0.2032" layer="20"/>
<wire x1="31.75" y1="21.59" x2="31.75" y2="1.27" width="0.2032" layer="20"/>
<wire x1="31.75" y1="1.27" x2="2.8575" y2="1.27" width="0.2032" layer="20"/>
<wire x1="2.8575" y1="1.27" x2="2.8575" y2="21.59" width="0.2032" layer="20"/>
</plain>
<libraries>
<library name="SparkFun">
<packages>
<package name="PTC-1206">
</package>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;h3&gt;USB Type 'A' Male Connector - PTH&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/10016.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="VALUE" value="10uF"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-00810"/>
<attribute name="VALUE" value="0.1uF"/>
</element>
<element name="U1" library="SparkFun" package="SSOP28DB" value="FT232R"/>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE" value="330"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="330">
<attribute name="PROD_ID" value="RES-00818"/>
<attribute name="VALUE" value="330"/>
</element>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="Red">
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="VALUE" value="RED"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value="Green">
<attribute name="PROD_ID" value="DIO-00821"/>
<attribute name="VALUE" value="GREEN"/>
</element>
<element name="F1" library="SparkFun" package="PTC-1206" value="500mA"/>
<element name="J1" library="SparkFun-Connectors" package="USB-A-H" value="USB_A_PTH_MALE">
<attribute name="PROD_ID" value="CONN-08367"/>
<attribute name="SF_ID" value="PRT-00437"/>
</element>
<element name="JP4" library="pinhead" package="1X07" value=""/>
<element name="U$1" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$2" library="adafruit" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="C5" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="25"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="21"/>
<contactref element="J1" pad="GND"/>
<contactref element="JP4" pad="7"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="USB_D-">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="D-"/>
</signal>
<signal name="USB_D+">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="D+"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="20"/>
<contactref element="C5" pad="A"/>
<contactref element="C2" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="JP4" pad="6"/>
</signal>
<signal name="RTS">
<contactref element="U1" pad="3"/>
</signal>
<signal name="CTS">
<contactref element="U1" pad="11"/>
</signal>
<signal name="DTR">
<contactref element="U1" pad="2"/>
</signal>
<signal name="DSR">
<contactref element="U1" pad="9"/>
</signal>
<signal name="DCD">
<contactref element="U1" pad="10"/>
</signal>
<signal name="RI">
<contactref element="U1" pad="6"/>
</signal>
<signal name="3.3V">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="TXLED">
<contactref element="U1" pad="23"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="RXLED">
<contactref element="U1" pad="22"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="PWREN">
<contactref element="U1" pad="14"/>
</signal>
<signal name="TXDEN">
<contactref element="U1" pad="13"/>
</signal>
<signal name="SLEEP">
<contactref element="U1" pad="12"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="F1" pad="1"/>
<contactref element="J1" pad="VBUS"/>
</signal>
<signal name="RADIO_TX">
<contactref element="JP4" pad="4"/>
<contactref element="U1" pad="5"/>
</signal>
<signal name="RADIO_RX">
<contactref element="JP4" pad="5"/>
<contactref element="U1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
