<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="38.1" y2="0" width="0" layer="20"/>
<wire x1="38.1" y1="0" x2="38.1" y2="41.275" width="0" layer="20"/>
<wire x1="38.1" y1="41.275" x2="0" y2="41.265" width="0" layer="20"/>
<wire x1="0" y1="41.265" x2="0" y2="0" width="0" layer="20"/>
<text>www.github.com/uChip/BubbleDisplay</text>
<text>SCL</text>
<text>SDA</text>
<text>GND</text>
<text>5V</text>
<text>C.Schnarel
07APR2014</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="ChipsParts">
<packages>
<package name="0805-POL">
</package>
<package name="BBD-VIA">
</package>
<package name="0805-LED">
<description>Variant of package 0805 from SparkFun-Resistor.lbr.  Changed silk to show orientation. Changed pin names to A (annode) and C (cathode).</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="2X3">
</package>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RESONATOR-SMD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04">
</package>
</packages>
</library>
<library name="SparkFun-Displays">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of display devices- LED displays, LCD displays, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIL12">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF-TIGHT">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="DISPLAY1" library="SparkFun-Displays" package="DIL12" value="hp"/>
<element name="DISPLAY2" library="SparkFun-Displays" package="DIL12" value="hp"/>
<element name="R3" library="SparkFun-Resistors" package="0805" value="75"/>
<element name="R4" library="SparkFun-Resistors" package="0805" value="75"/>
<element name="R5" library="SparkFun-Resistors" package="0805" value="75"/>
<element name="R6" library="SparkFun-Resistors" package="0805" value="75"/>
<element name="R7" library="SparkFun-Resistors" package="0805" value="75"/>
<element name="R8" library="SparkFun-Resistors" package="0805" value="75"/>
<element name="R9" library="SparkFun-Resistors" package="0805" value="75"/>
<element name="R10" library="SparkFun-Resistors" package="0805" value="75"/>
<element name="C2" library="ChipsParts" package="0805-POL" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun" package="2X3" value="ICSP">
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun" package="TQFP32-08" value="ATMEGA328"/>
<element name="Y1" library="SparkFun-FreqCtrl" package="RESONATOR-SMD" value="16MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="I2C">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="IRFML8244">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23" value="IRFML8244">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23" value="IRFML8244">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="SOT23" value="IRFML8244">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q8" library="SparkFun-DiscreteSemi" package="SOT23" value="IRFML8244">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q7" library="SparkFun-DiscreteSemi" package="SOT23" value="IRFML8244">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q6" library="SparkFun-DiscreteSemi" package="SOT23" value="IRFML8244">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="Q5" library="SparkFun-DiscreteSemi" package="SOT23" value="IRFML8244">
<attribute name="PROD_ID" value="TRANS-08345"/>
</element>
<element name="JP2" library="ChipsParts" package="BBD-VIA" value="BREADBD_VIA"/>
<element name="U$5" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
<element name="U$6" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
<element name="U$7" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
<element name="U$8" library="SparkFun-Electromechanical" package="STAND-OFF-TIGHT" value=""/>
<element name="R2" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="ChipsParts" package="0805-LED" value="Amber">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="SEGB">
<contactref element="DISPLAY2" pad="11"/>
<contactref element="DISPLAY1" pad="11"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="SEGD">
<contactref element="DISPLAY2" pad="8"/>
<contactref element="DISPLAY1" pad="8"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="SEGE">
<contactref element="DISPLAY2" pad="2"/>
<contactref element="DISPLAY1" pad="2"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="SEGF">
<contactref element="DISPLAY2" pad="9"/>
<contactref element="DISPLAY1" pad="9"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="SEGG">
<contactref element="DISPLAY2" pad="7"/>
<contactref element="DISPLAY1" pad="7"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="SEGDP">
<contactref element="DISPLAY2" pad="5"/>
<contactref element="DISPLAY1" pad="5"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="CATH4">
<contactref element="DISPLAY1" pad="6"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="CATH8">
<contactref element="DISPLAY2" pad="6"/>
<contactref element="Q8" pad="3"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="C3" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="C4" pad="1"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q8" pad="2"/>
<contactref element="Q7" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="SEGA">
<contactref element="R3" pad="1"/>
<contactref element="DISPLAY2" pad="12"/>
<contactref element="DISPLAY1" pad="12"/>
</signal>
<signal name="SEGC">
<contactref element="R5" pad="1"/>
<contactref element="DISPLAY2" pad="3"/>
<contactref element="DISPLAY1" pad="3"/>
</signal>
<signal name="DIG1">
<contactref element="U1" pad="26"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="CATH3">
<contactref element="DISPLAY1" pad="4"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="CATH2">
<contactref element="DISPLAY1" pad="10"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="CATH1">
<contactref element="DISPLAY1" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="CATH5">
<contactref element="DISPLAY2" pad="1"/>
<contactref element="Q5" pad="3"/>
</signal>
<signal name="CATH6">
<contactref element="DISPLAY2" pad="10"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="CATH7">
<contactref element="DISPLAY2" pad="4"/>
<contactref element="Q7" pad="3"/>
</signal>
<signal name="A">
<contactref element="U1" pad="30"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="B">
<contactref element="U1" pad="31"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="C">
<contactref element="U1" pad="32"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="D">
<contactref element="U1" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="E">
<contactref element="U1" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="F">
<contactref element="U1" pad="9"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="G">
<contactref element="U1" pad="10"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="DP">
<contactref element="U1" pad="11"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="DIG4">
<contactref element="U1" pad="23"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="DIG3">
<contactref element="U1" pad="24"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="DIG2">
<contactref element="U1" pad="25"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="DIG7">
<contactref element="Q7" pad="1"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="16"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="17"/>
<contactref element="J1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="J1" pad="5"/>
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="AREF">
<contactref element="U1" pad="20"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="27"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="28"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="DIG5">
<contactref element="Q5" pad="1"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="DIG6">
<contactref element="Q6" pad="1"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="MOSI/DIG8">
<contactref element="U1" pad="15"/>
<contactref element="Q8" pad="1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="EE">
<contactref element="JP2" pad="P$1"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$1">
<contactref element="R2" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
