<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="74.91" y2="0" width="0" layer="20"/>
<wire x1="74.91" y1="0" x2="74.91" y2="58.09" width="0" layer="20"/>
<wire x1="74.91" y1="58.09" x2="0" y2="58.09" width="0" layer="20"/>
<wire x1="0" y1="58.09" x2="0" y2="0" width="0" layer="20"/>
<text>Bar</text>
<text>v1.1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_2MM">
<description>&lt;h3&gt;Plated Through Hole - 2mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_2.54_SCREWTERM">
<description>&lt;h3&gt;2 Pin Screw Terminal - 2.54mm&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="FaBo-Motor">
<packages>
<package name="SO8P">
</package>
</packages>
</library>
<library name="ESP32-DEVKIT">
<packages>
<package name="ESP32-DEVKITV1">
<description>The DOIT Esp32 DevKit v1 is one of the development board created by DOIT to evaluate the ESP-WROOM-32 module. It is based on the ESP32 microcontroller that boasts Wifi, Bluetooth, Ethernet and Low Power support all in a single chip.</description>
</package>
</packages>
</library>
<library name="Seeed-Resistor">
<packages>
<package name="R0805">
</package>
</packages>
</library>
<library name="Seeed-Capacitor">
<packages>
<package name="C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="C10" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="C11" library="Seeed-Capacitor" package="C0805" value="10uf">
<attribute name="MPN" value="CC0805ZKY5V6BB106"/>
</element>
<element name="C2" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X01_2MM" value=""/>
<element name="J2" library="SparkFun-Connectors" package="1X01_2MM" value=""/>
<element name="J3" library="SparkFun-Connectors" package="1X01_2MM" value=""/>
<element name="J4" library="SparkFun-Connectors" package="1X01_2MM" value=""/>
<element name="M1" library="FaBo-Motor" package="SO8P" value=""/>
<element name="M2" library="FaBo-Motor" package="SO8P" value=""/>
<element name="R1" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R2" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R3" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R4" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="ESP32" library="ESP32-DEVKIT" package="ESP32-DEVKITV1" value="ESP32DEVKITV1"/>
<element name="PUMP1" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="PUMP2" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="POWER" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="LED1" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="VL53L0X1" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="VL53L0X2" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="R5" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R6" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="C3" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="M3" library="FaBo-Motor" package="SO8P" value=""/>
<element name="R7" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R8" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="C4" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="M4" library="FaBo-Motor" package="SO8P" value=""/>
<element name="C5" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="C6" library="Seeed-Capacitor" package="C0805" value="10uf">
<attribute name="MPN" value="CC0805ZKY5V6BB106"/>
</element>
<element name="PUMP3" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="PUMP4" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="R9" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R10" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="C7" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="M5" library="FaBo-Motor" package="SO8P" value=""/>
<element name="R11" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R12" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="C8" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="M6" library="FaBo-Motor" package="SO8P" value=""/>
<element name="C9" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="C12" library="Seeed-Capacitor" package="C0805" value="10uf">
<attribute name="MPN" value="CC0805ZKY5V6BB106"/>
</element>
<element name="PUMP5" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="PUMP6" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="R13" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R14" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="C13" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="M7" library="FaBo-Motor" package="SO8P" value=""/>
<element name="R15" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R16" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="C14" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="M8" library="FaBo-Motor" package="SO8P" value=""/>
<element name="C15" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="C16" library="Seeed-Capacitor" package="C0805" value="10uf">
<attribute name="MPN" value="CC0805ZKY5V6BB106"/>
</element>
<element name="PUMP7" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="PUMP8" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
<element name="C17" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="M9" library="FaBo-Motor" package="SO8P" value=""/>
<element name="R17" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="R18" library="Seeed-Resistor" package="R0805" value="10K">
<attribute name="MPN" value="RC0805FR-0710KL"/>
</element>
<element name="C18" library="Seeed-Capacitor" package="C0805" value="100nf">
<attribute name="MPN" value="CC0805KRX7R9BB104"/>
</element>
<element name="C19" library="Seeed-Capacitor" package="C0805" value="10uf">
<attribute name="MPN" value="CC0805ZKY5V6BB106"/>
</element>
<element name="PUMP9" library="SparkFun-Connectors" package="1X02_2.54_SCREWTERM" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="C1" pad="2"/>
<contactref element="M1" pad="4"/>
<contactref element="PUMP1" pad="P1"/>
</signal>
<signal name="PIN32">
<contactref element="M1" pad="7"/>
<contactref element="ESP32" pad="21"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="PIN33">
<contactref element="M1" pad="6"/>
<contactref element="ESP32" pad="22"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="GND">
<contactref element="M1" pad="8"/>
<contactref element="M1" pad="5"/>
<contactref element="J3" pad="1"/>
<contactref element="LED1" pad="P1"/>
<contactref element="VL53L0X1" pad="P1"/>
<contactref element="POWER" pad="P1"/>
<contactref element="M2" pad="8"/>
<contactref element="M2" pad="5"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="M3" pad="8"/>
<contactref element="M3" pad="5"/>
<contactref element="M4" pad="8"/>
<contactref element="M4" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="M5" pad="8"/>
<contactref element="M5" pad="5"/>
<contactref element="M6" pad="8"/>
<contactref element="M6" pad="5"/>
<contactref element="C9" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="M7" pad="8"/>
<contactref element="M7" pad="5"/>
<contactref element="M8" pad="8"/>
<contactref element="M8" pad="5"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="M9" pad="8"/>
<contactref element="M9" pad="5"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="ESP32" pad="29"/>
<contactref element="ESP32" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="M1" pad="2"/>
<contactref element="M1" pad="3"/>
<contactref element="POWER" pad="P2"/>
<contactref element="M2" pad="3"/>
<contactref element="M2" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="M3" pad="2"/>
<contactref element="M3" pad="3"/>
<contactref element="M4" pad="3"/>
<contactref element="M4" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="M5" pad="2"/>
<contactref element="M5" pad="3"/>
<contactref element="M6" pad="3"/>
<contactref element="M6" pad="2"/>
<contactref element="C9" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="M7" pad="2"/>
<contactref element="M7" pad="3"/>
<contactref element="M8" pad="3"/>
<contactref element="M8" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="R15" pad="2"/>
<contactref element="M9" pad="2"/>
<contactref element="M9" pad="3"/>
<contactref element="C18" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="ESP32" pad="30"/>
</signal>
<signal name="N$6">
<contactref element="C2" pad="2"/>
<contactref element="M2" pad="4"/>
<contactref element="PUMP2" pad="P1"/>
</signal>
<signal name="PIN25">
<contactref element="M2" pad="7"/>
<contactref element="ESP32" pad="23"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="PIN26">
<contactref element="M2" pad="6"/>
<contactref element="ESP32" pad="24"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PIN27">
<contactref element="ESP32" pad="25"/>
<contactref element="M3" pad="7"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="PIN14">
<contactref element="ESP32" pad="26"/>
<contactref element="M3" pad="6"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="PIN13">
<contactref element="ESP32" pad="28"/>
<contactref element="M4" pad="7"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="PIN23">
<contactref element="ESP32" pad="15"/>
<contactref element="M4" pad="6"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="PIN1">
<contactref element="ESP32" pad="13"/>
<contactref element="M5" pad="7"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="PIN3">
<contactref element="ESP32" pad="12"/>
<contactref element="M5" pad="6"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="PIN19">
<contactref element="ESP32" pad="10"/>
<contactref element="M6" pad="7"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="PIN18">
<contactref element="ESP32" pad="9"/>
<contactref element="M6" pad="6"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="PIN5">
<contactref element="ESP32" pad="8"/>
<contactref element="M7" pad="7"/>
<contactref element="R16" pad="1"/>
</signal>
<signal name="PIN17">
<contactref element="ESP32" pad="7"/>
<contactref element="M7" pad="6"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="PIN16">
<contactref element="ESP32" pad="6"/>
<contactref element="M8" pad="7"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="PIN4">
<contactref element="ESP32" pad="5"/>
<contactref element="M8" pad="6"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="PIN2">
<contactref element="ESP32" pad="4"/>
<contactref element="M9" pad="7"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="PIN15">
<contactref element="ESP32" pad="3"/>
<contactref element="M9" pad="6"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="PIN12">
<contactref element="ESP32" pad="27"/>
<contactref element="LED1" pad="P2"/>
</signal>
<signal name="PIN21">
<contactref element="ESP32" pad="11"/>
<contactref element="VL53L0X2" pad="P2"/>
</signal>
<signal name="PIN22">
<contactref element="ESP32" pad="14"/>
<contactref element="VL53L0X2" pad="P1"/>
</signal>
<signal name="PIN3V3">
<contactref element="ESP32" pad="1"/>
<contactref element="VL53L0X1" pad="P2"/>
</signal>
<signal name="N$1">
<contactref element="M1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="PUMP1" pad="P2"/>
</signal>
<signal name="N$3">
<contactref element="C2" pad="1"/>
<contactref element="M2" pad="1"/>
<contactref element="PUMP2" pad="P2"/>
</signal>
<signal name="N$4">
<contactref element="C3" pad="2"/>
<contactref element="M3" pad="4"/>
<contactref element="PUMP3" pad="P1"/>
</signal>
<signal name="N$5">
<contactref element="C4" pad="2"/>
<contactref element="M4" pad="4"/>
<contactref element="PUMP4" pad="P1"/>
</signal>
<signal name="N$7">
<contactref element="M3" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="PUMP3" pad="P2"/>
</signal>
<signal name="N$8">
<contactref element="C4" pad="1"/>
<contactref element="M4" pad="1"/>
<contactref element="PUMP4" pad="P2"/>
</signal>
<signal name="N$9">
<contactref element="C7" pad="2"/>
<contactref element="M5" pad="4"/>
<contactref element="PUMP5" pad="P1"/>
</signal>
<signal name="N$10">
<contactref element="C8" pad="2"/>
<contactref element="M6" pad="4"/>
<contactref element="PUMP6" pad="P1"/>
</signal>
<signal name="N$11">
<contactref element="M5" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="PUMP5" pad="P2"/>
</signal>
<signal name="N$12">
<contactref element="C8" pad="1"/>
<contactref element="M6" pad="1"/>
<contactref element="PUMP6" pad="P2"/>
</signal>
<signal name="N$13">
<contactref element="C13" pad="2"/>
<contactref element="M7" pad="4"/>
<contactref element="PUMP7" pad="P1"/>
</signal>
<signal name="N$14">
<contactref element="C14" pad="2"/>
<contactref element="M8" pad="4"/>
<contactref element="PUMP8" pad="P1"/>
</signal>
<signal name="N$15">
<contactref element="M7" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="PUMP7" pad="P2"/>
</signal>
<signal name="N$16">
<contactref element="C14" pad="1"/>
<contactref element="M8" pad="1"/>
<contactref element="PUMP8" pad="P2"/>
</signal>
<signal name="N$17">
<contactref element="C17" pad="2"/>
<contactref element="M9" pad="4"/>
<contactref element="PUMP9" pad="P1"/>
</signal>
<signal name="N$18">
<contactref element="M9" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="PUMP9" pad="P2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
