<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="63.5" x2="0" y2="2.54" width="0.1524" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0.1524" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="60.96" y2="0" width="0.1524" layer="20"/>
<wire x1="60.96" y1="0" x2="63.5" y2="2.54" width="0.1524" layer="20" curve="90"/>
<wire x1="63.5" y1="2.54" x2="63.5" y2="63.5" width="0.1524" layer="20"/>
<wire x1="63.5" y1="63.5" x2="60.96" y2="66.04" width="0.1524" layer="20" curve="90"/>
<wire x1="60.96" y1="66.04" x2="2.54" y2="66.04" width="0.1524" layer="20"/>
<wire x1="2.54" y1="66.04" x2="0" y2="63.5" width="0.1524" layer="20" curve="90"/>
<text>Retro-Pin</text>
</plain>
<libraries>
<library name="Teensy356">
<packages>
<package name="TEENSY_3.5/3.6_BASIC">
</package>
</packages>
</library>
<library name="ECA-Passives">
<description>&lt;h3&gt;Eric Conner Apps - Passives&lt;/h3&gt;
&lt;p&gt;This library contiains passive items such as ressistors, capacitors, diodes, LEDs, etc.&lt;/p&gt;</description>
<packages>
<package name="0805">
</package>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ECA-Connectors">
<description>&lt;h3&gt;Eric Conner Apps - Connectors&lt;/h3&gt;
&lt;p&gt;This library contains electrically-functional connectors.&lt;/p&gt;</description>
<packages>
<package name="2X10-SHROUDED">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="KK-156-3">
</package>
<package name="SJ-3523-SMT">
</package>
</packages>
</library>
<library name="ECA-DigitalIC">
<description>&lt;h3&gt;Eric Conner Apps - Digital IC&lt;/h3&gt;
&lt;p&gt;This library contains Digital Logic chips such as 7400 series logic, Microcontrollers, etc.&lt;/p&gt;</description>
<packages>
<package name="SOIC-24W">
</package>
</packages>
</library>
<library name="ECA-Aesthetics">
<description>&lt;h3&gt;Eric Conner Apps - Aesthetics&lt;/h3&gt;
&lt;p&gt;This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc.&lt;/p&gt;</description>
<packages>
<package name="MOUNT_HOLE-150MIL">
</package>
<package name="ECA_LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Teensy356" package="TEENSY_3.5/3.6_BASIC" value="TEENSY 3.6"/>
<element name="DRIVER" library="ECA-Connectors" package="2X10-SHROUDED" value="2X10-SHROUDED">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="DISPLAY" library="ECA-Connectors" package="2X10-SHROUDED" value="2X10-SHROUDED">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="POWER" library="ECA-Connectors" package="KK-156-3" value="1X3-MOLEX">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="R9" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R10" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R11" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R12" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R13" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R14" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C1" library="ECA-Passives" package="0805" value="1.0uF">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="C2" library="ECA-Passives" package="0805" value="1.0uF">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R1" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R2" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R3" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R4" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R5" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R6" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R7" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="R8" library="ECA-Passives" package="0805" value="4k7">
<attribute name="ATTRIBUTE" value="0805"/>
<attribute name="DIGIKEY" value=""/>
<attribute name="NAME"/>
</element>
<element name="AUX1" library="ECA-Passives" package="SJ" value="JUMPER-SJ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AUX2" library="ECA-Passives" package="SJ" value="JUMPER-SJ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="ECA-DigitalIC" package="SOIC-24W" value="74HC154">
<attribute name="DIGIKEY" value=""/>
</element>
<element name="HOLE3" library="ECA-Aesthetics" package="MOUNT_HOLE-150MIL" value=""/>
<element name="HOLE4" library="ECA-Aesthetics" package="MOUNT_HOLE-150MIL" value=""/>
<element name="HOLE2" library="ECA-Aesthetics" package="MOUNT_HOLE-150MIL" value=""/>
<element name="HOLE1" library="ECA-Aesthetics" package="MOUNT_HOLE-150MIL" value=""/>
<element name="AUDIO" library="ECA-Connectors" package="SJ-3523-SMT" value="SJ-3523-SMT"/>
<element name="U$16" library="ECA-Aesthetics" package="ECA_LOGO" value="">
<attribute name="PROJECT" value="Teensy 3.6 MPU"/>
<attribute name="VERSION" value="1.0.0"/>
<attribute name="YEAR" value="2017"/>
</element>
</elements>
<signals>
<signal name="D0">
<contactref element="U1" pad="2"/>
<contactref element="DRIVER" pad="3"/>
<contactref element="DISPLAY" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="3/CANTX"/>
<contactref element="DRIVER" pad="5"/>
<contactref element="DISPLAY" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="4/CANRX"/>
<contactref element="DRIVER" pad="7"/>
<contactref element="DISPLAY" pad="7"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="5"/>
<contactref element="DRIVER" pad="9"/>
<contactref element="DISPLAY" pad="9"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="6"/>
<contactref element="DRIVER" pad="11"/>
<contactref element="DISPLAY" pad="11"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="7"/>
<contactref element="DRIVER" pad="13"/>
<contactref element="DISPLAY" pad="13"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="8"/>
<contactref element="DRIVER" pad="15"/>
<contactref element="DISPLAY" pad="15"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="9/CS"/>
<contactref element="DRIVER" pad="17"/>
<contactref element="DISPLAY" pad="17"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="BLANKING">
<contactref element="U1" pad="10/CS"/>
<contactref element="DRIVER" pad="20"/>
<contactref element="R9" pad="1"/>
<contactref element="DISPLAY" pad="16"/>
</signal>
<signal name="CS_1">
<contactref element="U1" pad="24"/>
<contactref element="R10" pad="1"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="CS_2">
<contactref element="U1" pad="25"/>
<contactref element="R11" pad="1"/>
<contactref element="U3" pad="22"/>
</signal>
<signal name="CS_3">
<contactref element="U1" pad="26"/>
<contactref element="R12" pad="1"/>
<contactref element="U3" pad="21"/>
</signal>
<signal name="CS_4">
<contactref element="U1" pad="27"/>
<contactref element="R13" pad="1"/>
<contactref element="U3" pad="20"/>
</signal>
<signal name="CS_ENABLE">
<contactref element="U1" pad="28"/>
<contactref element="R14" pad="1"/>
<contactref element="U3" pad="18"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="AGND"/>
<contactref element="U1" pad="GND2"/>
<contactref element="U1" pad="GND"/>
<contactref element="DRIVER" pad="1"/>
<contactref element="DRIVER" pad="19"/>
<contactref element="DISPLAY" pad="1"/>
<contactref element="DISPLAY" pad="19"/>
<contactref element="DISPLAY" pad="2"/>
<contactref element="DISPLAY" pad="20"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="POWER" pad="2"/>
<contactref element="U3" pad="12"/>
<contactref element="U3" pad="19"/>
<contactref element="AUDIO" pad="1"/>
</signal>
<signal name="DISP_1">
<contactref element="DISPLAY" pad="6"/>
<contactref element="U3" pad="6"/>
</signal>
<signal name="DISP_2">
<contactref element="DISPLAY" pad="8"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="DISP_3">
<contactref element="DISPLAY" pad="10"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="DISP_4">
<contactref element="DISPLAY" pad="12"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="DISP_STB">
<contactref element="DISPLAY" pad="14"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="AUX_1">
<contactref element="AUX1" pad="2"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="AUX_2">
<contactref element="AUX2" pad="2"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="LMP_COL">
<contactref element="DRIVER" pad="6"/>
<contactref element="U3" pad="16"/>
</signal>
<signal name="SOL_4">
<contactref element="DRIVER" pad="16"/>
<contactref element="U3" pad="11"/>
</signal>
<signal name="SOL_3">
<contactref element="DRIVER" pad="14"/>
<contactref element="U3" pad="14"/>
</signal>
<signal name="SOL_2">
<contactref element="DRIVER" pad="12"/>
<contactref element="U3" pad="10"/>
</signal>
<signal name="SOL_1">
<contactref element="DRIVER" pad="10"/>
<contactref element="U3" pad="15"/>
</signal>
<signal name="LMP_ROW">
<contactref element="DRIVER" pad="8"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="SW_ROW">
<contactref element="DRIVER" pad="4"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="SW_COL">
<contactref element="DRIVER" pad="2"/>
<contactref element="U3" pad="17"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="3V3"/>
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U3" pad="24"/>
</signal>
<signal name="AUDIO_L">
<contactref element="U1" pad="A22/DAC1"/>
<contactref element="AUDIO" pad="2"/>
</signal>
<signal name="AUDIO_R">
<contactref element="U1" pad="21/DAC0"/>
<contactref element="AUDIO" pad="3"/>
</signal>
<signal name="AUX_1_EN">
<contactref element="AUX1" pad="1"/>
<contactref element="DISPLAY" pad="4"/>
</signal>
<signal name="AUX_2_EN">
<contactref element="DISPLAY" pad="18"/>
<contactref element="AUX2" pad="1"/>
</signal>
<signal name="SOL_SPECIAL">
<contactref element="U3" pad="13"/>
<contactref element="DRIVER" pad="18"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="VIN"/>
<contactref element="POWER" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
