<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.2">
<drawing>
<board>
<plain>
<circle x="4.65" y="0.65" radius="1.524" width="0" layer="20"/>
<circle x="20.75" y="0.65" radius="1.524" width="0" layer="20"/>
<circle x="3.65" y="102.95" radius="1.524" width="0" layer="20"/>
<circle x="22.75" y="102.95" radius="1.524" width="0" layer="20"/>
<text>OpenEMG
Intan Headstage Breakout
Radu Darie
11/2016</text>
<text>Intan Headstage
ICs facing here</text>
<wire x1="-12.7" y1="-2.7" x2="38.1" y2="-2.7" width="0" layer="20"/>
<wire x1="38.1" y1="-2.7" x2="38.1" y2="107.3" width="0" layer="20"/>
<wire x1="38.1" y1="107.3" x2="-12.7" y2="107.3" width="0" layer="20"/>
<wire x1="-12.7" y1="107.3" x2="-12.7" y2="-2.7" width="0" layer="20"/>
</plain>
<libraries>
<library name="RHD2000_eval_board">
<description>Intan Technologies RHD2000 Eval Board</description>
<packages>
<package name="OMNETICS_A79024">
</package>
</packages>
</library>
<library name="omneticsToPolarized">
<description>Generated from &lt;b&gt;omneticsToPolarized.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="MOLEX-1X3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IN05" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN02" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN12" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN13" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN00" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN01" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN14" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN15" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN04" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN09" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN11" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN06" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN07" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN08" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN10" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="IN03" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
<element name="S1" library="RHD2000_eval_board" package="OMNETICS_A79024" value="OMNETICS_A79024"/>
<element name="J1" library="omneticsToPolarized" package="MOLEX-1X3" value=""/>
</elements>
<signals>
<signal name="AGND">
<contactref element="S1" pad="B1"/>
<contactref element="S1" pad="T1"/>
<contactref element="S1" pad="T18"/>
<contactref element="S1" pad="B18"/>
<contactref element="IN03" pad="1"/>
<contactref element="IN02" pad="1"/>
<contactref element="IN00" pad="1"/>
<contactref element="IN01" pad="1"/>
<contactref element="IN12" pad="1"/>
<contactref element="IN13" pad="1"/>
<contactref element="IN14" pad="1"/>
<contactref element="IN15" pad="1"/>
<contactref element="IN04" pad="1"/>
<contactref element="IN05" pad="1"/>
<contactref element="IN06" pad="1"/>
<contactref element="IN07" pad="1"/>
<contactref element="IN11" pad="1"/>
<contactref element="IN10" pad="1"/>
<contactref element="IN09" pad="1"/>
<contactref element="IN08" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="IN3-">
<contactref element="IN03" pad="3"/>
<contactref element="S1" pad="T2"/>
</signal>
<signal name="IN3+">
<contactref element="IN03" pad="2"/>
<contactref element="S1" pad="T3"/>
</signal>
<signal name="IN2-">
<contactref element="IN02" pad="3"/>
<contactref element="S1" pad="T4"/>
</signal>
<signal name="IN2+">
<contactref element="IN02" pad="2"/>
<contactref element="S1" pad="T5"/>
</signal>
<signal name="IN1-">
<contactref element="IN01" pad="3"/>
<contactref element="S1" pad="T6"/>
</signal>
<signal name="IN1+">
<contactref element="IN01" pad="2"/>
<contactref element="S1" pad="T7"/>
</signal>
<signal name="IN0-">
<contactref element="IN00" pad="3"/>
<contactref element="S1" pad="T8"/>
</signal>
<signal name="IN0+">
<contactref element="IN00" pad="2"/>
<contactref element="S1" pad="T9"/>
</signal>
<signal name="IN11-">
<contactref element="S1" pad="B17"/>
<contactref element="IN11" pad="3"/>
</signal>
<signal name="IN11+">
<contactref element="S1" pad="B16"/>
<contactref element="IN11" pad="2"/>
</signal>
<signal name="IN5+">
<contactref element="IN05" pad="2"/>
<contactref element="S1" pad="B4"/>
</signal>
<signal name="IN5-">
<contactref element="IN05" pad="3"/>
<contactref element="S1" pad="B5"/>
</signal>
<signal name="IN6+">
<contactref element="IN06" pad="2"/>
<contactref element="S1" pad="B6"/>
</signal>
<signal name="IN6-">
<contactref element="IN06" pad="3"/>
<contactref element="S1" pad="B7"/>
</signal>
<signal name="IN7+">
<contactref element="IN07" pad="2"/>
<contactref element="S1" pad="B8"/>
</signal>
<signal name="IN7-">
<contactref element="IN07" pad="3"/>
<contactref element="S1" pad="B9"/>
</signal>
<signal name="IN15-">
<contactref element="IN15" pad="3"/>
<contactref element="S1" pad="T10"/>
</signal>
<signal name="IN15+">
<contactref element="IN15" pad="2"/>
<contactref element="S1" pad="T11"/>
</signal>
<signal name="IN4-">
<contactref element="IN04" pad="3"/>
<contactref element="S1" pad="B3"/>
</signal>
<signal name="IN4+">
<contactref element="IN04" pad="2"/>
<contactref element="S1" pad="B2"/>
</signal>
<signal name="IN13-">
<contactref element="IN13" pad="3"/>
<contactref element="S1" pad="T14"/>
</signal>
<signal name="IN13+">
<contactref element="IN13" pad="2"/>
<contactref element="S1" pad="T15"/>
</signal>
<signal name="IN12-">
<contactref element="IN12" pad="3"/>
<contactref element="S1" pad="T16"/>
</signal>
<signal name="IN12+">
<contactref element="IN12" pad="2"/>
<contactref element="S1" pad="T17"/>
</signal>
<signal name="IN8+">
<contactref element="S1" pad="B10"/>
<contactref element="IN08" pad="2"/>
</signal>
<signal name="IN8-">
<contactref element="S1" pad="B11"/>
<contactref element="IN08" pad="3"/>
</signal>
<signal name="IN9+">
<contactref element="S1" pad="B12"/>
<contactref element="IN09" pad="2"/>
</signal>
<signal name="IN9-">
<contactref element="S1" pad="B13"/>
<contactref element="IN09" pad="3"/>
</signal>
<signal name="IN10+">
<contactref element="S1" pad="B14"/>
<contactref element="IN10" pad="2"/>
</signal>
<signal name="IN10-">
<contactref element="S1" pad="B15"/>
<contactref element="IN10" pad="3"/>
</signal>
<signal name="IN14+">
<contactref element="IN14" pad="2"/>
<contactref element="S1" pad="T13"/>
</signal>
<signal name="IN14-">
<contactref element="IN14" pad="3"/>
<contactref element="S1" pad="T12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
