<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="19.05" y2="0" width="0" layer="20"/>
<wire x1="19.05" y1="0" x2="19.05" y2="25.4" width="0" layer="20"/>
<wire x1="19.05" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<text>Vb</text>
<text>GND</text>
<text>Vr</text>
<text>DIR</text>
<text>PWM</text>
</plain>
<libraries>
<library name="PES_Passives">
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="PES_Connectors">
<packages>
<package name="1X05">
</package>
<package name="PAD-1.5X4.5">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
<package name="SOT23-3">
</package>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="PES_Passives" package="0805" value="100"/>
<element name="R2" library="PES_Passives" package="0805" value="100"/>
<element name="R3" library="PES_Passives" package="0805" value="1K"/>
<element name="R4" library="PES_Passives" package="0805" value="1K"/>
<element name="R5" library="PES_Passives" package="0805" value="10K"/>
<element name="R6" library="PES_Passives" package="0805" value="1K"/>
<element name="R7" library="PES_Passives" package="0805" value="10K"/>
<element name="R8" library="PES_Passives" package="0805" value="1K"/>
<element name="R9" library="PES_Passives" package="0805" value="1K"/>
<element name="JP1" library="PES_Connectors" package="1X05" value=""/>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23" value="2N4401"/>
<element name="Q4" library="SparkFun-DiscreteSemi" package="SOT23" value="2N4401"/>
<element name="Q5" library="SparkFun-DiscreteSemi" package="SOT23" value="2N4401"/>
<element name="Q6" library="SparkFun-DiscreteSemi" package="SOT23" value="2N4401"/>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2N4403"/>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2N4403"/>
<element name="Q7" library="SparkFun-DiscreteSemi" package="SOT23-3" value="2N4403"/>
<element name="Q8" library="SparkFun-DiscreteSemi" package="SOT223" value="FZT849"/>
<element name="Q9" library="SparkFun-DiscreteSemi" package="SOT223" value="FZT849"/>
<element name="Q10" library="SparkFun-DiscreteSemi" package="SOT223" value="FZT949"/>
<element name="Q11" library="SparkFun-DiscreteSemi" package="SOT223" value="FZT949"/>
<element name="M+" library="PES_Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
<element name="M-" library="PES_Connectors" package="PAD-1.5X4.5" value="M01SMD-4.5X1.5"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="Q11" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="1"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="Q11" pad="2"/>
<contactref element="Q8" pad="2"/>
<contactref element="M-" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="Q10" pad="2"/>
<contactref element="Q9" pad="2"/>
<contactref element="M+" pad="P$1"/>
</signal>
<signal name="N$6">
<contactref element="Q10" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R2" pad="2"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="R3" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R5" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="2"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R5" pad="2"/>
<contactref element="Q5" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="Q6" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="V_BATT">
<contactref element="Q10" pad="3"/>
<contactref element="Q11" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="Q6" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="Q8" pad="3"/>
<contactref element="Q9" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="Q2" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="2"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="R7" pad="2"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R7" pad="1"/>
<contactref element="Q7" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="Q7" pad="1"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="Q5" pad="1"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="Q7" pad="3"/>
<contactref element="Q5" pad="3"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="R8" pad="2"/>
<contactref element="R9" pad="2"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$9">
<contactref element="Q8" pad="1"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="Q9" pad="1"/>
<contactref element="Q4" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="Q1" pad="1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$22">
</signal>
</signals>
</board>
</drawing>
</eagle>
