<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="5.08" y2="0" width="0.0762" layer="20"/>
<wire x1="8.89" y1="0" x2="21.336" y2="0" width="0.0762" layer="20"/>
<wire x1="25.146" y1="0" x2="30.277" y2="0" width="0.0762" layer="20"/>
<wire x1="30.277" y1="0" x2="30.277" y2="43.297" width="0.0762" layer="20"/>
<wire x1="30.277" y1="43.297" x2="17.018" y2="43.307" width="0.0762" layer="20"/>
<wire x1="13.218" y1="43.297" x2="0" y2="43.297" width="0.0762" layer="20"/>
<wire x1="0" y1="43.297" x2="0" y2="0" width="0.0762" layer="20"/>
<text>SDA</text>
<text>SCL</text>
<text>GND</text>
<text>T1 IN</text>
<text>T2 IN</text>
<text>PUMP</text>
<text>VBatt</text>
<text>GND</text>
<text>F1 OUT</text>
<text>F2 OUT</text>
<text>IO1</text>
<text>IO2</text>
<text>IO2</text>
<text>F2 OUT</text>
<text>IO1</text>
<text>F1 OUT</text>
<text>GND</text>
<text>VBatt</text>
<text>PUMP</text>
<wire x1="17.018" y1="43.307" x2="13.208" y2="43.307" width="0.0762" layer="20" curve="-180"/>
<wire x1="5.08" y1="0" x2="8.89" y2="0" width="0.0762" layer="20" curve="-180"/>
<wire x1="21.336" y1="0" x2="25.146" y2="0" width="0.0762" layer="20" curve="-180"/>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1210">
<description>&lt;p&gt;&lt;b&gt;Generic 3225 (1210) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
<description>SOD-323 (Small Outline Diode)</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DPACK_3">
<description>&lt;b&gt;DPAK&lt;/b&gt;&lt;p&gt;Style 3 (Motorola)</description>
</package>
</packages>
</library>
<library name="Seeed-Transistor">
<packages>
<package name="SOT-23">
<description>&lt;b&gt;SOT23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Seeed-Resistor">
<packages>
<package name="R0805">
</package>
</packages>
</library>
<library name="Teensy_3_and_LC_Series_Boards_v1.1">
<packages>
<package name="TEENSY3-DIL">
</package>
</packages>
</library>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2101">
<description>.100" (2.54mm) Center Header - 10 Pin</description>
</package>
<package name="22-23-2041">
<description>.100" (2.54mm) Center Header - 4 Pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="1210" value="47uF"/>
<element name="C2" library="SparkFun-Capacitors" package="1210" value="47uF"/>
<element name="C3" library="SparkFun-Capacitors" package="1210" value="47uF"/>
<element name="C4" library="SparkFun-Capacitors" package="1210" value="47uF"/>
<element name="C5" library="SparkFun-Capacitors" package="1210" value="47uF"/>
<element name="C6" library="SparkFun-Capacitors" package="1210" value="47uF"/>
<element name="C7" library="SparkFun-Capacitors" package="1210" value="47uF"/>
<element name="C8" library="SparkFun-Capacitors" package="1210" value="47uF"/>
<element name="D1" library="SparkFun-DiscreteSemi" package="SOD-323" value="3V">
<attribute name="PROD_ID" value="DIO-08199"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="3V">
<attribute name="PROD_ID" value="DIO-08199"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="SOD-323" value="3V">
<attribute name="PROD_ID" value="DIO-08199"/>
</element>
<element name="D4" library="SparkFun-DiscreteSemi" package="SOD-323" value="3V">
<attribute name="PROD_ID" value="DIO-08199"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="SOD-323" value="3V">
<attribute name="PROD_ID" value="DIO-08199"/>
</element>
<element name="D6" library="SparkFun-DiscreteSemi" package="SOD-323" value="3V">
<attribute name="PROD_ID" value="DIO-08199"/>
</element>
<element name="IC1" library="linear" package="DPACK_3" value="MC7805ABT"/>
<element name="Q1" library="Seeed-Transistor" package="SOT-23" value="BT2222">
<attribute name="MPN" value="S9013"/>
</element>
<element name="Q2" library="Seeed-Transistor" package="SOT-23" value="BT2222">
<attribute name="MPN" value="S9013"/>
</element>
<element name="Q3" library="Seeed-Transistor" package="SOT-23" value="BT2222">
<attribute name="MPN" value="S9013"/>
</element>
<element name="R1" library="Seeed-Resistor" package="R0805" value="39.2">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R10" library="Seeed-Resistor" package="R0805" value="1k">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R2" library="Seeed-Resistor" package="R0805" value="39.2">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R3" library="Seeed-Resistor" package="R0805" value="1k">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R4" library="Seeed-Resistor" package="R0805" value="1k">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R5" library="Seeed-Resistor" package="R0805" value="1k">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R6" library="Seeed-Resistor" package="R0805" value="1k">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R7" library="Seeed-Resistor" package="R0805" value="70">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R8" library="Seeed-Resistor" package="R0805" value="70">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="R9" library="Seeed-Resistor" package="R0805" value="1k">
<attribute name="MPN" value="39.2 1%"/>
</element>
<element name="U$1" library="Teensy_3_and_LC_Series_Boards_v1.1" package="TEENSY3-DIL" value="TEENSY_3.1_DIL"/>
<element name="VEHICLE_SIGNAL" library="con-molex" package="22-23-2101" value="22-23-2101">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2101"/>
<attribute name="OC_FARNELL" value="1756828"/>
<attribute name="OC_NEWARK" value="94C0765"/>
</element>
<element name="X1" library="con-molex" package="22-23-2041" value="DATA_BUS">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2041"/>
<attribute name="OC_FARNELL" value="1462920"/>
<attribute name="OC_NEWARK" value="38C0355"/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="U$1" pad="AGND"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="3.3V"/>
</signal>
<signal name="N$2">
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="VEHICLE_SIGNAL" pad="8"/>
</signal>
<signal name="N$3">
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="VEHICLE_SIGNAL" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="Q2" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R10" pad="2"/>
<contactref element="VEHICLE_SIGNAL" pad="10"/>
</signal>
<signal name="N$9">
<contactref element="R9" pad="2"/>
<contactref element="VEHICLE_SIGNAL" pad="9"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="3"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="U$1" pad="VIN"/>
</signal>
<signal name="N$15">
<contactref element="D2" pad="C"/>
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="16/A2"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="1"/>
<contactref element="U$1" pad="20/A6"/>
</signal>
<signal name="N$6">
<contactref element="Q2" pad="1"/>
<contactref element="U$1" pad="21/A7"/>
</signal>
<signal name="N$16">
<contactref element="D1" pad="C"/>
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="17/A3"/>
</signal>
<signal name="N$12">
<contactref element="IC1" pad="1"/>
<contactref element="VEHICLE_SIGNAL" pad="5"/>
</signal>
<signal name="N$17">
<contactref element="D4" pad="C"/>
<contactref element="R6" pad="2"/>
<contactref element="U$1" pad="22/A8"/>
</signal>
<signal name="N$21">
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="IC1" pad="4"/>
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="Q3" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="A"/>
<contactref element="VEHICLE_SIGNAL" pad="6"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="D3" pad="C"/>
<contactref element="R5" pad="2"/>
<contactref element="U$1" pad="23/A9"/>
</signal>
<signal name="N$18">
<contactref element="R5" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="VEHICLE_SIGNAL" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="VEHICLE_SIGNAL" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="Q3" pad="1"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="N$20">
<contactref element="Q3" pad="3"/>
<contactref element="VEHICLE_SIGNAL" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="D5" pad="C"/>
<contactref element="R9" pad="1"/>
<contactref element="U$1" pad="15/A1"/>
</signal>
<signal name="N$23">
<contactref element="D6" pad="C"/>
<contactref element="R10" pad="1"/>
<contactref element="U$1" pad="14/A0"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="18/A4"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U$1" pad="19/A5"/>
<contactref element="X1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
