<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="15.5575" y1="1.42875" x2="15.5575" y2="18.89125" width="0" layer="20"/>
<wire x1="-0.3175" y1="18.89125" x2="-0.3175" y2="1.42875" width="0" layer="20"/>
<text>DM</text>
<text>DP</text>
<text>GND</text>
<text>DTRC</text>
<text>GND</text>
<text>G0</text>
<text>EN</text>
<text>TXD</text>
<text>RXD</text>
<text>5V</text>
<text>GND</text>
<text>G0</text>
<text>EN</text>
<text>TXD</text>
<text>RXD</text>
<text>5V</text>
<text>3V3</text>
<text>VUSB</text>
<text>DM</text>
<text>DP</text>
<text>GND</text>
<text>DTRC</text>
<text>VUSB</text>
<text>3V3</text>
<text>J1</text>
<text>C1</text>
<text>J2</text>
<text>U1</text>
<text>U2</text>
<text>U3</text>
<text>3904</text>
<text>FT231XS</text>
<text>AP2112</text>
<text>LED1</text>
<text>BLU</text>
<text>D1</text>
<text>C2</text>
<text>100n</text>
<text>100n</text>
<text>C3</text>
<text>100n</text>
<text>47p</text>
<text>33</text>
<text>47p</text>
<text>33</text>
<text>R1</text>
<text>R2</text>
<text>C4</text>
<text>C5</text>
<text>C6</text>
<text>C7</text>
<text>100n</text>
<text>100n</text>
<text>C9</text>
<text>C10</text>
<text>C8</text>
<text>22u</text>
<text>100n</text>
<text>100n</text>
<text>12K</text>
<text>R3</text>
<text>R5</text>
<text>R6</text>
<text>12K</text>
<text>12K</text>
<text>C11</text>
<text>100n</text>
<text>R4</text>
<text>2K2</text>
<text>R10</text>
<text>R7</text>
<text>R8</text>
<text>R9</text>
<text>0R</text>
<text>0R</text>
<text>1K</text>
<text>1K</text>
<text>AIoT USB FT SMD</text>
<text>3V3</text>
<text>5V</text>
<wire x1="-0.3175" y1="18.89125" x2="-0.15875" y2="19.05" width="0" layer="20" curve="-90"/>
<wire x1="-0.15875" y1="19.05" x2="15.39875" y2="19.05" width="0" layer="20"/>
<wire x1="15.39875" y1="19.05" x2="15.5575" y2="18.89125" width="0" layer="20" curve="-90"/>
<wire x1="-0.3175" y1="1.42875" x2="-0.15875" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="-0.15875" y1="1.27" x2="15.39875" y2="1.27" width="0" layer="20"/>
<wire x1="15.39875" y1="1.27" x2="15.5575" y2="1.42875" width="0" layer="20" curve="90"/>
</plain>
<libraries>
<library name="SparkFun-DigitalIC-2">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SSOP20_L">
<description>Longer version of SSOP-20 Package</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC-2">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT363">
</package>
</packages>
</library>
<library name="Resistor-2016">
<packages>
<package name="R0402">
</package>
</packages>
</library>
<library name="Capacitor-2016">
<packages>
<package name="C0402">
<description>&lt;b&gt;0402&lt;b&gt;&lt;p&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;0805&lt;b&gt;&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="Seeed-OPL-Diode">
<packages>
<package name="SOD-123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
<package name="LED-0402">
</package>
</packages>
</library>
<library name="lamloei_logo_3">
<packages>
<package name="LAMLOEI_MIDLOGO">
</package>
</packages>
</library>
<library name="SparkFun-Connectors5">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="SparkFun-DigitalIC-2" package="SSOP20_L" value="FT231XS">
<attribute name="PROD_ID" value="IC-11524"/>
</element>
<element name="U1" library="SparkFun-PowerIC-2" package="SOT23-5" value="3.3V">
<attribute name="PROD_ID" value="VREG-12457"/>
</element>
<element name="U3" library="SparkFun-DiscreteSemi" package="SOT363" value="MMDT3904">
<attribute name="PROD_ID" value="TRANS-09373"/>
</element>
<element name="R1" library="Resistor-2016" package="R0402" value="33R">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="R2" library="Resistor-2016" package="R0402" value="33R">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="C4" library="Capacitor-2016" package="C0402" value="47PF">
<attribute name="MPN" value="CC0402JRNPO9BN470"/>
</element>
<element name="C5" library="Capacitor-2016" package="C0402" value="47PF">
<attribute name="MPN" value="CC0402JRNPO9BN470"/>
</element>
<element name="C7" library="Capacitor-2016" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
</element>
<element name="C8" library="Capacitor-2016" package="C0805" value="22uf">
<attribute name="MPN" value="CC0805MKX5R5BB226"/>
</element>
<element name="C10" library="Capacitor-2016" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
</element>
<element name="C3" library="Capacitor-2016" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
</element>
<element name="C1" library="Capacitor-2016" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
</element>
<element name="C2" library="Capacitor-2016" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
</element>
<element name="R10" library="Resistor-2016" package="R0402" value="1K">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="R9" library="Resistor-2016" package="R0402" value="1K">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="R5" library="Resistor-2016" package="R0402" value="12K">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="R6" library="Resistor-2016" package="R0402" value="12K">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="R3" library="Resistor-2016" package="R0402" value="12K">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="C9" library="Capacitor-2016" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
</element>
<element name="R7" library="Resistor-2016" package="R0402" value="0R">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="R8" library="Resistor-2016" package="R0402" value="0R">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="D1" library="Seeed-OPL-Diode" package="SOD-123" value="40V-500MA">
<attribute name="MPN" value="B0540W"/>
<attribute name="NAME"/>
</element>
<element name="C11" library="Capacitor-2016" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
</element>
<element name="C6" library="Capacitor-2016" package="C0402" value="100nf">
<attribute name="MPN" value="CC0402KRX7R8BB104"/>
</element>
<element name="LED1" library="Seeed-OPL-Diode" package="LED-0402" value="BLUE-0402">
<attribute name="MPN" value="BL-HB337A-AV-TRB"/>
</element>
<element name="R4" library="Resistor-2016" package="R0402" value="2K2">
<attribute name="MPN" value="RC0402FR-0722RL"/>
</element>
<element name="ZL1" library="lamloei_logo_3" package="LAMLOEI_MIDLOGO" value="LAMLOEI_MIDLOGO"/>
<element name="J1" library="SparkFun-Connectors5" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors5" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3.3V">
<contactref element="U1" pad="5"/>
<contactref element="C8" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="13"/>
<contactref element="R7" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="V_USB">
<contactref element="U2" pad="15"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="D1" pad="+"/>
<contactref element="LED1" pad="+"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="DM">
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="DP">
<contactref element="R2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="GND">
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="16"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="DTRC">
<contactref element="C7" pad="2"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="DTR">
<contactref element="U2" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="RTS">
<contactref element="U2" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="11"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="12"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="TXD">
<contactref element="R10" pad="2"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="R9" pad="2"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="R10" pad="1"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="N$6">
<contactref element="R9" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="G0">
<contactref element="U3" pad="3"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="EN">
<contactref element="U3" pad="6"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="U3" pad="5"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="VCCIO">
<contactref element="U2" pad="3"/>
<contactref element="R3" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="U2" pad="14"/>
<contactref element="C9" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="5V">
<contactref element="D1" pad="-"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="R4" pad="2"/>
<contactref element="LED1" pad="-"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
