<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="89.9668" y2="0" width="0" layer="20"/>
<wire x1="89.9668" y1="0" x2="89.9668" y2="38.608" width="0" layer="20"/>
<wire x1="89.9668" y1="38.608" x2="0" y2="38.608" width="0" layer="20"/>
<wire x1="0" y1="38.608" x2="0" y2="0" width="0" layer="20"/>
<text>Rx  Tx</text>
<text>+</text>
<text>GND MISO VCC</text>
<text>+</text>
<text>chip@seeinsights.com</text>
<text>v1.1-  9-18-19</text>
<text>1 Hour Watchdog</text>
<text>LiPO Battery</text>
<text>5-6V @ 10W</text>
<text>A1 A0 Vcc GND</text>
<text>GND D3 D2 SCL SDA Vcc</text>
<text>User Btn</text>
<text>SCL SDA VCC GND</text>
<text>Power - Push On / Push Off</text>
<text>MOSI SCK SS
</text>
</plain>
<libraries>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="FIDUCIAL-MICRO">
<description>&lt;h3&gt;Fiducial - Circle, 0.25in&lt;/h3&gt;
&lt;p&gt;Point-of-reference for pick-and-place machines and other optical instruments.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FIDUCIAL&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="CREATIVE_COMMONS">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Fujitsu_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 15:17:27</description>
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805@1">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_LOCK">
<description>This footprint was designed to help hold the alignment of a through-hole component (i.e.  6-pin header) while soldering it into place.  
You may notice that each hole has been shifted either up or down by 0.005 of an inch from it's more standard position (which is a perfectly straight line).  
This slight alteration caused the pins (the squares in the middle) to touch the edges of the holes.  Because they are alternating, it causes a "brace" 
to hold the component in place.  0.005 has proven to be the perfect amount of "off-center" position when using our standard breakaway headers.
Although looks a little odd when you look at the bare footprint, once you have a header in there, the alteration is very hard to notice.  Also,
if you push a header all the way into place, it is covered up entirely on the bottom side.  This idea of altering the position of holes to aid alignment 
will be further integrated into the Sparkfun Library for other footprints.  It can help hold any component with 3 or more connection pins.</description>
</package>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="JST-2-SMD">
<description>&lt;h3&gt;JST-Right Angle Male Header SMT&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/20404.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;li&gt;JST_2MM_MALE&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="MC14093B-TSSOP14">
<description>&lt;b&gt;plastic thin shrink small outline package; 14 leads; body width 4.4 mm &lt;/b&gt;&lt;p&gt;
SOT402-1&lt;br&gt;
Source: http://www.onsemi.com/pub_link/Collateral/MC14093B-D.PDF</description>
</package>
<package name="B3F-40XX-ROUND">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Custom Components">
<packages>
<package name="SOT-23-5">
</package>
<package name="0805">
</package>
<package name="TSOT-23">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="TMP36">
<packages>
<package name="RJ_5">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="STAND-OFF">
<description>&lt;b&gt;Stand Off&lt;/b&gt;&lt;p&gt;
This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components. SKU : PRT-00447</description>
</package>
</packages>
</library>
<library name="SparkFun-Fuses">
<description>&lt;h3&gt;SparkFun Fuses&lt;/h3&gt;
In this library you'll find fuses, or fuse like components such as PTCs. Reference designator F.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
<description>&lt;p&gt;&lt;b&gt;Generic 3216 (1206) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="MF_Passives">
<packages>
<package name="CP10MM">
<description>&lt;b&gt;Description:&lt;/b&gt; 10MM Round Package for Electrolytic Capacitors. Based on Panasonic Electrolytic Capacitors.
&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="MF_Discrete_Semiconductor">
<packages>
<package name="SOD-123">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Diodes in SOD-123 Standard.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="Carrier Board">
<description>Generated from &lt;b&gt;Carrier Board.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="PARTICLE-DEVICES_BORON">
</package>
</packages>
</library>
<library name="MF_Switches">
<packages>
<package name="TACT6MM">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 6MM Tact Switch Package.&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_1-NC_TRACE_SILK">
</package>
<package name="SMT-JUMPER_2_NC_PASTE_SILK">
</package>
</packages>
</library>
<library name="OPL_Connector">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service
&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;
&lt;br&gt;&lt;/b&gt;</description>
<packages>
<package name="HW4-SMD-2.0">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U3" library="Fujitsu_By_element14_Batch_1" package="SOIC127P600X175-8N" value="MB85RC64">
<attribute name="MPN" value="MB85RC128PNF-G-JNE1"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1831995"/>
<attribute name="OC_NEWARK" value="93R5161"/>
<attribute name="PACKAGE" value="SO-8"/>
<attribute name="SUPPLIER" value="FUJITSU"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805@1" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X06_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="G1" library="Custom Components" package="SOT-23-5" value="D5V0L4B5TS">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="4.7k">
<attribute name="NAME"/>
</element>
<element name="U7" library="adafruit" package="MC14093B-TSSOP14" value="NAND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="adafruit" package="B3F-40XX-ROUND" value="B3F-4000">
<attribute name="NAME"/>
</element>
<element name="V1" library="Custom Components" package="0805" value="VC080505C150DP ">
<attribute name="NAME"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="D1" library="MF_Discrete_Semiconductor" package="SOD-123" value="MF-DIO-SOD123-BAT42">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-BAT42"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-BAT42"/>
</element>
<element name="R14" library="SparkFun-Passives" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="R12" library="SparkFun-Passives" package="0805" value="100">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805@1" value="1uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="270k">
<attribute name="NAME"/>
</element>
<element name="V3" library="Custom Components" package="0805" value="VC080505C150DP ">
<attribute name="NAME"/>
</element>
<element name="U1" library="TMP36" package="RJ_5" value="TMP36GRTZ">
<attribute name="MANUFACTURER_PART_NUMBER" value="TMP36GRTZREEL7"/>
<attribute name="NAME"/>
<attribute name="VENDOR" value="Analog Devices Inc"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805@1" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805@1" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="R13" library="SparkFun-Passives" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="R11" library="SparkFun-Passives" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="FD1" library="SparkFun-Aesthetics" package="FIDUCIAL-MICRO" value="FIDUCIALUFIDUCIAL"/>
<element name="FD2" library="SparkFun-Aesthetics" package="FIDUCIAL-MICRO" value="FIDUCIALUFIDUCIAL"/>
<element name="JP5" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP3" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP4" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="JP6" library="SparkFun" package="STAND-OFF" value="STAND-OFF"/>
<element name="J3" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="JST-2-SMD" value="S2B-PH-SM4-TB(LF)(SN)">
<attribute name="MFG" value="S2B-PH-SM4-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="JST-2-SMD" value="S2B-PH-SM4-TB(LF)(SN)">
<attribute name="MFG" value="S2B-PH-SM4-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11443"/>
<attribute name="SF_ID" value="PRT-08612"/>
</element>
<element name="F1" library="SparkFun-Fuses" package="1206" value="1.5A - SLOW BLOW">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08585"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="100k">
<attribute name="NAME"/>
</element>
<element name="F3" library="SparkFun-Fuses" package="1206" value="500mA - FAST BLOW">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08585"/>
</element>
<element name="U$2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
<element name="R2" library="SparkFun-Passives" package="0805" value="270k">
<attribute name="NAME"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="FRAME2" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="FRAME3" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="R5" library="SparkFun-Passives" package="0805" value="10k">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805@1" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="D2" library="MF_Discrete_Semiconductor" package="SOD-123" value="MF-DIO-SOD123-BAT42">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-BAT42"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-BAT42"/>
</element>
<element name="D3" library="MF_Discrete_Semiconductor" package="SOD-123" value="MF-DIO-SOD123-BAT42">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-BAT42"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-BAT42"/>
</element>
<element name="C8" library="MF_Passives" package="CP10MM" value="470uF">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="U2" library="Custom Components" package="TSOT-23" value="TPL5010">
<attribute name="NAME"/>
</element>
<element name="BORON/ARGON/XENON" library="Carrier Board" package="PARTICLE-DEVICES_BORON" value="PARTICLE-DEVICES-BORON">
<attribute name="NAME"/>
</element>
<element name="SW2" library="MF_Switches" package="TACT6MM" value="MF-SW-TACT-6MM">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-SW-TACT-6MM"/>
<attribute name="NAME"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-SW-TACT-6MM"/>
</element>
<element name="V2" library="Custom Components" package="0805" value="VC080505C150DP ">
<attribute name="NAME"/>
</element>
<element name="F2" library="SparkFun-Fuses" package="1206" value="500mA - FAST BLOW">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08585"/>
</element>
<element name="JP7" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="JUMPER-SMT_3_1-NC_TRACE_SILK">
<attribute name="NAME"/>
</element>
<element name="JP9" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NC_PASTE_SILK" value="JUMPER-SMT_2_NC_PASTE_SILK">
<attribute name="NAME"/>
</element>
<element name="J1" library="OPL_Connector" package="HW4-SMD-2.0" value="H4P-SMD-2.0">
<attribute name="NAME"/>
</element>
<element name="J2" library="OPL_Connector" package="HW4-SMD-2.0" value="H4P-SMD-2.0">
<attribute name="NAME"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="2X3" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09701"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U3" pad="4"/>
<contactref element="U3" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="G1" pad="2"/>
<contactref element="U7" pad="7"/>
<contactref element="JP1" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="J5" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="V1" pad="1"/>
<contactref element="V3" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C8" pad="P$2"/>
<contactref element="U2" pad="2"/>
<contactref element="BORON/ARGON/XENON" pad="GND"/>
<contactref element="SW2" pad="P$4"/>
<contactref element="SW2" pad="P$3"/>
<contactref element="V2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="J2" pad="SS2"/>
<contactref element="J2" pad="SS1"/>
<contactref element="J1" pad="SS1"/>
<contactref element="J1" pad="SS2"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U3" pad="6"/>
<contactref element="G1" pad="3"/>
<contactref element="R7" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="BORON/ARGON/XENON" pad="SCL"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U3" pad="5"/>
<contactref element="G1" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="JP1" pad="5"/>
<contactref element="BORON/ARGON/XENON" pad="SDA"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U3" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="F3" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="F2" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="JP9" pad="2"/>
<contactref element="BORON/ARGON/XENON" pad="3V3"/>
</signal>
<signal name="LI+">
<contactref element="BORON/ARGON/XENON" pad="LI+"/>
<contactref element="J5" pad="2"/>
<contactref element="D2" pad="ANODE"/>
</signal>
<signal name="D2">
<contactref element="G1" pad="5"/>
<contactref element="JP1" pad="3"/>
<contactref element="BORON/ARGON/XENON" pad="D2"/>
</signal>
<signal name="D3">
<contactref element="G1" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="BORON/ARGON/XENON" pad="D3"/>
</signal>
<signal name="TX">
<contactref element="J3" pad="2"/>
<contactref element="BORON/ARGON/XENON" pad="TX"/>
</signal>
<signal name="A2">
<contactref element="BORON/ARGON/XENON" pad="A2"/>
</signal>
<signal name="N$14">
<contactref element="U7" pad="10"/>
<contactref element="U7" pad="12"/>
<contactref element="U7" pad="13"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="BUTTON-STATE">
<contactref element="U7" pad="11"/>
<contactref element="R13" pad="1"/>
<contactref element="U7" pad="5"/>
</signal>
<signal name="N$24">
<contactref element="S2" pad="3"/>
<contactref element="S2" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="U7" pad="8"/>
<contactref element="U7" pad="9"/>
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="!RST">
<contactref element="BORON/ARGON/XENON" pad="RST"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="HARD-RESET">
<contactref element="R10" pad="2"/>
<contactref element="BORON/ARGON/XENON" pad="D6"/>
</signal>
<signal name="N$16">
<contactref element="R10" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="Q1" pad="3"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="DELAY">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="DONE">
<contactref element="U2" pad="4"/>
<contactref element="BORON/ARGON/XENON" pad="A3"/>
</signal>
<signal name="RX">
<contactref element="J3" pad="1"/>
<contactref element="BORON/ARGON/XENON" pad="RX"/>
</signal>
<signal name="TEMP">
<contactref element="U1" pad="1"/>
<contactref element="BORON/ARGON/XENON" pad="A4"/>
</signal>
<signal name="!HARD-RESET">
<contactref element="R12" pad="1"/>
<contactref element="R14" pad="1"/>
<contactref element="D1" pad="ANODE"/>
<contactref element="U7" pad="6"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U7" pad="4"/>
<contactref element="U7" pad="1"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="VCC-EXT">
<contactref element="V3" pad="2"/>
<contactref element="F3" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="J6" pad="5"/>
</signal>
<signal name="USER-SW">
<contactref element="R5" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="BORON/ARGON/XENON" pad="D4"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="SW2" pad="P$2"/>
<contactref element="SW2" pad="P$1"/>
</signal>
<signal name="DC-IN-EXT">
<contactref element="J4" pad="2"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="SS">
<contactref element="BORON/ARGON/XENON" pad="A5"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="ENABLE-PWR">
<contactref element="R14" pad="2"/>
<contactref element="D1" pad="CATHODE"/>
<contactref element="D3" pad="CATHODE"/>
<contactref element="D2" pad="CATHODE"/>
<contactref element="U7" pad="14"/>
</signal>
<signal name="MD">
<contactref element="BORON/ARGON/XENON" pad="MD"/>
</signal>
<signal name="A0">
<contactref element="BORON/ARGON/XENON" pad="A0"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="A1">
<contactref element="BORON/ARGON/XENON" pad="A1"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="BORON/ARGON/XENON" pad="SCK"/>
<contactref element="J6" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="BORON/ARGON/XENON" pad="MO"/>
<contactref element="J6" pad="6"/>
</signal>
<signal name="MISO">
<contactref element="BORON/ARGON/XENON" pad="MI"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="WAKE">
<contactref element="U2" pad="5"/>
<contactref element="BORON/ARGON/XENON" pad="D8"/>
</signal>
<signal name="EN">
<contactref element="BORON/ARGON/XENON" pad="EN"/>
<contactref element="U7" pad="3"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="VUSB">
<contactref element="BORON/ARGON/XENON" pad="VUSB"/>
<contactref element="F1" pad="2"/>
<contactref element="V1" pad="2"/>
<contactref element="D3" pad="ANODE"/>
<contactref element="C8" pad="P$1"/>
</signal>
<signal name="VCC2-EXT">
<contactref element="F2" pad="2"/>
<contactref element="V2" pad="2"/>
<contactref element="JP1" pad="6"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="RESET">
<contactref element="R3" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="U2" pad="1"/>
<contactref element="JP9" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
