<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="27.92" y2="0" width="0" layer="20"/>
<wire x1="27.92" y1="0" x2="27.92" y2="36.5" width="0" layer="20"/>
<wire x1="27.92" y1="36.5" x2="0" y2="36.5" width="0" layer="20"/>
<wire x1="0" y1="36.5" x2="0" y2="0" width="0" layer="20"/>
<text>SDI
SII
SDO
SCI
+5V
RST
GND</text>
<text>SDI
SII
SDO
SCI
+5V
RST
GND</text>
<text>GND
+12V</text>
<text>GND
+12V</text>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X07">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="SOD-523">
<description>SOD-523 (0.8x1.2mm)

&lt;p&gt;Source: http://www.rohm.com/products/databook/di/pdf/rb751s-40.pdf&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP08_MCU">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="SO08-EIAJ_MCU">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="transistor" package="SOT23-BEC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-Retired" package="DIP08_MCU" value="TINY85-20-DIP">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-Retired" package="SO08-EIAJ_MCU" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
</element>
<element name="D1" library="adafruit" package="SOD-523" value=""/>
</elements>
<signals>
<signal name="+5V">
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="8"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U2" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="T1" pad="E"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="+12V">
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="T1" pad="B"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="T1" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="5"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="6"/>
<contactref element="U2" pad="6"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="7"/>
<contactref element="U2" pad="7"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U1" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SCI">
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="SDO">
<contactref element="R6" pad="2"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="SII">
<contactref element="R2" pad="2"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SDI">
<contactref element="R4" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
